/*
 * Copyright (C) 2012 Texas Instruments Incorporated - http://www.ti.com/
 *
 * This program is free software; you can redistribute it and/or modify
 * it under the terms of the GNU General Public License version 2 as
 * published by the Free Software Foundation.
 */
/dts-v1/;

#include "omap4460.dtsi"
#include "omap4-panda-common.dtsi"

/* Audio routing is differnet between PandaBoard4430 and PandaBoardES */
&sound {
	ti,model = "PandaBoardES";

	/* Audio routing */
	ti,audio-routing =
		"Headset Stereophone", "HSOL",
		"Headset Stereophone", "HSOR",
		"Ext Spk", "HFL",
		"Ext Spk", "HFR",
		"Line Out", "AUXL",
		"Line Out", "AUXR",
		"AFML", "Line In",
		"AFMR", "Line In";
};

/* PandaboardES has external pullups on SCL & SDA */
&dss_hdmi_pins {
	pinctrl-single,pins = <
		0x5a (PIN_INPUT_PULLUP | MUX_MODE0)	/* hdmi_cec.hdmi_cec */
		0x5c (PIN_INPUT | MUX_MODE0)		/* hdmi_scl.hdmi_scl */
		0x5e (PIN_INPUT | MUX_MODE0)		/* hdmi_sda.hdmi_sda */
		>;
};

&omap4_pmx_core {
	led_gpio_pins: gpio_led_pmx {
		pinctrl-single,pins = <
			0xb6 (PIN_OUTPUT | MUX_MODE3)	/* gpio_110 */
		>;
	};
};

&led_wkgpio_pins {
	pinctrl-single,pins = <
		0x1c (PIN_OUTPUT | MUX_MODE3)	/* gpio_wk8 */
	>;
};

&leds {
	pinctrl-0 = <
		&led_gpio_pins
		&led_wkgpio_pins
	>;

	heartbeat {
		gpios = <&gpio4 14 GPIO_ACTIVE_HIGH>;
	};
	mmc {
		gpios = <&gpio1 8 GPIO_ACTIVE_HIGH>;
	};
};

&gpio1 {
	 ti,no-reset-on-init;
};
