/dts-v1/;

#include "skeleton.dtsi"

/ {
	model = "Qualcomm APQ 8084";
	compatible = "qcom,apq8084";
	interrupt-parent = <&intc>;

	cpus {
		#address-cells = <1>;
		#size-cells = <0>;

		cpu@0 {
			device_type = "cpu";
			compatible = "qcom,krait";
			reg = <0>;
			enable-method = "qcom,kpss-acc-v2";
			next-level-cache = <&L2>;
			qcom,acc = <&acc0>;
		};

		cpu@1 {
			device_type = "cpu";
			compatible = "qcom,krait";
			reg = <1>;
			enable-method = "qcom,kpss-acc-v2";
			next-level-cache = <&L2>;
			qcom,acc = <&acc1>;
		};

		cpu@2 {
			device_type = "cpu";
			compatible = "qcom,krait";
			reg = <2>;
			enable-method = "qcom,kpss-acc-v2";
			next-level-cache = <&L2>;
			qcom,acc = <&acc2>;
		};

		cpu@3 {
			device_type = "cpu";
			compatible = "qcom,krait";
			reg = <3>;
			enable-method = "qcom,kpss-acc-v2";
			next-level-cache = <&L2>;
			qcom,acc = <&acc3>;
		};

		L2: l2-cache {
			compatible = "qcom,arch-cache";
			cache-level = <2>;
			qcom,saw = <&saw_l2>;
		};
	};

	cpu-pmu {
		compatible = "qcom,krait-pmu";
		interrupts = <1 7 0xf04>;
	};

	timer {
		compatible = "arm,armv7-timer";
		interrupts = <1 2 0xf08>,
			     <1 3 0xf08>,
			     <1 4 0xf08>,
			     <1 1 0xf08>;
		clock-frequency = <19200000>;
	};

	soc: soc {
		#address-cells = <1>;
		#size-cells = <1>;
		ranges;
		compatible = "simple-bus";

		intc: interrupt-controller@f9000000 {
			compatible = "qcom,msm-qgic2";
			interrupt-controller;
			#interrupt-cells = <3>;
			reg = <0xf9000000 0x1000>,
			      <0xf9002000 0x1000>;
		};

		timer@f9020000 {
			#address-cells = <1>;
			#size-cells = <1>;
			ranges;
			compatible = "arm,armv7-timer-mem";
			reg = <0xf9020000 0x1000>;
			clock-frequency = <19200000>;

			frame@f9021000 {
				frame-number = <0>;
				interrupts = <0 8 0x4>,
					     <0 7 0x4>;
				reg = <0xf9021000 0x1000>,
				      <0xf9022000 0x1000>;
			};

			frame@f9023000 {
				frame-number = <1>;
				interrupts = <0 9 0x4>;
				reg = <0xf9023000 0x1000>;
				status = "disabled";
			};

			frame@f9024000 {
				frame-number = <2>;
				interrupts = <0 10 0x4>;
				reg = <0xf9024000 0x1000>;
				status = "disabled";
			};

			frame@f9025000 {
				frame-number = <3>;
				interrupts = <0 11 0x4>;
				reg = <0xf9025000 0x1000>;
				status = "disabled";
			};

			frame@f9026000 {
				frame-number = <4>;
				interrupts = <0 12 0x4>;
				reg = <0xf9026000 0x1000>;
				status = "disabled";
			};

			frame@f9027000 {
				frame-number = <5>;
				interrupts = <0 13 0x4>;
				reg = <0xf9027000 0x1000>;
				status = "disabled";
			};

			frame@f9028000 {
				frame-number = <6>;
				interrupts = <0 14 0x4>;
				reg = <0xf9028000 0x1000>;
				status = "disabled";
			};
		};

		saw_l2: regulator@f9012000 {
			compatible = "qcom,saw2";
			reg = <0xf9012000 0x1000>;
			regulator;
		};

		acc0: clock-controller@f9088000 {
			compatible = "qcom,kpss-acc-v2";
			reg = <0xf9088000 0x1000>,
			      <0xf9008000 0x1000>;
		};

		acc1: clock-controller@f9098000 {
			compatible = "qcom,kpss-acc-v2";
			reg = <0xf9098000 0x1000>,
			      <0xf9008000 0x1000>;
		};

		acc2: clock-controller@f90a8000 {
			compatible = "qcom,kpss-acc-v2";
			reg = <0xf90a8000 0x1000>,
			      <0xf9008000 0x1000>;
		};

		acc3: clock-controller@f90b8000 {
			compatible = "qcom,kpss-acc-v2";
			reg = <0xf90b8000 0x1000>,
			      <0xf9008000 0x1000>;
		};

		restart@fc4ab000 {
			compatible = "qcom,pshold";
			reg = <0xfc4ab000 0x4>;
		};
	};
};
