/*
 * Copyright 2013 Eukréa Electromatique <denis@eukrea.com>
 *
 * This program is free software; you can redistribute it and/or
 * modify it under the terms of the GNU General Public License
 * as published by the Free Software Foundation; either version 2
 * of the License, or (at your option) any later version.
 * This program is distributed in the hope that it will be useful,
 * but WITHOUT ANY WARRANTY; without even the implied warranty of
 * MERCHANTABILITY or FITNESS FOR A PARTICULAR PURPOSE.  See the
 * GNU General Public License for more details.
 */

#include "imx35.dtsi"

/ {
	model = "Eukrea CPUIMX35";
	compatible = "eukrea,cpuimx35", "fsl,imx35";

	memory {
		reg = <0x80000000 0x8000000>; /* 128M */
	};
};

&fec {
	pinctrl-names = "default";
	pinctrl-0 = <&pinctrl_fec>;
	status = "okay";
};

&i2c1 {
	pinctrl-names = "default";
	pinctrl-0 = <&pinctrl_i2c1>;
	status = "okay";

	pcf8563@51 {
		compatible = "nxp,pcf8563";
		reg = <0x51>;
	};

	tsc2007: tsc2007@48 {
		compatible = "ti,tsc2007";
		gpios = <&gpio3 2 0>;
		interrupt-parent = <&gpio3>;
		interrupts = <0x2 0x8>;
		pinctrl-names = "default";
		pinctrl-0 = <&pinctrl_tsc2007_1>;
		reg = <0x48>;
		ti,x-plate-ohms = <180>;
	};
};

&iomuxc {
	imx35-eukrea {
		pinctrl_fec: fecgrp {
			fsl,pins = <
				MX35_PAD_FEC_TX_CLK__FEC_TX_CLK		0x80000000
				MX35_PAD_FEC_RX_CLK__FEC_RX_CLK		0x80000000
				MX35_PAD_FEC_RX_DV__FEC_RX_DV		0x80000000
				MX35_PAD_FEC_COL__FEC_COL		0x80000000
				MX35_PAD_FEC_RDATA0__FEC_RDATA_0	0x80000000
				MX35_PAD_FEC_TDATA0__FEC_TDATA_0	0x80000000
				MX35_PAD_FEC_TX_EN__FEC_TX_EN		0x80000000
				MX35_PAD_FEC_MDC__FEC_MDC		0x80000000
				MX35_PAD_FEC_MDIO__FEC_MDIO		0x80000000
				MX35_PAD_FEC_TX_ERR__FEC_TX_ERR		0x80000000
				MX35_PAD_FEC_RX_ERR__FEC_RX_ERR		0x80000000
				MX35_PAD_FEC_CRS__FEC_CRS		0x80000000
				MX35_PAD_FEC_RDATA1__FEC_RDATA_1	0x80000000
				MX35_PAD_FEC_TDATA1__FEC_TDATA_1	0x80000000
				MX35_PAD_FEC_RDATA2__FEC_RDATA_2	0x80000000
				MX35_PAD_FEC_TDATA2__FEC_TDATA_2	0x80000000
				MX35_PAD_FEC_RDATA3__FEC_RDATA_3	0x80000000
				MX35_PAD_FEC_TDATA3__FEC_TDATA_3	0x80000000
			>;
		};

		pinctrl_i2c1: i2c1grp {
			fsl,pins = <
				MX35_PAD_I2C1_CLK__I2C1_SCL		0x80000000
				MX35_PAD_I2C1_DAT__I2C1_SDA		0x80000000
			>;
		};

		pinctrl_tsc2007_1: tsc2007grp-1 {
			fsl,pins = <MX35_PAD_ATA_DA2__GPIO3_2 0x80000000>;
		};
	};
};

&nfc {
	nand-bus-width = <8>;
	nand-ecc-mode = "hw";
	nand-on-flash-bbt;
	status = "okay";
};
