/*
 * Copyright 2011 Freescale Semiconductor, Inc.
 * Copyright 2011 Linaro Ltd.
 *
 * The code contained herein is licensed under the GNU General Public
 * License. You may obtain a copy of the GNU General Public License
 * Version 2 or later at the following locations:
 *
 * http://www.opensource.org/licenses/gpl-license.html
 * http://www.gnu.org/copyleft/gpl.html
 */

/dts-v1/;
#include "imx53.dtsi"

/ {
	model = "Freescale i.MX53 Smart Mobile Reference Design Board";
	compatible = "fsl,imx53-smd", "fsl,imx53";

	memory {
		reg = <0x70000000 0x40000000>;
	};

	gpio-keys {
		compatible = "gpio-keys";

		volume-up {
			label = "Volume Up";
			gpios = <&gpio2 14 0>;
			linux,code = <115>; /* KEY_VOLUMEUP */
		};

		volume-down {
			label = "Volume Down";
			gpios = <&gpio2 15 0>;
			linux,code = <114>; /* KEY_VOLUMEDOWN */
		};
	};
};

&esdhc1 {
	pinctrl-names = "default";
	pinctrl-0 = <&pinctrl_esdhc1>;
	cd-gpios = <&gpio3 13 0>;
	wp-gpios = <&gpio4 11 0>;
	status = "okay";
};

&esdhc2 {
	pinctrl-names = "default";
	pinctrl-0 = <&pinctrl_esdhc2>;
	non-removable;
	status = "okay";
};

&uart3 {
	pinctrl-names = "default";
	pinctrl-0 = <&pinctrl_uart3>;
	fsl,uart-has-rtscts;
	status = "okay";
};

&ecspi1 {
	pinctrl-names = "default";
	pinctrl-0 = <&pinctrl_ecspi1>;
	fsl,spi-num-chipselects = <2>;
	cs-gpios = <&gpio2 30 0>, <&gpio3 19 0>;
	status = "okay";

	zigbee: mc1323@0 {
		compatible = "fsl,mc1323";
		spi-max-frequency = <8000000>;
		reg = <0>;
	};

	flash: m25p32@1 {
		#address-cells = <1>;
		#size-cells = <1>;
		compatible = "st,m25p32", "st,m25p";
		spi-max-frequency = <20000000>;
		reg = <1>;

		partition@0 {
			label = "U-Boot";
			reg = <0x0 0x40000>;
			read-only;
		};

		partition@40000 {
			label = "Kernel";
			reg = <0x40000 0x3c0000>;
		};
	};
};

&esdhc3 {
	pinctrl-names = "default";
	pinctrl-0 = <&pinctrl_esdhc3>;
	non-removable;
	status = "okay";
};

&iomuxc {
	pinctrl-names = "default";
	pinctrl-0 = <&pinctrl_hog>;

	imx53-smd {
		pinctrl_hog: hoggrp {
			fsl,pins = <
				MX53_PAD_PATA_DATA14__GPIO2_14 0x80000000
				MX53_PAD_PATA_DATA15__GPIO2_15 0x80000000
				MX53_PAD_EIM_EB2__GPIO2_30     0x80000000
				MX53_PAD_EIM_DA13__GPIO3_13    0x80000000
				MX53_PAD_EIM_D19__GPIO3_19     0x80000000
				MX53_PAD_KEY_ROW2__GPIO4_11    0x80000000
				MX53_PAD_PATA_DA_0__GPIO7_6    0x80000000
			>;
		};

		pinctrl_ecspi1: ecspi1grp {
			fsl,pins = <
				MX53_PAD_EIM_D16__ECSPI1_SCLK		0x80000000
				MX53_PAD_EIM_D17__ECSPI1_MISO		0x80000000
				MX53_PAD_EIM_D18__ECSPI1_MOSI		0x80000000
			>;
		};

		pinctrl_esdhc1: esdhc1grp {
			fsl,pins = <
				MX53_PAD_SD1_DATA0__ESDHC1_DAT0		0x1d5
				MX53_PAD_SD1_DATA1__ESDHC1_DAT1		0x1d5
				MX53_PAD_SD1_DATA2__ESDHC1_DAT2		0x1d5
				MX53_PAD_SD1_DATA3__ESDHC1_DAT3		0x1d5
				MX53_PAD_SD1_CMD__ESDHC1_CMD		0x1d5
				MX53_PAD_SD1_CLK__ESDHC1_CLK		0x1d5
			>;
		};

		pinctrl_esdhc2: esdhc2grp {
			fsl,pins = <
				MX53_PAD_SD2_CMD__ESDHC2_CMD		0x1d5
				MX53_PAD_SD2_CLK__ESDHC2_CLK		0x1d5
				MX53_PAD_SD2_DATA0__ESDHC2_DAT0		0x1d5
				MX53_PAD_SD2_DATA1__ESDHC2_DAT1		0x1d5
				MX53_PAD_SD2_DATA2__ESDHC2_DAT2		0x1d5
				MX53_PAD_SD2_DATA3__ESDHC2_DAT3		0x1d5
			>;
		};

		pinctrl_esdhc3: esdhc3grp {
			fsl,pins = <
				MX53_PAD_PATA_DATA8__ESDHC3_DAT0	0x1d5
				MX53_PAD_PATA_DATA9__ESDHC3_DAT1	0x1d5
				MX53_PAD_PATA_DATA10__ESDHC3_DAT2	0x1d5
				MX53_PAD_PATA_DATA11__ESDHC3_DAT3	0x1d5
				MX53_PAD_PATA_DATA0__ESDHC3_DAT4	0x1d5
				MX53_PAD_PATA_DATA1__ESDHC3_DAT5	0x1d5
				MX53_PAD_PATA_DATA2__ESDHC3_DAT6	0x1d5
				MX53_PAD_PATA_DATA3__ESDHC3_DAT7	0x1d5
				MX53_PAD_PATA_RESET_B__ESDHC3_CMD	0x1d5
				MX53_PAD_PATA_IORDY__ESDHC3_CLK		0x1d5
			>;
		};

		pinctrl_fec: fecgrp {
			fsl,pins = <
				MX53_PAD_FEC_MDC__FEC_MDC		0x80000000
				MX53_PAD_FEC_MDIO__FEC_MDIO		0x80000000
				MX53_PAD_FEC_REF_CLK__FEC_TX_CLK	0x80000000
				MX53_PAD_FEC_RX_ER__FEC_RX_ER		0x80000000
				MX53_PAD_FEC_CRS_DV__FEC_RX_DV		0x80000000
				MX53_PAD_FEC_RXD1__FEC_RDATA_1		0x80000000
				MX53_PAD_FEC_RXD0__FEC_RDATA_0		0x80000000
				MX53_PAD_FEC_TX_EN__FEC_TX_EN		0x80000000
				MX53_PAD_FEC_TXD1__FEC_TDATA_1		0x80000000
				MX53_PAD_FEC_TXD0__FEC_TDATA_0		0x80000000
			>;
		};

		pinctrl_i2c1: i2c1grp {
			fsl,pins = <
				MX53_PAD_CSI0_DAT8__I2C1_SDA		0xc0000000
				MX53_PAD_CSI0_DAT9__I2C1_SCL		0xc0000000
			>;
		};

		pinctrl_i2c2: i2c2grp {
			fsl,pins = <
				MX53_PAD_KEY_ROW3__I2C2_SDA		0xc0000000
				MX53_PAD_KEY_COL3__I2C2_SCL		0xc0000000
			>;
		};

		pinctrl_uart1: uart1grp {
			fsl,pins = <
				MX53_PAD_CSI0_DAT10__UART1_TXD_MUX	0x1e4
				MX53_PAD_CSI0_DAT11__UART1_RXD_MUX	0x1e4
			>;
		};

		pinctrl_uart2: uart2grp {
			fsl,pins = <
				MX53_PAD_PATA_BUFFER_EN__UART2_RXD_MUX	0x1e4
				MX53_PAD_PATA_DMARQ__UART2_TXD_MUX	0x1e4
			>;
		};

		pinctrl_uart3: uart3grp {
			fsl,pins = <
				MX53_PAD_PATA_CS_0__UART3_TXD_MUX	0x1e4
				MX53_PAD_PATA_CS_1__UART3_RXD_MUX	0x1e4
				MX53_PAD_PATA_DA_1__UART3_CTS		0x1e4
				MX53_PAD_PATA_DA_2__UART3_RTS		0x1e4
			>;
		};
	};
};

&uart1 {
	pinctrl-names = "default";
	pinctrl-0 = <&pinctrl_uart1>;
	status = "okay";
};

&uart2 {
	pinctrl-names = "default";
	pinctrl-0 = <&pinctrl_uart2>;
	status = "okay";
};

&i2c2 {
	pinctrl-names = "default";
	pinctrl-0 = <&pinctrl_i2c2>;
	status = "okay";

	codec: sgtl5000@0a {
		compatible = "fsl,sgtl5000";
		reg = <0x0a>;
	};

	magnetometer: mag3110@0e {
		compatible = "fsl,mag3110";
		reg = <0x0e>;
	};

	touchkey: mpr121@5a {
		compatible = "fsl,mpr121";
		reg = <0x5a>;
	};
};

&i2c1 {
	pinctrl-names = "default";
	pinctrl-0 = <&pinctrl_i2c1>;
	status = "okay";

	accelerometer: mma8450@1c {
		compatible = "fsl,mma8450";
		reg = <0x1c>;
	};

	camera: ov5642@3c {
		compatible = "ovti,ov5642";
		reg = <0x3c>;
	};

	pmic: dialog@48 {
		compatible = "dialog,da9053", "dialog,da9052";
		reg = <0x48>;
	};
};

&fec {
	pinctrl-names = "default";
	pinctrl-0 = <&pinctrl_fec>;
	phy-mode = "rmii";
	phy-reset-gpios = <&gpio7 6 0>;
	status = "okay";
};
