/*
 * Copyright 2014 Texas Instruments, Inc.
 *
 * Keystone 2 Lamarr SoC specific device tree
 *
 * This program is free software; you can redistribute it and/or modify
 * it under the terms of the GNU General Public License version 2 as
 * published by the Free Software Foundation.
 */

/ {
	cpus {
		#address-cells = <1>;
		#size-cells = <0>;

		interrupt-parent = <&gic>;

		cpu@0 {
			compatible = "arm,cortex-a15";
			device_type = "cpu";
			reg = <0>;
		};

		cpu@1 {
			compatible = "arm,cortex-a15";
			device_type = "cpu";
			reg = <1>;
		};
	};

	soc {

		/include/ "k2l-clocks.dtsi"

		uart2: serial@02348400 {
			compatible = "ns16550a";
			current-speed = <115200>;
			reg-shift = <2>;
			reg-io-width = <4>;
			reg = <0x02348400 0x100>;
			clocks	= <&clkuart2>;
			interrupts = <GIC_SPI 432 IRQ_TYPE_EDGE_RISING>;
		};

		uart3:	serial@02348800 {
			compatible = "ns16550a";
			current-speed = <115200>;
			reg-shift = <2>;
			reg-io-width = <4>;
			reg = <0x02348800 0x100>;
			clocks	= <&clkuart3>;
			interrupts = <GIC_SPI 435 IRQ_TYPE_EDGE_RISING>;
		};
	};
};
