/*
 * P3041DS Device Tree Source
 *
 * Copyright 2010-2011 Freescale Semiconductor Inc.
 *
 * Redistribution and use in source and binary forms, with or without
 * modification, are permitted provided that the following conditions are met:
 *     * Redistributions of source code must retain the above copyright
 *       notice, this list of conditions and the following disclaimer.
 *     * Redistributions in binary form must reproduce the above copyright
 *       notice, this list of conditions and the following disclaimer in the
 *       documentation and/or other materials provided with the distribution.
 *     * Neither the name of Freescale Semiconductor nor the
 *       names of its contributors may be used to endorse or promote products
 *       derived from this software without specific prior written permission.
 *
 *
 * ALTERNATIVELY, this software may be distributed under the terms of the
 * GNU General Public License ("GPL") as published by the Free Software
 * Foundation, either version 2 of that License or (at your option) any
 * later version.
 *
 * THIS SOFTWARE IS PROVIDED BY Freescale Semiconductor ``AS IS'' AND ANY
 * EXPRESS OR IMPLIED WARRANTIES, INCLUDING, BUT NOT LIMITED TO, THE IMPLIED
 * WARRANTIES OF MERCHANTABILITY AND FITNESS FOR A PARTICULAR PURPOSE ARE
 * DISCLAIMED. IN NO EVENT SHALL Freescale Semiconductor BE LIABLE FOR ANY
 * DIRECT, INDIRECT, INCIDENTAL, SPECIAL, EXEMPLARY, OR CONSEQUENTIAL DAMAGES
 * (INCLUDING, BUT NOT LIMITED TO, PROCUREMENT OF SUBSTITUTE GOODS OR SERVICES;
 * LOSS OF USE, DATA, OR PROFITS; OR BUSINESS INTERRUPTION) HOWEVER CAUSED AND
 * ON ANY THEORY OF LIABILITY, WHETHER IN CONTRACT, STRICT LIABILITY, OR TORT
 * (INCLUDING NEGLIGENCE OR OTHERWISE) ARISING IN ANY WAY OUT OF THE USE OF THIS
 * SOFTWARE, EVEN IF ADVISED OF THE POSSIBILITY OF SUCH DAMAGE.
 */

/include/ "fsl/p3041si-pre.dtsi"

/ {
	model = "fsl,P3041DS";
	compatible = "fsl,P3041DS";
	#address-cells = <2>;
	#size-cells = <2>;
	interrupt-parent = <&mpic>;

	memory {
		device_type = "memory";
	};

	dcsr: dcsr@f00000000 {
		ranges = <0x00000000 0xf 0x00000000 0x01008000>;
	};

	soc: soc@ffe000000 {
		ranges = <0x00000000 0xf 0xfe000000 0x1000000>;
		reg = <0xf 0xfe000000 0 0x00001000>;
		spi@110000 {
			flash@0 {
				#address-cells = <1>;
				#size-cells = <1>;
				compatible = "spansion,s25sl12801";
				reg = <0>;
				spi-max-frequency = <35000000>; /* input clock */
				partition@u-boot {
					label = "u-boot";
					reg = <0x00000000 0x00100000>;
					read-only;
				};
				partition@kernel {
					label = "kernel";
					reg = <0x00100000 0x00500000>;
					read-only;
				};
				partition@dtb {
					label = "dtb";
					reg = <0x00600000 0x00100000>;
					read-only;
				};
				partition@fs {
					label = "file system";
					reg = <0x00700000 0x00900000>;
				};
			};
		};

		i2c@118100 {
			eeprom@51 {
				compatible = "at24,24c256";
				reg = <0x51>;
			};
			eeprom@52 {
				compatible = "at24,24c256";
				reg = <0x52>;
			};
		};

		i2c@119100 {
			rtc@68 {
				compatible = "dallas,ds3232";
				reg = <0x68>;
				interrupts = <0x1 0x1 0 0>;
			};
			adt7461@4c {
				compatible = "adi,adt7461";
				reg = <0x4c>;
			};
		};
	};

	rio: rapidio@ffe0c0000 {
		reg = <0xf 0xfe0c0000 0 0x11000>;

		port1 {
			ranges = <0 0 0xc 0x20000000 0 0x10000000>;
		};
		port2 {
			ranges = <0 0 0xc 0x30000000 0 0x10000000>;
		};
	};

	lbc: localbus@ffe124000 {
		reg = <0xf 0xfe124000 0 0x1000>;
		ranges = <0 0 0xf 0xe8000000 0x08000000
			  2 0 0xf 0xffa00000 0x00040000
			  3 0 0xf 0xffdf0000 0x00008000>;

		flash@0,0 {
			compatible = "cfi-flash";
			reg = <0 0 0x08000000>;
			bank-width = <2>;
			device-width = <2>;
		};

		nand@2,0 {
			#address-cells = <1>;
			#size-cells = <1>;
			compatible = "fsl,elbc-fcm-nand";
			reg = <0x2 0x0 0x40000>;

			partition@0 {
				label = "NAND U-Boot Image";
				reg = <0x0 0x02000000>;
				read-only;
			};

			partition@2000000 {
				label = "NAND Root File System";
				reg = <0x02000000 0x10000000>;
			};

			partition@12000000 {
				label = "NAND Compressed RFS Image";
				reg = <0x12000000 0x08000000>;
			};

			partition@1a000000 {
				label = "NAND Linux Kernel Image";
				reg = <0x1a000000 0x04000000>;
			};

			partition@1e000000 {
				label = "NAND DTB Image";
				reg = <0x1e000000 0x01000000>;
			};

			partition@1f000000 {
				label = "NAND Writable User area";
				reg = <0x1f000000 0x21000000>;
			};
		};

		board-control@3,0 {
			compatible = "fsl,p3041ds-fpga", "fsl,fpga-ngpixis";
			reg = <3 0 0x30>;
		};
	};

	pci0: pcie@ffe200000 {
		reg = <0xf 0xfe200000 0 0x1000>;
		ranges = <0x02000000 0 0xe0000000 0xc 0x00000000 0x0 0x20000000
			  0x01000000 0 0x00000000 0xf 0xf8000000 0x0 0x00010000>;
		pcie@0 {
			ranges = <0x02000000 0 0xe0000000
				  0x02000000 0 0xe0000000
				  0 0x20000000

				  0x01000000 0 0x00000000
				  0x01000000 0 0x00000000
				  0 0x00010000>;
		};
	};

	pci1: pcie@ffe201000 {
		reg = <0xf 0xfe201000 0 0x1000>;
		ranges = <0x02000000 0x0 0xe0000000 0xc 0x20000000 0x0 0x20000000
			  0x01000000 0x0 0x00000000 0xf 0xf8010000 0x0 0x00010000>;
		pcie@0 {
			ranges = <0x02000000 0 0xe0000000
				  0x02000000 0 0xe0000000
				  0 0x20000000

				  0x01000000 0 0x00000000
				  0x01000000 0 0x00000000
				  0 0x00010000>;
		};
	};

	pci2: pcie@ffe202000 {
		reg = <0xf 0xfe202000 0 0x1000>;
		ranges = <0x02000000 0 0xe0000000 0xc 0x40000000 0 0x20000000
			  0x01000000 0 0x00000000 0xf 0xf8020000 0 0x00010000>;
		pcie@0 {
			ranges = <0x02000000 0 0xe0000000
				  0x02000000 0 0xe0000000
				  0 0x20000000

				  0x01000000 0 0x00000000
				  0x01000000 0 0x00000000
				  0 0x00010000>;
		};
	};

	pci3: pcie@ffe203000 {
		reg = <0xf 0xfe203000 0 0x1000>;
		ranges = <0x02000000 0 0xe0000000 0xc 0x60000000 0 0x20000000
			  0x01000000 0 0x00000000 0xf 0xf8030000 0 0x00010000>;
		pcie@0 {
			ranges = <0x02000000 0 0xe0000000
				  0x02000000 0 0xe0000000
				  0 0x20000000

				  0x01000000 0 0x00000000
				  0x01000000 0 0x00000000
				  0 0x00010000>;
		};
	};
};

/include/ "fsl/p3041si-post.dtsi"
