/*
 * Common features on the Zoom debug board
 */

#include "omap-gpmc-smsc911x.dtsi"

&gpmc {
	ranges = <3 0 0x10000000 0x00000400>,
		 <7 0 0x2c000000 0x01000000>;

	/*
	 * Four port TL16CP754C serial port on GPMC,
	 * they probably share the same GPIO IRQ
	 * REVISIT: Add timing support from slls644g.pdf
	 */
	uart@3,0 {
		compatible = "ns16550a";
		reg = <3 0 0x100>;
		bank-width = <2>;
		reg-shift = <1>;
		reg-io-width = <1>;
		interrupt-parent = <&gpio4>;
		interrupts = <6 IRQ_TYPE_EDGE_RISING>;	/* gpio102 */
		clock-frequency = <1843200>;
		current-speed = <115200>;
	};

	ethernet@gpmc {
		reg = <7 0 0xff>;
		interrupt-parent = <&gpio5>;
		interrupts = <30 IRQ_TYPE_LEVEL_LOW>;	/* gpio158 */
	};
};
