/*
 * SAMSUNG EXYNOS5250 SoC device tree source
 *
 * Copyright (c) 2012 Samsung Electronics Co., Ltd.
 *		http://www.samsung.com
 *
 * SAMSUNG EXYNOS5250 SoC device nodes are listed in this file.
 * EXYNOS5250 based board files can include this file and provide
 * values for board specfic bindings.
 *
 * Note: This file does not include device nodes for all the controllers in
 * EXYNOS5250 SoC. As device tree coverage for EXYNOS5250 increases,
 * additional nodes can be added to this file.
 *
 * This program is free software; you can redistribute it and/or modify
 * it under the terms of the GNU General Public License version 2 as
 * published by the Free Software Foundation.
*/

#include <dt-bindings/clock/exynos5250.h>
#include "exynos5.dtsi"
#include "exynos5250-pinctrl.dtsi"

#include <dt-bindings/clock/exynos-audss-clk.h>

/ {
	compatible = "samsung,exynos5250", "samsung,exynos5";

	aliases {
		spi0 = &spi_0;
		spi1 = &spi_1;
		spi2 = &spi_2;
		gsc0 = &gsc_0;
		gsc1 = &gsc_1;
		gsc2 = &gsc_2;
		gsc3 = &gsc_3;
		mshc0 = &mmc_0;
		mshc1 = &mmc_1;
		mshc2 = &mmc_2;
		mshc3 = &mmc_3;
		i2c0 = &i2c_0;
		i2c1 = &i2c_1;
		i2c2 = &i2c_2;
		i2c3 = &i2c_3;
		i2c4 = &i2c_4;
		i2c5 = &i2c_5;
		i2c6 = &i2c_6;
		i2c7 = &i2c_7;
		i2c8 = &i2c_8;
		i2c9 = &i2c_9;
		pinctrl0 = &pinctrl_0;
		pinctrl1 = &pinctrl_1;
		pinctrl2 = &pinctrl_2;
		pinctrl3 = &pinctrl_3;
	};

	cpus {
		#address-cells = <1>;
		#size-cells = <0>;

		cpu@0 {
			device_type = "cpu";
			compatible = "arm,cortex-a15";
			reg = <0>;
			clock-frequency = <1700000000>;
		};
		cpu@1 {
			device_type = "cpu";
			compatible = "arm,cortex-a15";
			reg = <1>;
			clock-frequency = <1700000000>;
		};
	};

	sysram@02020000 {
		compatible = "mmio-sram";
		reg = <0x02020000 0x30000>;
		#address-cells = <1>;
		#size-cells = <1>;
		ranges = <0 0x02020000 0x30000>;

		smp-sysram@0 {
			compatible = "samsung,exynos4210-sysram";
			reg = <0x0 0x1000>;
		};

		smp-sysram@2f000 {
			compatible = "samsung,exynos4210-sysram-ns";
			reg = <0x2f000 0x1000>;
		};
	};

	pd_gsc: gsc-power-domain@10044000 {
		compatible = "samsung,exynos4210-pd";
		reg = <0x10044000 0x20>;
	};

	pd_mfc: mfc-power-domain@10044040 {
		compatible = "samsung,exynos4210-pd";
		reg = <0x10044040 0x20>;
	};

	clock: clock-controller@10010000 {
		compatible = "samsung,exynos5250-clock";
		reg = <0x10010000 0x30000>;
		#clock-cells = <1>;
	};

	clock_audss: audss-clock-controller@3810000 {
		compatible = "samsung,exynos5250-audss-clock";
		reg = <0x03810000 0x0C>;
		#clock-cells = <1>;
		clocks = <&clock CLK_FIN_PLL>, <&clock CLK_FOUT_EPLL>,
			 <&clock CLK_SCLK_AUDIO0>, <&clock CLK_DIV_PCM0>;
		clock-names = "pll_ref", "pll_in", "sclk_audio", "sclk_pcm_in";
	};

	timer {
		compatible = "arm,armv7-timer";
		interrupts = <1 13 0xf08>,
			     <1 14 0xf08>,
			     <1 11 0xf08>,
			     <1 10 0xf08>;
		/* Unfortunately we need this since some versions of U-Boot
		 * on Exynos don't set the CNTFRQ register, so we need the
		 * value from DT.
		 */
		clock-frequency = <24000000>;
	};

	mct@101C0000 {
		compatible = "samsung,exynos4210-mct";
		reg = <0x101C0000 0x800>;
		interrupt-controller;
		#interrups-cells = <2>;
		interrupt-parent = <&mct_map>;
		interrupts = <0 0>, <1 0>, <2 0>, <3 0>,
			     <4 0>, <5 0>;
		clocks = <&clock CLK_FIN_PLL>, <&clock CLK_MCT>;
		clock-names = "fin_pll", "mct";

		mct_map: mct-map {
			#interrupt-cells = <2>;
			#address-cells = <0>;
			#size-cells = <0>;
			interrupt-map = <0x0 0 &combiner 23 3>,
					<0x1 0 &combiner 23 4>,
					<0x2 0 &combiner 25 2>,
					<0x3 0 &combiner 25 3>,
					<0x4 0 &gic 0 120 0>,
					<0x5 0 &gic 0 121 0>;
		};
	};

	pmu {
		compatible = "arm,cortex-a15-pmu";
		interrupt-parent = <&combiner>;
		interrupts = <1 2>, <22 4>;
	};

	pinctrl_0: pinctrl@11400000 {
		compatible = "samsung,exynos5250-pinctrl";
		reg = <0x11400000 0x1000>;
		interrupts = <0 46 0>;

		wakup_eint: wakeup-interrupt-controller {
			compatible = "samsung,exynos4210-wakeup-eint";
			interrupt-parent = <&gic>;
			interrupts = <0 32 0>;
		};
	};

	pinctrl_1: pinctrl@13400000 {
		compatible = "samsung,exynos5250-pinctrl";
		reg = <0x13400000 0x1000>;
		interrupts = <0 45 0>;
	};

	pinctrl_2: pinctrl@10d10000 {
		compatible = "samsung,exynos5250-pinctrl";
		reg = <0x10d10000 0x1000>;
		interrupts = <0 50 0>;
	};

	pinctrl_3: pinctrl@03860000 {
		compatible = "samsung,exynos5250-pinctrl";
		reg = <0x03860000 0x1000>;
		interrupts = <0 47 0>;
	};

	pmu_system_controller: system-controller@10040000 {
		compatible = "samsung,exynos5250-pmu", "syscon";
		reg = <0x10040000 0x5000>;
	};

	sysreg_system_controller: syscon@10050000 {
		compatible = "samsung,exynos5-sysreg", "syscon";
		reg = <0x10050000 0x5000>;
	};

	watchdog@101D0000 {
		compatible = "samsung,exynos5250-wdt";
		reg = <0x101D0000 0x100>;
		interrupts = <0 42 0>;
		clocks = <&clock CLK_WDT>;
		clock-names = "watchdog";
		samsung,syscon-phandle = <&pmu_system_controller>;
	};

	g2d@10850000 {
		compatible = "samsung,exynos5250-g2d";
		reg = <0x10850000 0x1000>;
		interrupts = <0 91 0>;
		clocks = <&clock CLK_G2D>;
		clock-names = "fimg2d";
	};

	codec@11000000 {
		compatible = "samsung,mfc-v6";
		reg = <0x11000000 0x10000>;
		interrupts = <0 96 0>;
		samsung,power-domain = <&pd_mfc>;
		clocks = <&clock CLK_MFC>;
		clock-names = "mfc";
	};

	rtc@101E0000 {
		clocks = <&clock CLK_RTC>;
		clock-names = "rtc";
		status = "disabled";
	};

	tmu@10060000 {
		compatible = "samsung,exynos5250-tmu";
		reg = <0x10060000 0x100>;
		interrupts = <0 65 0>;
		clocks = <&clock CLK_TMU>;
		clock-names = "tmu_apbif";
	};

	serial@12C00000 {
		clocks = <&clock CLK_UART0>, <&clock CLK_SCLK_UART0>;
		clock-names = "uart", "clk_uart_baud0";
	};

	serial@12C10000 {
		clocks = <&clock CLK_UART1>, <&clock CLK_SCLK_UART1>;
		clock-names = "uart", "clk_uart_baud0";
	};

	serial@12C20000 {
		clocks = <&clock CLK_UART2>, <&clock CLK_SCLK_UART2>;
		clock-names = "uart", "clk_uart_baud0";
	};

	serial@12C30000 {
		clocks = <&clock CLK_UART3>, <&clock CLK_SCLK_UART3>;
		clock-names = "uart", "clk_uart_baud0";
	};

	sata@122F0000 {
		compatible = "snps,dwc-ahci";
		samsung,sata-freq = <66>;
		reg = <0x122F0000 0x1ff>;
		interrupts = <0 115 0>;
		clocks = <&clock CLK_SATA>, <&clock CLK_SCLK_SATA>;
		clock-names = "sata", "sclk_sata";
		phys = <&sata_phy>;
		phy-names = "sata-phy";
		status = "disabled";
	};

	sata_phy: sata-phy@12170000 {
		compatible = "samsung,exynos5250-sata-phy";
		reg = <0x12170000 0x1ff>;
		clocks = <&clock CLK_SATA_PHYCTRL>;
		clock-names = "sata_phyctrl";
		#phy-cells = <0>;
		samsung,syscon-phandle = <&pmu_system_controller>;
		status = "disabled";
	};

	i2c_0: i2c@12C60000 {
		compatible = "samsung,s3c2440-i2c";
		reg = <0x12C60000 0x100>;
		interrupts = <0 56 0>;
		#address-cells = <1>;
		#size-cells = <0>;
		clocks = <&clock CLK_I2C0>;
		clock-names = "i2c";
		pinctrl-names = "default";
		pinctrl-0 = <&i2c0_bus>;
		status = "disabled";
	};

	i2c_1: i2c@12C70000 {
		compatible = "samsung,s3c2440-i2c";
		reg = <0x12C70000 0x100>;
		interrupts = <0 57 0>;
		#address-cells = <1>;
		#size-cells = <0>;
		clocks = <&clock CLK_I2C1>;
		clock-names = "i2c";
		pinctrl-names = "default";
		pinctrl-0 = <&i2c1_bus>;
		status = "disabled";
	};

	i2c_2: i2c@12C80000 {
		compatible = "samsung,s3c2440-i2c";
		reg = <0x12C80000 0x100>;
		interrupts = <0 58 0>;
		#address-cells = <1>;
		#size-cells = <0>;
		clocks = <&clock CLK_I2C2>;
		clock-names = "i2c";
		pinctrl-names = "default";
		pinctrl-0 = <&i2c2_bus>;
		status = "disabled";
	};

	i2c_3: i2c@12C90000 {
		compatible = "samsung,s3c2440-i2c";
		reg = <0x12C90000 0x100>;
		interrupts = <0 59 0>;
		#address-cells = <1>;
		#size-cells = <0>;
		clocks = <&clock CLK_I2C3>;
		clock-names = "i2c";
		pinctrl-names = "default";
		pinctrl-0 = <&i2c3_bus>;
		status = "disabled";
	};

	i2c_4: i2c@12CA0000 {
		compatible = "samsung,s3c2440-i2c";
		reg = <0x12CA0000 0x100>;
		interrupts = <0 60 0>;
		#address-cells = <1>;
		#size-cells = <0>;
		clocks = <&clock CLK_I2C4>;
		clock-names = "i2c";
		pinctrl-names = "default";
		pinctrl-0 = <&i2c4_bus>;
		status = "disabled";
	};

	i2c_5: i2c@12CB0000 {
		compatible = "samsung,s3c2440-i2c";
		reg = <0x12CB0000 0x100>;
		interrupts = <0 61 0>;
		#address-cells = <1>;
		#size-cells = <0>;
		clocks = <&clock CLK_I2C5>;
		clock-names = "i2c";
		pinctrl-names = "default";
		pinctrl-0 = <&i2c5_bus>;
		status = "disabled";
	};

	i2c_6: i2c@12CC0000 {
		compatible = "samsung,s3c2440-i2c";
		reg = <0x12CC0000 0x100>;
		interrupts = <0 62 0>;
		#address-cells = <1>;
		#size-cells = <0>;
		clocks = <&clock CLK_I2C6>;
		clock-names = "i2c";
		pinctrl-names = "default";
		pinctrl-0 = <&i2c6_bus>;
		status = "disabled";
	};

	i2c_7: i2c@12CD0000 {
		compatible = "samsung,s3c2440-i2c";
		reg = <0x12CD0000 0x100>;
		interrupts = <0 63 0>;
		#address-cells = <1>;
		#size-cells = <0>;
		clocks = <&clock CLK_I2C7>;
		clock-names = "i2c";
		pinctrl-names = "default";
		pinctrl-0 = <&i2c7_bus>;
		status = "disabled";
	};

	i2c_8: i2c@12CE0000 {
		compatible = "samsung,s3c2440-hdmiphy-i2c";
		reg = <0x12CE0000 0x1000>;
		interrupts = <0 64 0>;
		#address-cells = <1>;
		#size-cells = <0>;
		clocks = <&clock CLK_I2C_HDMI>;
		clock-names = "i2c";
		status = "disabled";
	};

	i2c_9: i2c@121D0000 {
                compatible = "samsung,exynos5-sata-phy-i2c";
                reg = <0x121D0000 0x100>;
                #address-cells = <1>;
                #size-cells = <0>;
		clocks = <&clock CLK_SATA_PHYI2C>;
		clock-names = "i2c";
		status = "disabled";
	};

	spi_0: spi@12d20000 {
		compatible = "samsung,exynos4210-spi";
		status = "disabled";
		reg = <0x12d20000 0x100>;
		interrupts = <0 66 0>;
		dmas = <&pdma0 5
			&pdma0 4>;
		dma-names = "tx", "rx";
		#address-cells = <1>;
		#size-cells = <0>;
		clocks = <&clock CLK_SPI0>, <&clock CLK_SCLK_SPI0>;
		clock-names = "spi", "spi_busclk0";
		pinctrl-names = "default";
		pinctrl-0 = <&spi0_bus>;
	};

	spi_1: spi@12d30000 {
		compatible = "samsung,exynos4210-spi";
		status = "disabled";
		reg = <0x12d30000 0x100>;
		interrupts = <0 67 0>;
		dmas = <&pdma1 5
			&pdma1 4>;
		dma-names = "tx", "rx";
		#address-cells = <1>;
		#size-cells = <0>;
		clocks = <&clock CLK_SPI1>, <&clock CLK_SCLK_SPI1>;
		clock-names = "spi", "spi_busclk0";
		pinctrl-names = "default";
		pinctrl-0 = <&spi1_bus>;
	};

	spi_2: spi@12d40000 {
		compatible = "samsung,exynos4210-spi";
		status = "disabled";
		reg = <0x12d40000 0x100>;
		interrupts = <0 68 0>;
		dmas = <&pdma0 7
			&pdma0 6>;
		dma-names = "tx", "rx";
		#address-cells = <1>;
		#size-cells = <0>;
		clocks = <&clock CLK_SPI2>, <&clock CLK_SCLK_SPI2>;
		clock-names = "spi", "spi_busclk0";
		pinctrl-names = "default";
		pinctrl-0 = <&spi2_bus>;
	};

	mmc_0: mmc@12200000 {
		compatible = "samsung,exynos5250-dw-mshc";
		interrupts = <0 75 0>;
		#address-cells = <1>;
		#size-cells = <0>;
		reg = <0x12200000 0x1000>;
		clocks = <&clock CLK_SDMMC0>, <&clock CLK_SCLK_MMC0>;
		clock-names = "biu", "ciu";
		fifo-depth = <0x80>;
		status = "disabled";
	};

	mmc_1: mmc@12210000 {
		compatible = "samsung,exynos5250-dw-mshc";
		interrupts = <0 76 0>;
		#address-cells = <1>;
		#size-cells = <0>;
		reg = <0x12210000 0x1000>;
		clocks = <&clock CLK_SDMMC1>, <&clock CLK_SCLK_MMC1>;
		clock-names = "biu", "ciu";
		fifo-depth = <0x80>;
		status = "disabled";
	};

	mmc_2: mmc@12220000 {
		compatible = "samsung,exynos5250-dw-mshc";
		interrupts = <0 77 0>;
		#address-cells = <1>;
		#size-cells = <0>;
		reg = <0x12220000 0x1000>;
		clocks = <&clock CLK_SDMMC2>, <&clock CLK_SCLK_MMC2>;
		clock-names = "biu", "ciu";
		fifo-depth = <0x80>;
		status = "disabled";
	};

	mmc_3: mmc@12230000 {
		compatible = "samsung,exynos5250-dw-mshc";
		reg = <0x12230000 0x1000>;
		interrupts = <0 78 0>;
		#address-cells = <1>;
		#size-cells = <0>;
		clocks = <&clock CLK_SDMMC3>, <&clock CLK_SCLK_MMC3>;
		clock-names = "biu", "ciu";
		fifo-depth = <0x80>;
		status = "disabled";
	};

	i2s0: i2s@03830000 {
		compatible = "samsung,s5pv210-i2s";
		status = "disabled";
		reg = <0x03830000 0x100>;
		dmas = <&pdma0 10
			&pdma0 9
			&pdma0 8>;
		dma-names = "tx", "rx", "tx-sec";
		clocks = <&clock_audss EXYNOS_I2S_BUS>,
			<&clock_audss EXYNOS_I2S_BUS>,
			<&clock_audss EXYNOS_SCLK_I2S>;
		clock-names = "iis", "i2s_opclk0", "i2s_opclk1";
		samsung,idma-addr = <0x03000000>;
		pinctrl-names = "default";
		pinctrl-0 = <&i2s0_bus>;
	};

	i2s1: i2s@12D60000 {
		compatible = "samsung,s3c6410-i2s";
		status = "disabled";
		reg = <0x12D60000 0x100>;
		dmas = <&pdma1 12
			&pdma1 11>;
		dma-names = "tx", "rx";
		clocks = <&clock CLK_I2S1>, <&clock CLK_DIV_I2S1>;
		clock-names = "iis", "i2s_opclk0";
		pinctrl-names = "default";
		pinctrl-0 = <&i2s1_bus>;
	};

	i2s2: i2s@12D70000 {
		compatible = "samsung,s3c6410-i2s";
		status = "disabled";
		reg = <0x12D70000 0x100>;
		dmas = <&pdma0 12
			&pdma0 11>;
		dma-names = "tx", "rx";
		clocks = <&clock CLK_I2S2>, <&clock CLK_DIV_I2S2>;
		clock-names = "iis", "i2s_opclk0";
		pinctrl-names = "default";
		pinctrl-0 = <&i2s2_bus>;
	};

	usb@12000000 {
		compatible = "samsung,exynos5250-dwusb3";
		clocks = <&clock CLK_USB3>;
		clock-names = "usbdrd30";
		#address-cells = <1>;
		#size-cells = <1>;
		ranges;

		dwc3 {
			compatible = "synopsys,dwc3";
			reg = <0x12000000 0x10000>;
			interrupts = <0 72 0>;
			phys = <&usbdrd_phy 0>, <&usbdrd_phy 1>;
			phy-names = "usb2-phy", "usb3-phy";
		};
	};

	usbdrd_phy: phy@12100000 {
		compatible = "samsung,exynos5250-usbdrd-phy";
		reg = <0x12100000 0x100>;
		clocks = <&clock CLK_USB3>, <&clock CLK_FIN_PLL>;
		clock-names = "phy", "ref";
		samsung,pmu-syscon = <&pmu_system_controller>;
		#phy-cells = <1>;
	};

	usb@12110000 {
		compatible = "samsung,exynos4210-ehci";
		reg = <0x12110000 0x100>;
		interrupts = <0 71 0>;

		clocks = <&clock CLK_USB2>;
		clock-names = "usbhost";
		#address-cells = <1>;
		#size-cells = <0>;
		port@0 {
			reg = <0>;
			phys = <&usb2_phy_gen 1>;
		};
	};

	usb@12120000 {
		compatible = "samsung,exynos4210-ohci";
		reg = <0x12120000 0x100>;
		interrupts = <0 71 0>;

		clocks = <&clock CLK_USB2>;
		clock-names = "usbhost";
		#address-cells = <1>;
		#size-cells = <0>;
		port@0 {
			reg = <0>;
			phys = <&usb2_phy_gen 1>;
		};
	};

	usb2_phy: usbphy@12130000 {
		compatible = "samsung,exynos5250-usb2phy";
		reg = <0x12130000 0x100>;
		clocks = <&clock CLK_FIN_PLL>, <&clock CLK_USB2>;
		clock-names = "ext_xtal", "usbhost";
		#address-cells = <1>;
		#size-cells = <1>;
		ranges;

		usbphy-sys {
			reg = <0x10040704 0x8>,
			      <0x10050230 0x4>;
		};
	};

	usb2_phy_gen: phy@12130000 {
		compatible = "samsung,exynos5250-usb2-phy";
		reg = <0x12130000 0x100>;
		clocks = <&clock CLK_USB2>, <&clock CLK_FIN_PLL>;
		clock-names = "phy", "ref";
		#phy-cells = <1>;
		samsung,sysreg-phandle = <&sysreg_system_controller>;
		samsung,pmureg-phandle = <&pmu_system_controller>;
	};

	pwm: pwm@12dd0000 {
		compatible = "samsung,exynos4210-pwm";
		reg = <0x12dd0000 0x100>;
		samsung,pwm-outputs = <0>, <1>, <2>, <3>;
		#pwm-cells = <3>;
		clocks = <&clock CLK_PWM>;
		clock-names = "timers";
	};

	amba {
		#address-cells = <1>;
		#size-cells = <1>;
		compatible = "arm,amba-bus";
		interrupt-parent = <&gic>;
		ranges;

		pdma0: pdma@121A0000 {
			compatible = "arm,pl330", "arm,primecell";
			reg = <0x121A0000 0x1000>;
			interrupts = <0 34 0>;
			clocks = <&clock CLK_PDMA0>;
			clock-names = "apb_pclk";
			#dma-cells = <1>;
			#dma-channels = <8>;
			#dma-requests = <32>;
		};

		pdma1: pdma@121B0000 {
			compatible = "arm,pl330", "arm,primecell";
			reg = <0x121B0000 0x1000>;
			interrupts = <0 35 0>;
			clocks = <&clock CLK_PDMA1>;
			clock-names = "apb_pclk";
			#dma-cells = <1>;
			#dma-channels = <8>;
			#dma-requests = <32>;
		};

		mdma0: mdma@10800000 {
			compatible = "arm,pl330", "arm,primecell";
			reg = <0x10800000 0x1000>;
			interrupts = <0 33 0>;
			clocks = <&clock CLK_MDMA0>;
			clock-names = "apb_pclk";
			#dma-cells = <1>;
			#dma-channels = <8>;
			#dma-requests = <1>;
		};

		mdma1: mdma@11C10000 {
			compatible = "arm,pl330", "arm,primecell";
			reg = <0x11C10000 0x1000>;
			interrupts = <0 124 0>;
			clocks = <&clock CLK_MDMA1>;
			clock-names = "apb_pclk";
			#dma-cells = <1>;
			#dma-channels = <8>;
			#dma-requests = <1>;
		};
	};

	gsc_0:  gsc@13e00000 {
		compatible = "samsung,exynos5-gsc";
		reg = <0x13e00000 0x1000>;
		interrupts = <0 85 0>;
		samsung,power-domain = <&pd_gsc>;
		clocks = <&clock CLK_GSCL0>;
		clock-names = "gscl";
	};

	gsc_1:  gsc@13e10000 {
		compatible = "samsung,exynos5-gsc";
		reg = <0x13e10000 0x1000>;
		interrupts = <0 86 0>;
		samsung,power-domain = <&pd_gsc>;
		clocks = <&clock CLK_GSCL1>;
		clock-names = "gscl";
	};

	gsc_2:  gsc@13e20000 {
		compatible = "samsung,exynos5-gsc";
		reg = <0x13e20000 0x1000>;
		interrupts = <0 87 0>;
		samsung,power-domain = <&pd_gsc>;
		clocks = <&clock CLK_GSCL2>;
		clock-names = "gscl";
	};

	gsc_3:  gsc@13e30000 {
		compatible = "samsung,exynos5-gsc";
		reg = <0x13e30000 0x1000>;
		interrupts = <0 88 0>;
		samsung,power-domain = <&pd_gsc>;
		clocks = <&clock CLK_GSCL3>;
		clock-names = "gscl";
	};

	hdmi {
		compatible = "samsung,exynos4212-hdmi";
		reg = <0x14530000 0x70000>;
		interrupts = <0 95 0>;
		clocks = <&clock CLK_HDMI>, <&clock CLK_SCLK_HDMI>,
			 <&clock CLK_SCLK_PIXEL>, <&clock CLK_SCLK_HDMIPHY>,
			 <&clock CLK_MOUT_HDMI>;
		clock-names = "hdmi", "sclk_hdmi", "sclk_pixel",
				"sclk_hdmiphy", "mout_hdmi";
		samsung,syscon-phandle = <&pmu_system_controller>;
	};

	mixer {
		compatible = "samsung,exynos5250-mixer";
		reg = <0x14450000 0x10000>;
		interrupts = <0 94 0>;
		clocks = <&clock CLK_MIXER>, <&clock CLK_SCLK_HDMI>;
		clock-names = "mixer", "sclk_hdmi";
	};

	dp_phy: video-phy@10040720 {
		compatible = "samsung,exynos5250-dp-video-phy";
		reg = <0x10040720 4>;
		#phy-cells = <0>;
	};

	dp-controller@145B0000 {
		clocks = <&clock CLK_DP>;
		clock-names = "dp";
		phys = <&dp_phy>;
		phy-names = "dp";
	};

	fimd@14400000 {
		clocks = <&clock CLK_SCLK_FIMD1>, <&clock CLK_FIMD1>;
		clock-names = "sclk_fimd", "fimd";
	};

	adc: adc@12D10000 {
		compatible = "samsung,exynos-adc-v1";
		reg = <0x12D10000 0x100>, <0x10040718 0x4>;
		interrupts = <0 106 0>;
		clocks = <&clock CLK_ADC>;
		clock-names = "adc";
		#io-channel-cells = <1>;
		io-channel-ranges;
		status = "disabled";
	};

	sss@10830000 {
		compatible = "samsung,exynos4210-secss";
		reg = <0x10830000 0x10000>;
		interrupts = <0 112 0>;
		clocks = <&clock CLK_SSS>;
		clock-names = "secss";
	};
};
