/*
 * wm8505.dtsi - Device tree file for Wondermedia WM8505 SoC
 *
 * Copyright (C) 2012 Tony Prisk <linux@prisktech.co.nz>
 *
 * Licensed under GPLv2 or later
 */

/include/ "skeleton.dtsi"

/ {
	compatible = "wm,wm8505";

	cpus {
		#address-cells = <0>;
		#size-cells = <0>;

		cpu {
			device_type = "cpu";
			compatible = "arm,arm926ej-s";
		};
	};

 	aliases {
		serial0 = &uart0;
		serial1 = &uart1;
		serial2 = &uart2;
		serial3 = &uart3;
		serial4 = &uart4;
		serial5 = &uart5;
 	};

	soc {
		#address-cells = <1>;
		#size-cells = <1>;
		compatible = "simple-bus";
		ranges;
		interrupt-parent = <&intc0>;

		intc0: interrupt-controller@d8140000 {
			compatible = "via,vt8500-intc";
			interrupt-controller;
			reg = <0xd8140000 0x10000>;
			#interrupt-cells = <1>;
		};

		/* Secondary IC cascaded to intc0 */
		intc1: interrupt-controller@d8150000 {
			compatible = "via,vt8500-intc";
			interrupt-controller;
			#interrupt-cells = <1>;
			reg = <0xD8150000 0x10000>;
			interrupts = <56 57 58 59 60 61 62 63>;
		};

		pinctrl: pinctrl@d8110000 {
			compatible = "wm,wm8505-pinctrl";
			reg = <0xd8110000 0x10000>;
			interrupt-controller;
			#interrupt-cells = <2>;
			gpio-controller;
			#gpio-cells = <2>;
		};

		pmc@d8130000 {
			compatible = "via,vt8500-pmc";
			reg = <0xd8130000 0x1000>;
			clocks {
				#address-cells = <1>;
				#size-cells = <0>;

				ref24: ref24M {
					#clock-cells = <0>;
					compatible = "fixed-clock";
					clock-frequency = <24000000>;
				};

				ref25: ref25M {
					#clock-cells = <0>;
					compatible = "fixed-clock";
					clock-frequency = <25000000>;
				};

				plla: plla {
					#clock-cells = <0>;
					compatible = "via,vt8500-pll-clock";
					clocks = <&ref25>;
					reg = <0x200>;
				};

				pllb: pllb {
					#clock-cells = <0>;
					compatible = "via,vt8500-pll-clock";
					clocks = <&ref25>;
					reg = <0x204>;
				};

				pllc: pllc {
					#clock-cells = <0>;
					compatible = "via,vt8500-pll-clock";
					clocks = <&ref25>;
					reg = <0x208>;
				};

				plld: plld {
					#clock-cells = <0>;
					compatible = "via,vt8500-pll-clock";
					clocks = <&ref25>;
					reg = <0x20c>;
				};

				clkarm: arm {
					#clock-cells = <0>;
					compatible = "via,vt8500-device-clock";
					clocks = <&plla>;
					divisor-reg = <0x300>;
				};

				clkahb: ahb {
					#clock-cells = <0>;
					compatible = "via,vt8500-device-clock";
					clocks = <&pllb>;
					divisor-reg = <0x304>;
				};

				clkapb: apb {
					#clock-cells = <0>;
					compatible = "via,vt8500-device-clock";
					clocks = <&pllb>;
					divisor-reg = <0x350>;
				};

				clkddr: ddr {
					#clock-cells = <0>;
					compatible = "via,vt8500-device-clock";
					clocks = <&plld>;
					divisor-reg = <0x310>;
				};

				clkuart0: uart0 {
					#clock-cells = <0>;
					compatible = "via,vt8500-device-clock";
					clocks = <&ref24>;
					enable-reg = <0x250>;
					enable-bit = <1>;
				};

				clkuart1: uart1 {
					#clock-cells = <0>;
					compatible = "via,vt8500-device-clock";
					clocks = <&ref24>;
					enable-reg = <0x250>;
					enable-bit = <2>;
				};

				clkuart2: uart2 {
					#clock-cells = <0>;
					compatible = "via,vt8500-device-clock";
					clocks = <&ref24>;
					enable-reg = <0x250>;
					enable-bit = <3>;
				};

				clkuart3: uart3 {
					#clock-cells = <0>;
					compatible = "via,vt8500-device-clock";
					clocks = <&ref24>;
					enable-reg = <0x250>;
					enable-bit = <4>;
				};

				clkuart4: uart4 {
					#clock-cells = <0>;
					compatible = "via,vt8500-device-clock";
					clocks = <&ref24>;
					enable-reg = <0x250>;
					enable-bit = <22>;
				};

				clkuart5: uart5 {
					#clock-cells = <0>;
					compatible = "via,vt8500-device-clock";
					clocks = <&ref24>;
					enable-reg = <0x250>;
					enable-bit = <23>;
				};

				clksdhc: sdhc {
					#clock-cells = <0>;
					compatible = "via,vt8500-device-clock";
					clocks = <&pllb>;
					divisor-reg = <0x328>;
					divisor-mask = <0x3f>;
					enable-reg = <0x254>;
					enable-bit = <18>;
				};
			};
		};

		timer@d8130100 {
			compatible = "via,vt8500-timer";
			reg = <0xd8130100 0x28>;
			interrupts = <36>;
		};

		ehci@d8007100 {
			compatible = "via,vt8500-ehci";
			reg = <0xd8007100 0x200>;
			interrupts = <1>;
		};

		uhci@d8007300 {
			compatible = "platform-uhci";
			reg = <0xd8007300 0x200>;
			interrupts = <0>;
		};

		fb: fb@d8050800 {
			compatible = "wm,wm8505-fb";
			reg = <0xd8050800 0x200>;
		};

		ge_rops@d8050400 {
			compatible = "wm,prizm-ge-rops";
			reg = <0xd8050400 0x100>;
		};

		uart0: serial@d8200000 {
			compatible = "via,vt8500-uart";
			reg = <0xd8200000 0x1040>;
			interrupts = <32>;
			clocks = <&clkuart0>;
			status = "disabled";
		};

		uart1: serial@d82b0000 {
			compatible = "via,vt8500-uart";
			reg = <0xd82b0000 0x1040>;
			interrupts = <33>;
			clocks = <&clkuart1>;
			status = "disabled";
		};

		uart2: serial@d8210000 {
			compatible = "via,vt8500-uart";
			reg = <0xd8210000 0x1040>;
			interrupts = <47>;
			clocks = <&clkuart2>;
			status = "disabled";
		};

		uart3: serial@d82c0000 {
			compatible = "via,vt8500-uart";
			reg = <0xd82c0000 0x1040>;
			interrupts = <50>;
			clocks = <&clkuart3>;
			status = "disabled";
		};

		uart4: serial@d8370000 {
			compatible = "via,vt8500-uart";
			reg = <0xd8370000 0x1040>;
			interrupts = <31>;
			clocks = <&clkuart4>;
			status = "disabled";
		};

		uart5: serial@d8380000 {
			compatible = "via,vt8500-uart";
			reg = <0xd8380000 0x1040>;
			interrupts = <30>;
			clocks = <&clkuart5>;
			status = "disabled";
		};

		rtc@d8100000 {
			compatible = "via,vt8500-rtc";
			reg = <0xd8100000 0x10000>;
			interrupts = <48>;
		};

		sdhc@d800a000 {
			compatible = "wm,wm8505-sdhc";
			reg = <0xd800a000 0x1000>;
			interrupts = <20 21>;
			clocks = <&clksdhc>;
			bus-width = <4>;
		};
	};
};
