/*
 * Samsung's Exynos5420 based Arndale Octa board device tree source
 *
 * Copyright (c) 2013 Samsung Electronics Co., Ltd.
 *		http://www.samsung.com
 *
 * This program is free software; you can redistribute it and/or modify
 * it under the terms of the GNU General Public License version 2 as
 * published by the Free Software Foundation.
*/

/dts-v1/;
#include "exynos5420.dtsi"
#include <dt-bindings/interrupt-controller/irq.h>
#include <dt-bindings/input/input.h>

/ {
	model = "Insignal Arndale Octa evaluation board based on EXYNOS5420";
	compatible = "insignal,arndale-octa", "samsung,exynos5420", "samsung,exynos5";

	memory {
		reg = <0x20000000 0x80000000>;
	};

	chosen {
		bootargs = "console=ttySAC3,115200";
	};

	firmware@02073000 {
		compatible = "samsung,secure-firmware";
		reg = <0x02073000 0x1000>;
	};

	fixed-rate-clocks {
		oscclk {
			compatible = "samsung,exynos5420-oscclk";
			clock-frequency = <24000000>;
		};
	};

	rtc@101E0000 {
		status = "okay";
	};

	codec@11000000 {
		samsung,mfc-r = <0x43000000 0x800000>;
		samsung,mfc-l = <0x51000000 0x800000>;
	};

	mmc@12200000 {
		status = "okay";
		broken-cd;
		supports-highspeed;
		card-detect-delay = <200>;
		samsung,dw-mshc-ciu-div = <3>;
		samsung,dw-mshc-sdr-timing = <0 4>;
		samsung,dw-mshc-ddr-timing = <0 2>;
		pinctrl-names = "default";
		pinctrl-0 = <&sd0_clk &sd0_cmd &sd0_bus4 &sd0_bus8>;
		vmmc-supply = <&ldo10_reg>;

		slot@0 {
			reg = <0>;
			bus-width = <8>;
		};
	};

	mmc@12220000 {
		status = "okay";
		supports-highspeed;
		card-detect-delay = <200>;
		samsung,dw-mshc-ciu-div = <3>;
		samsung,dw-mshc-sdr-timing = <2 3>;
		samsung,dw-mshc-ddr-timing = <1 2>;
		pinctrl-names = "default";
		pinctrl-0 = <&sd2_clk &sd2_cmd &sd2_cd &sd2_bus4>;
		vmmc-supply = <&ldo10_reg>;

		slot@0 {
			reg = <0>;
			bus-width = <4>;
		};
	};

	hsi2c_4: i2c@12CA0000 {
		status = "okay";

		s2mps11_pmic@66 {
			compatible = "samsung,s2mps11-pmic";
			reg = <0x66>;
			s2mps11,buck2-ramp-delay = <12>;
			s2mps11,buck34-ramp-delay = <12>;
			s2mps11,buck16-ramp-delay = <12>;
			s2mps11,buck6-ramp-enable = <1>;
			s2mps11,buck2-ramp-enable = <1>;
			s2mps11,buck3-ramp-enable = <1>;
			s2mps11,buck4-ramp-enable = <1>;

			interrupt-parent = <&gpx3>;
			interrupts = <2 IRQ_TYPE_LEVEL_HIGH>;

			s2mps11_osc: clocks {
				#clock-cells = <1>;
				clock-output-names = "s2mps11_ap",
						"s2mps11_cp", "s2mps11_bt";
			};

			regulators {
				ldo1_reg: LDO1 {
					regulator-name = "PVDD_ALIVE_1V0";
					regulator-min-microvolt = <1000000>;
					regulator-max-microvolt = <1000000>;
					regulator-always-on;
				};

				ldo2_reg: LDO2 {
					regulator-name = "PVDD_APIO_1V8";
					regulator-min-microvolt = <1800000>;
					regulator-max-microvolt = <1800000>;
				};

				ldo3_reg: LDO3 {
					regulator-name = "PVDD_APIO_MMCON_1V8";
					regulator-min-microvolt = <1800000>;
					regulator-max-microvolt = <1800000>;
					regulator-always-on;
				};

				ldo4_reg: LDO4 {
					regulator-name = "PVDD_ADC_1V8";
					regulator-min-microvolt = <1800000>;
					regulator-max-microvolt = <1800000>;
				};

				ldo5_reg: LDO5 {
					regulator-name = "PVDD_PLL_1V8";
					regulator-min-microvolt = <1800000>;
					regulator-max-microvolt = <1800000>;
					regulator-always-on;
				};

				ldo6_reg: LDO6 {
					regulator-name = "PVDD_ANAIP_1V0";
					regulator-min-microvolt = <1000000>;
					regulator-max-microvolt = <1000000>;
				};

				ldo7_reg: LDO7 {
					regulator-name = "PVDD_ANAIP_1V8";
					regulator-min-microvolt = <1800000>;
					regulator-max-microvolt = <1800000>;
				};

				ldo8_reg: LDO8 {
					regulator-name = "PVDD_ABB_1V8";
					regulator-min-microvolt = <1800000>;
					regulator-max-microvolt = <1800000>;
				};

				ldo9_reg: LDO9 {
					regulator-name = "PVDD_USB_3V3";
					regulator-min-microvolt = <3000000>;
					regulator-max-microvolt = <3000000>;
					regulator-always-on;
				};

				ldo10_reg: LDO10 {
					regulator-name = "PVDD_PRE_1V8";
					regulator-min-microvolt = <1800000>;
					regulator-max-microvolt = <1800000>;
					regulator-always-on;
				};

				ldo11_reg: LDO11 {
					regulator-name = "PVDD_USB_1V0";
					regulator-min-microvolt = <1000000>;
					regulator-max-microvolt = <1000000>;
					regulator-always-on;
				};

				ldo12_reg: LDO12 {
					regulator-name = "PVDD_HSIC_1V8";
					regulator-min-microvolt = <1800000>;
					regulator-max-microvolt = <1800000>;
				};

				ldo13_reg: LDO13 {
					regulator-name = "PVDD_APIO_MMCOFF_2V8";
					regulator-min-microvolt = <2800000>;
					regulator-max-microvolt = <2800000>;
				};

				ldo15_reg: LDO15 {
					regulator-name = "PVDD_PERI_2V8";
					regulator-min-microvolt = <3300000>;
					regulator-max-microvolt = <3300000>;
				};

				ldo16_reg: LDO16 {
					regulator-name = "PVDD_PERI_3V3";
					regulator-min-microvolt = <2200000>;
					regulator-max-microvolt = <2200000>;
				};

				ldo18_reg: LDO18 {
					regulator-name = "PVDD_EMMC_1V8";
					regulator-min-microvolt = <1800000>;
					regulator-max-microvolt = <1800000>;
				};

				ldo19_reg: LDO19 {
					regulator-name = "PVDD_TFLASH_2V8";
					regulator-min-microvolt = <2800000>;
					regulator-max-microvolt = <2800000>;
				};

				ldo20_reg: LDO20 {
					regulator-name = "PVDD_BTWIFI_1V8";
					regulator-min-microvolt = <1800000>;
					regulator-max-microvolt = <1800000>;
				};

				ldo21_reg: LDO21 {
					regulator-name = "PVDD_CAM1IO_1V8";
					regulator-min-microvolt = <1800000>;
					regulator-max-microvolt = <1800000>;
				};

				ldo23_reg: LDO23 {
					regulator-name = "PVDD_MIFS_1V1";
					regulator-min-microvolt = <1200000>;
					regulator-max-microvolt = <1200000>;
					regulator-always-on;
				};

				ldo24_reg: LDO24 {
					regulator-name = "PVDD_CAM1_AVDD_2V8";
					regulator-min-microvolt = <2800000>;
					regulator-max-microvolt = <2800000>;
				};

				ldo26_reg: LDO26 {
					regulator-name = "PVDD_CAM0_AF_2V8";
					regulator-min-microvolt = <3000000>;
					regulator-max-microvolt = <3000000>;
				};

				ldo27_reg: LDO27 {
					regulator-name = "PVDD_G3DS_1V0";
					regulator-min-microvolt = <1200000>;
					regulator-max-microvolt = <1200000>;
				};

				ldo28_reg: LDO28 {
					regulator-name = "PVDD_TSP_3V3";
					regulator-min-microvolt = <3300000>;
					regulator-max-microvolt = <3300000>;
				};

				ldo29_reg: LDO29 {
					regulator-name = "PVDD_AUDIO_1V8";
					regulator-min-microvolt = <1800000>;
					regulator-max-microvolt = <1800000>;
				};

				ldo31_reg: LDO31 {
					regulator-name = "PVDD_PERI_1V8";
					regulator-min-microvolt = <1800000>;
					regulator-max-microvolt = <1800000>;
				};

				ldo32_reg: LDO32 {
					regulator-name = "PVDD_LCD_1V8";
					regulator-min-microvolt = <1800000>;
					regulator-max-microvolt = <1800000>;
				};

				ldo33_reg: LDO33 {
					regulator-name = "PVDD_CAM0IO_1V8";
					regulator-min-microvolt = <1800000>;
					regulator-max-microvolt = <1800000>;
				};

				ldo35_reg: LDO35 {
					regulator-name = "PVDD_CAM0_DVDD_1V2";
					regulator-min-microvolt = <1200000>;
					regulator-max-microvolt = <1200000>;
				};

				ldo38_reg: LDO38 {
					regulator-name = "PVDD_CAM0_AVDD_2V8";
					regulator-min-microvolt = <2800000>;
					regulator-max-microvolt = <2800000>;
				};

				buck1_reg: BUCK1 {
					regulator-name = "PVDD_MIF_1V1";
					regulator-min-microvolt = <800000>;
					regulator-max-microvolt = <1100000>;
					regulator-always-on;
				};

				buck2_reg: BUCK2 {
					regulator-name = "vdd_arm";
					regulator-min-microvolt = <800000>;
					regulator-max-microvolt = <1000000>;
					regulator-always-on;
				};

				buck3_reg: BUCK3 {
					regulator-name = "PVDD_INT_1V0";
					regulator-min-microvolt = <800000>;
					regulator-max-microvolt = <1000000>;
					regulator-always-on;
				};

				buck4_reg: BUCK4 {
					regulator-name = "PVDD_G3D_1V0";
					regulator-min-microvolt = <800000>;
					regulator-max-microvolt = <1000000>;
				};

				buck5_reg: BUCK5 {
					regulator-name = "PVDD_LPDDR3_1V2";
					regulator-min-microvolt = <800000>;
					regulator-max-microvolt = <1200000>;
					regulator-always-on;
				};

				buck6_reg: BUCK6 {
					regulator-name = "PVDD_KFC_1V0";
					regulator-min-microvolt = <800000>;
					regulator-max-microvolt = <1000000>;
					regulator-always-on;
				};

				buck7_reg: BUCK7 {
					regulator-name = "VIN_LLDO_1V4";
					regulator-min-microvolt = <800000>;
					regulator-max-microvolt = <1400000>;
					regulator-always-on;
				};

				buck8_reg: BUCK8 {
					regulator-name = "VIN_MLDO_2V0";
					regulator-min-microvolt = <800000>;
					regulator-max-microvolt = <2000000>;
					regulator-always-on;
				};

				buck9_reg: BUCK9 {
					regulator-name = "VIN_HLDO_3V5";
					regulator-min-microvolt = <3000000>;
					regulator-max-microvolt = <3500000>;
					regulator-always-on;
				};

				buck10_reg: BUCK10 {
					regulator-name = "PVDD_EMMCF_2V8";
					regulator-min-microvolt = <2800000>;
					regulator-max-microvolt = <2800000>;
				};
			};
		};
	};

	gpio_keys {
		compatible = "gpio-keys";

		wakeup {
			label = "SW-TACT1";
			gpios = <&gpx2 7 1>;
			linux,code = <KEY_WAKEUP>;
			gpio-key,wakeup;
		};
	};
};
