/*
 * Device Tree Source for the r8a73a4 SoC
 *
 * Copyright (C) 2013 Renesas Solutions Corp.
 * Copyright (C) 2013 Magnus Damm
 *
 * This file is licensed under the terms of the GNU General Public License
 * version 2.  This program is licensed "as is" without any warranty of any
 * kind, whether express or implied.
 */

#include <dt-bindings/interrupt-controller/arm-gic.h>
#include <dt-bindings/interrupt-controller/irq.h>

/ {
	compatible = "renesas,r8a73a4";
	interrupt-parent = <&gic>;
	#address-cells = <2>;
	#size-cells = <2>;

	cpus {
		#address-cells = <1>;
		#size-cells = <0>;

		cpu0: cpu@0 {
			device_type = "cpu";
			compatible = "arm,cortex-a15";
			reg = <0>;
			clock-frequency = <1500000000>;
		};
	};

	gic: interrupt-controller@f1001000 {
		compatible = "arm,cortex-a15-gic";
		#interrupt-cells = <3>;
		#address-cells = <0>;
		interrupt-controller;
		reg = <0 0xf1001000 0 0x1000>,
			<0 0xf1002000 0 0x1000>,
			<0 0xf1004000 0 0x2000>,
			<0 0xf1006000 0 0x2000>;
		interrupts = <1 9 (GIC_CPU_MASK_SIMPLE(4) | IRQ_TYPE_LEVEL_HIGH)>;
	};

	timer {
		compatible = "arm,armv7-timer";
		interrupts = <1 13 (GIC_CPU_MASK_SIMPLE(4) | IRQ_TYPE_LEVEL_LOW)>,
			     <1 14 (GIC_CPU_MASK_SIMPLE(4) | IRQ_TYPE_LEVEL_LOW)>,
			     <1 11 (GIC_CPU_MASK_SIMPLE(4) | IRQ_TYPE_LEVEL_LOW)>,
			     <1 10 (GIC_CPU_MASK_SIMPLE(4) | IRQ_TYPE_LEVEL_LOW)>;
	};

	irqc0: interrupt-controller@e61c0000 {
		compatible = "renesas,irqc";
		#interrupt-cells = <2>;
		interrupt-controller;
		reg = <0 0xe61c0000 0 0x200>;
		interrupts = <0 0 IRQ_TYPE_LEVEL_HIGH>,
			     <0 1 IRQ_TYPE_LEVEL_HIGH>,
			     <0 2 IRQ_TYPE_LEVEL_HIGH>,
			     <0 3 IRQ_TYPE_LEVEL_HIGH>,
			     <0 4 IRQ_TYPE_LEVEL_HIGH>,
			     <0 5 IRQ_TYPE_LEVEL_HIGH>,
			     <0 6 IRQ_TYPE_LEVEL_HIGH>,
			     <0 7 IRQ_TYPE_LEVEL_HIGH>,
			     <0 8 IRQ_TYPE_LEVEL_HIGH>,
			     <0 9 IRQ_TYPE_LEVEL_HIGH>,
			     <0 10 IRQ_TYPE_LEVEL_HIGH>,
			     <0 11 IRQ_TYPE_LEVEL_HIGH>,
			     <0 12 IRQ_TYPE_LEVEL_HIGH>,
			     <0 13 IRQ_TYPE_LEVEL_HIGH>,
			     <0 14 IRQ_TYPE_LEVEL_HIGH>,
			     <0 15 IRQ_TYPE_LEVEL_HIGH>,
			     <0 16 IRQ_TYPE_LEVEL_HIGH>,
			     <0 17 IRQ_TYPE_LEVEL_HIGH>,
			     <0 18 IRQ_TYPE_LEVEL_HIGH>,
			     <0 19 IRQ_TYPE_LEVEL_HIGH>,
			     <0 20 IRQ_TYPE_LEVEL_HIGH>,
			     <0 21 IRQ_TYPE_LEVEL_HIGH>,
			     <0 22 IRQ_TYPE_LEVEL_HIGH>,
			     <0 23 IRQ_TYPE_LEVEL_HIGH>,
			     <0 24 IRQ_TYPE_LEVEL_HIGH>,
			     <0 25 IRQ_TYPE_LEVEL_HIGH>,
			     <0 26 IRQ_TYPE_LEVEL_HIGH>,
			     <0 27 IRQ_TYPE_LEVEL_HIGH>,
			     <0 28 IRQ_TYPE_LEVEL_HIGH>,
			     <0 29 IRQ_TYPE_LEVEL_HIGH>,
			     <0 30 IRQ_TYPE_LEVEL_HIGH>,
			     <0 31 IRQ_TYPE_LEVEL_HIGH>;
	};

	irqc1: interrupt-controller@e61c0200 {
		compatible = "renesas,irqc";
		#interrupt-cells = <2>;
		interrupt-controller;
		reg = <0 0xe61c0200 0 0x200>;
		interrupts = <0 32 IRQ_TYPE_LEVEL_HIGH>,
			     <0 33 IRQ_TYPE_LEVEL_HIGH>,
			     <0 34 IRQ_TYPE_LEVEL_HIGH>,
			     <0 35 IRQ_TYPE_LEVEL_HIGH>,
			     <0 36 IRQ_TYPE_LEVEL_HIGH>,
			     <0 37 IRQ_TYPE_LEVEL_HIGH>,
			     <0 38 IRQ_TYPE_LEVEL_HIGH>,
			     <0 39 IRQ_TYPE_LEVEL_HIGH>,
			     <0 40 IRQ_TYPE_LEVEL_HIGH>,
			     <0 41 IRQ_TYPE_LEVEL_HIGH>,
			     <0 42 IRQ_TYPE_LEVEL_HIGH>,
			     <0 43 IRQ_TYPE_LEVEL_HIGH>,
			     <0 44 IRQ_TYPE_LEVEL_HIGH>,
			     <0 45 IRQ_TYPE_LEVEL_HIGH>,
			     <0 46 IRQ_TYPE_LEVEL_HIGH>,
			     <0 47 IRQ_TYPE_LEVEL_HIGH>,
			     <0 48 IRQ_TYPE_LEVEL_HIGH>,
			     <0 49 IRQ_TYPE_LEVEL_HIGH>,
			     <0 50 IRQ_TYPE_LEVEL_HIGH>,
			     <0 51 IRQ_TYPE_LEVEL_HIGH>,
			     <0 52 IRQ_TYPE_LEVEL_HIGH>,
			     <0 53 IRQ_TYPE_LEVEL_HIGH>,
			     <0 54 IRQ_TYPE_LEVEL_HIGH>,
			     <0 55 IRQ_TYPE_LEVEL_HIGH>,
			     <0 56 IRQ_TYPE_LEVEL_HIGH>,
			     <0 57 IRQ_TYPE_LEVEL_HIGH>;
	};

	dmac: dma-multiplexer@0 {
		compatible = "renesas,shdma-mux";
		#dma-cells = <1>;
		dma-channels = <20>;
		dma-requests = <256>;
		#address-cells = <2>;
		#size-cells = <2>;
		ranges;

		dma0: dma-controller@e6700020 {
			compatible = "renesas,shdma-r8a73a4";
			reg = <0 0xe6700020 0 0x89e0>;
			interrupts = <0 220 IRQ_TYPE_LEVEL_HIGH
					0 200 IRQ_TYPE_LEVEL_HIGH
					0 201 IRQ_TYPE_LEVEL_HIGH
					0 202 IRQ_TYPE_LEVEL_HIGH
					0 203 IRQ_TYPE_LEVEL_HIGH
					0 204 IRQ_TYPE_LEVEL_HIGH
					0 205 IRQ_TYPE_LEVEL_HIGH
					0 206 IRQ_TYPE_LEVEL_HIGH
					0 207 IRQ_TYPE_LEVEL_HIGH
					0 208 IRQ_TYPE_LEVEL_HIGH
					0 209 IRQ_TYPE_LEVEL_HIGH
					0 210 IRQ_TYPE_LEVEL_HIGH
					0 211 IRQ_TYPE_LEVEL_HIGH
					0 212 IRQ_TYPE_LEVEL_HIGH
					0 213 IRQ_TYPE_LEVEL_HIGH
					0 214 IRQ_TYPE_LEVEL_HIGH
					0 215 IRQ_TYPE_LEVEL_HIGH
					0 216 IRQ_TYPE_LEVEL_HIGH
					0 217 IRQ_TYPE_LEVEL_HIGH
					0 218 IRQ_TYPE_LEVEL_HIGH
					0 219 IRQ_TYPE_LEVEL_HIGH>;
			interrupt-names = "error",
					"ch0", "ch1", "ch2", "ch3",
					"ch4", "ch5", "ch6", "ch7",
					"ch8", "ch9", "ch10", "ch11",
					"ch12", "ch13", "ch14", "ch15",
					"ch16", "ch17", "ch18", "ch19";
		};
	};

	thermal@e61f0000 {
		compatible = "renesas,rcar-thermal";
		reg = <0 0xe61f0000 0 0x14>, <0 0xe61f0100 0 0x38>,
			 <0 0xe61f0200 0 0x38>, <0 0xe61f0300 0 0x38>;
		interrupts = <0 69 IRQ_TYPE_LEVEL_HIGH>;
	};

	i2c0: i2c@e6500000 {
		#address-cells = <1>;
		#size-cells = <0>;
		compatible = "renesas,rmobile-iic";
		reg = <0 0xe6500000 0 0x428>;
		interrupts = <0 174 IRQ_TYPE_LEVEL_HIGH>;
		status = "disabled";
	};

	i2c1: i2c@e6510000 {
		#address-cells = <1>;
		#size-cells = <0>;
		compatible = "renesas,rmobile-iic";
		reg = <0 0xe6510000 0 0x428>;
		interrupts = <0 175 IRQ_TYPE_LEVEL_HIGH>;
		status = "disabled";
	};

	i2c2: i2c@e6520000 {
		#address-cells = <1>;
		#size-cells = <0>;
		compatible = "renesas,rmobile-iic";
		reg = <0 0xe6520000 0 0x428>;
		interrupts = <0 176 IRQ_TYPE_LEVEL_HIGH>;
		status = "disabled";
	};

	i2c3: i2c@e6530000 {
		#address-cells = <1>;
		#size-cells = <0>;
		compatible = "renesas,rmobile-iic";
		reg = <0 0xe6530000 0 0x428>;
		interrupts = <0 177 IRQ_TYPE_LEVEL_HIGH>;
		status = "disabled";
	};

	i2c4: i2c@e6540000 {
		#address-cells = <1>;
		#size-cells = <0>;
		compatible = "renesas,rmobile-iic";
		reg = <0 0xe6540000 0 0x428>;
		interrupts = <0 178 IRQ_TYPE_LEVEL_HIGH>;
		status = "disabled";
	};

	i2c5: i2c@e60b0000 {
		#address-cells = <1>;
		#size-cells = <0>;
		compatible = "renesas,rmobile-iic";
		reg = <0 0xe60b0000 0 0x428>;
		interrupts = <0 179 IRQ_TYPE_LEVEL_HIGH>;
		status = "disabled";
	};

	i2c6: i2c@e6550000 {
		#address-cells = <1>;
		#size-cells = <0>;
		compatible = "renesas,rmobile-iic";
		reg = <0 0xe6550000 0 0x428>;
		interrupts = <0 184 IRQ_TYPE_LEVEL_HIGH>;
		status = "disabled";
	};

	i2c7: i2c@e6560000 {
		#address-cells = <1>;
		#size-cells = <0>;
		compatible = "renesas,rmobile-iic";
		reg = <0 0xe6560000 0 0x428>;
		interrupts = <0 185 IRQ_TYPE_LEVEL_HIGH>;
		status = "disabled";
	};

	i2c8: i2c@e6570000 {
		#address-cells = <1>;
		#size-cells = <0>;
		compatible = "renesas,rmobile-iic";
		reg = <0 0xe6570000 0 0x428>;
		interrupts = <0 173 IRQ_TYPE_LEVEL_HIGH>;
		status = "disabled";
	};

	mmcif0: mmc@ee200000 {
		compatible = "renesas,sh-mmcif";
		reg = <0 0xee200000 0 0x80>;
		interrupts = <0 169 IRQ_TYPE_LEVEL_HIGH>;
		reg-io-width = <4>;
		status = "disabled";
	};

	mmcif1: mmc@ee220000 {
		compatible = "renesas,sh-mmcif";
		reg = <0 0xee220000 0 0x80>;
		interrupts = <0 170 IRQ_TYPE_LEVEL_HIGH>;
		reg-io-width = <4>;
		status = "disabled";
	};

	pfc: pfc@e6050000 {
		compatible = "renesas,pfc-r8a73a4";
		reg = <0 0xe6050000 0 0x9000>;
		gpio-controller;
		#gpio-cells = <2>;
		interrupts-extended =
			<&irqc0  0 0>, <&irqc0  1 0>, <&irqc0  2 0>, <&irqc0  3 0>,
			<&irqc0  4 0>, <&irqc0  5 0>, <&irqc0  6 0>, <&irqc0  7 0>,
			<&irqc0  8 0>, <&irqc0  9 0>, <&irqc0 10 0>, <&irqc0 11 0>,
			<&irqc0 12 0>, <&irqc0 13 0>, <&irqc0 14 0>, <&irqc0 15 0>,
			<&irqc0 16 0>, <&irqc0 17 0>, <&irqc0 18 0>, <&irqc0 19 0>,
			<&irqc0 20 0>, <&irqc0 21 0>, <&irqc0 22 0>, <&irqc0 23 0>,
			<&irqc0 24 0>, <&irqc0 25 0>, <&irqc0 26 0>, <&irqc0 27 0>,
			<&irqc0 28 0>, <&irqc0 29 0>, <&irqc0 30 0>, <&irqc0 31 0>,
			<&irqc1  0 0>, <&irqc1  1 0>, <&irqc1  2 0>, <&irqc1  3 0>,
			<&irqc1  4 0>, <&irqc1  5 0>, <&irqc1  6 0>, <&irqc1  7 0>,
			<&irqc1  8 0>, <&irqc1  9 0>, <&irqc1 10 0>, <&irqc1 11 0>,
			<&irqc1 12 0>, <&irqc1 13 0>, <&irqc1 14 0>, <&irqc1 15 0>,
			<&irqc1 16 0>, <&irqc1 17 0>, <&irqc1 18 0>, <&irqc1 19 0>,
			<&irqc1 20 0>, <&irqc1 21 0>, <&irqc1 22 0>, <&irqc1 23 0>,
			<&irqc1 24 0>, <&irqc1 25 0>;
	};

	sdhi0: sd@ee100000 {
		compatible = "renesas,sdhi-r8a73a4";
		reg = <0 0xee100000 0 0x100>;
		interrupts = <0 165 IRQ_TYPE_LEVEL_HIGH>;
		cap-sd-highspeed;
		status = "disabled";
	};

	sdhi1: sd@ee120000 {
		compatible = "renesas,sdhi-r8a73a4";
		reg = <0 0xee120000 0 0x100>;
		interrupts = <0 166 IRQ_TYPE_LEVEL_HIGH>;
		cap-sd-highspeed;
		status = "disabled";
	};

	sdhi2: sd@ee140000 {
		compatible = "renesas,sdhi-r8a73a4";
		reg = <0 0xee140000 0 0x100>;
		interrupts = <0 167 IRQ_TYPE_LEVEL_HIGH>;
		cap-sd-highspeed;
		status = "disabled";
	};
};
