/*
 * MPC8360E RDK Device Tree Source
 *
 * Copyright 2006 Freescale Semiconductor Inc.
 * Copyright 2007-2008 MontaVista Software, Inc.
 *
 * Author: Anton Vorontsov <avorontsov@ru.mvista.com>
 *
 * This program is free software; you can redistribute  it and/or modify it
 * under  the terms of  the GNU General  Public License as published by the
 * Free Software Foundation;  either version 2 of the  License, or (at your
 * option) any later version.
 */

/dts-v1/;

/ {
	#address-cells = <1>;
	#size-cells = <1>;
	compatible = "fsl,mpc8360rdk";

	aliases {
		serial0 = &serial0;
		serial1 = &serial1;
		serial2 = &serial2;
		serial3 = &serial3;
		ethernet0 = &enet0;
		ethernet1 = &enet1;
		ethernet2 = &enet2;
		ethernet3 = &enet3;
		pci0 = &pci0;
	};

	cpus {
		#address-cells = <1>;
		#size-cells = <0>;

		PowerPC,8360@0 {
			device_type = "cpu";
			reg = <0>;
			d-cache-line-size = <32>;
			i-cache-line-size = <32>;
			d-cache-size = <32768>;
			i-cache-size = <32768>;
			/* filled by u-boot */
			timebase-frequency = <0>;
			bus-frequency = <0>;
			clock-frequency = <0>;
		};
	};

	memory {
		device_type = "memory";
		/* filled by u-boot */
		reg = <0 0>;
	};

	soc@e0000000 {
		#address-cells = <1>;
		#size-cells = <1>;
		device_type = "soc";
		compatible = "fsl,mpc8360-immr", "fsl,immr", "fsl,soc",
			     "simple-bus";
		ranges = <0 0xe0000000 0x200000>;
		reg = <0xe0000000 0x200>;
		/* filled by u-boot */
		bus-frequency = <0>;

		wdt@200 {
			compatible = "mpc83xx_wdt";
			reg = <0x200 0x100>;
		};

		pmc: power@b00 {
			compatible = "fsl,mpc8360-pmc", "fsl,mpc8349-pmc";
			reg = <0xb00 0x100 0xa00 0x100>;
			interrupts = <80 0x8>;
			interrupt-parent = <&ipic>;
		};

		i2c@3000 {
			#address-cells = <1>;
			#size-cells = <0>;
			cell-index = <0>;
			compatible = "fsl-i2c";
			reg = <0x3000 0x100>;
			interrupts = <14 8>;
			interrupt-parent = <&ipic>;
			dfsrr;
		};

		i2c@3100 {
			#address-cells = <1>;
			#size-cells = <0>;
			cell-index = <1>;
			compatible = "fsl-i2c";
			reg = <0x3100 0x100>;
			interrupts = <16 8>;
			interrupt-parent = <&ipic>;
			dfsrr;
		};

		serial0: serial@4500 {
			device_type = "serial";
			compatible = "fsl,ns16550", "ns16550";
			reg = <0x4500 0x100>;
			interrupts = <9 8>;
			interrupt-parent = <&ipic>;
			/* filled by u-boot */
			clock-frequency = <0>;
		};

		serial1: serial@4600 {
			device_type = "serial";
			compatible = "fsl,ns16550", "ns16550";
			reg = <0x4600 0x100>;
			interrupts = <10 8>;
			interrupt-parent = <&ipic>;
			/* filled by u-boot */
			clock-frequency = <0>;
		};

		dma@82a8 {
			#address-cells = <1>;
			#size-cells = <1>;
			compatible = "fsl,mpc8360-dma", "fsl,elo-dma";
			reg = <0x82a8 4>;
			ranges = <0 0x8100 0x1a8>;
			interrupt-parent = <&ipic>;
			interrupts = <71 8>;
			cell-index = <0>;
			dma-channel@0 {
				compatible = "fsl,mpc8360-dma-channel", "fsl,elo-dma-channel";
				reg = <0 0x80>;
				cell-index = <0>;
				interrupt-parent = <&ipic>;
				interrupts = <71 8>;
			};
			dma-channel@80 {
				compatible = "fsl,mpc8360-dma-channel", "fsl,elo-dma-channel";
				reg = <0x80 0x80>;
				cell-index = <1>;
				interrupt-parent = <&ipic>;
				interrupts = <71 8>;
			};
			dma-channel@100 {
				compatible = "fsl,mpc8360-dma-channel", "fsl,elo-dma-channel";
				reg = <0x100 0x80>;
				cell-index = <2>;
				interrupt-parent = <&ipic>;
				interrupts = <71 8>;
			};
			dma-channel@180 {
				compatible = "fsl,mpc8360-dma-channel", "fsl,elo-dma-channel";
				reg = <0x180 0x28>;
				cell-index = <3>;
				interrupt-parent = <&ipic>;
				interrupts = <71 8>;
			};
		};

		crypto@30000 {
			compatible = "fsl,sec2.0";
			reg = <0x30000 0x10000>;
			interrupts = <11 0x8>;
			interrupt-parent = <&ipic>;
			fsl,num-channels = <4>;
			fsl,channel-fifo-len = <24>;
			fsl,exec-units-mask = <0x7e>;
			fsl,descriptor-types-mask = <0x01010ebf>;
			sleep = <&pmc 0x03000000>;
		};

		ipic: interrupt-controller@700 {
			#address-cells = <0>;
			#interrupt-cells = <2>;
			compatible = "fsl,pq2pro-pic", "fsl,ipic";
			interrupt-controller;
			reg = <0x700 0x100>;
		};

		qe_pio_b: gpio-controller@1418 {
			#gpio-cells = <2>;
			compatible = "fsl,mpc8360-qe-pario-bank",
				     "fsl,mpc8323-qe-pario-bank";
			reg = <0x1418 0x18>;
			gpio-controller;
		};

		qe_pio_e: gpio-controller@1460 {
			#gpio-cells = <2>;
			compatible = "fsl,mpc8360-qe-pario-bank",
				     "fsl,mpc8323-qe-pario-bank";
			reg = <0x1460 0x18>;
			gpio-controller;
		};

		qe@100000 {
			#address-cells = <1>;
			#size-cells = <1>;
			device_type = "qe";
			compatible = "fsl,qe", "simple-bus";
			ranges = <0 0x100000 0x100000>;
			reg = <0x100000 0x480>;
			/* filled by u-boot */
			clock-frequency = <0>;
			bus-frequency = <0>;
			brg-frequency = <0>;
			fsl,qe-num-riscs = <2>;
			fsl,qe-num-snums = <28>;

			muram@10000 {
				#address-cells = <1>;
				#size-cells = <1>;
				compatible = "fsl,qe-muram", "fsl,cpm-muram";
				ranges = <0 0x10000 0xc000>;

				data-only@0 {
					compatible = "fsl,qe-muram-data",
						     "fsl,cpm-muram-data";
					reg = <0 0xc000>;
				};
			};

			timer@440 {
				compatible = "fsl,mpc8360-qe-gtm",
					     "fsl,qe-gtm", "fsl,gtm";
				reg = <0x440 0x40>;
				interrupts = <12 13 14 15>;
				interrupt-parent = <&qeic>;
				clock-frequency = <166666666>;
			};

			usb@6c0 {
				compatible = "fsl,mpc8360-qe-usb",
					     "fsl,mpc8323-qe-usb";
				reg = <0x6c0 0x40 0x8b00 0x100>;
				interrupts = <11>;
				interrupt-parent = <&qeic>;
				fsl,fullspeed-clock = "clk21";
				gpios = <&qe_pio_b  2 0 /* USBOE */
					 &qe_pio_b  3 0 /* USBTP */
					 &qe_pio_b  8 0 /* USBTN */
					 &qe_pio_b  9 0 /* USBRP */
					 &qe_pio_b 11 0 /* USBRN */
					 &qe_pio_e 20 0 /* SPEED */
					 &qe_pio_e 21 1 /* POWER */>;
			};

			spi@4c0 {
				cell-index = <0>;
				compatible = "fsl,spi";
				reg = <0x4c0 0x40>;
				interrupts = <2>;
				interrupt-parent = <&qeic>;
				mode = "cpu-qe";
			};

			spi@500 {
				cell-index = <1>;
				compatible = "fsl,spi";
				reg = <0x500 0x40>;
				interrupts = <1>;
				interrupt-parent = <&qeic>;
				mode = "cpu-qe";
			};

			enet0: ucc@2000 {
				device_type = "network";
				compatible = "ucc_geth";
				cell-index = <1>;
				reg = <0x2000 0x200>;
				interrupts = <32>;
				interrupt-parent = <&qeic>;
				rx-clock-name = "none";
				tx-clock-name = "clk9";
				phy-handle = <&phy2>;
				phy-connection-type = "rgmii-rxid";
				/* filled by u-boot */
				local-mac-address = [ 00 00 00 00 00 00 ];
			};

			enet1: ucc@3000 {
				device_type = "network";
				compatible = "ucc_geth";
				cell-index = <2>;
				reg = <0x3000 0x200>;
				interrupts = <33>;
				interrupt-parent = <&qeic>;
				rx-clock-name = "none";
				tx-clock-name = "clk4";
				phy-handle = <&phy4>;
				phy-connection-type = "rgmii-rxid";
				/* filled by u-boot */
				local-mac-address = [ 00 00 00 00 00 00 ];
			};

			enet2: ucc@2600 {
				device_type = "network";
				compatible = "ucc_geth";
				cell-index = <7>;
				reg = <0x2600 0x200>;
				interrupts = <42>;
				interrupt-parent = <&qeic>;
				rx-clock-name = "clk20";
				tx-clock-name = "clk19";
				phy-handle = <&phy1>;
				phy-connection-type = "mii";
				/* filled by u-boot */
				local-mac-address = [ 00 00 00 00 00 00 ];
			};

			enet3: ucc@3200 {
				device_type = "network";
				compatible = "ucc_geth";
				cell-index = <4>;
				reg = <0x3200 0x200>;
				interrupts = <35>;
				interrupt-parent = <&qeic>;
				rx-clock-name = "clk8";
				tx-clock-name = "clk7";
				phy-handle = <&phy3>;
				phy-connection-type = "mii";
				/* filled by u-boot */
				local-mac-address = [ 00 00 00 00 00 00 ];
			};

			mdio@2120 {
				#address-cells = <1>;
				#size-cells = <0>;
				compatible = "fsl,ucc-mdio";
				reg = <0x2120 0x18>;

				phy1: ethernet-phy@1 {
					compatible = "national,DP83848VV";
					reg = <1>;
				};

				phy2: ethernet-phy@2 {
					compatible = "broadcom,BCM5481UA2KMLG";
					reg = <2>;
				};

				phy3: ethernet-phy@3 {
					compatible = "national,DP83848VV";
					reg = <3>;
				};

				phy4: ethernet-phy@4 {
					compatible = "broadcom,BCM5481UA2KMLG";
					reg = <4>;
				};
			};

			serial2: ucc@2400 {
				device_type = "serial";
				compatible = "ucc_uart";
				reg = <0x2400 0x200>;
				cell-index = <5>;
				port-number = <0>;
				rx-clock-name = "brg7";
				tx-clock-name = "brg8";
				interrupts = <40>;
				interrupt-parent = <&qeic>;
				soft-uart;
			};

			serial3: ucc@3400 {
				device_type = "serial";
				compatible = "ucc_uart";
				reg = <0x3400 0x200>;
				cell-index = <6>;
				port-number = <1>;
				rx-clock-name = "brg13";
				tx-clock-name = "brg14";
				interrupts = <41>;
				interrupt-parent = <&qeic>;
				soft-uart;
			};

			qeic: interrupt-controller@80 {
				#address-cells = <0>;
				#interrupt-cells = <1>;
				compatible = "fsl,qe-ic";
				interrupt-controller;
				reg = <0x80 0x80>;
				big-endian;
				interrupts = <32 8 33 8>;
				interrupt-parent = <&ipic>;
			};
		};
	};

	localbus@e0005000 {
		#address-cells = <2>;
		#size-cells = <1>;
		compatible = "fsl,mpc8360-localbus", "fsl,pq2pro-localbus",
			     "simple-bus";
		reg = <0xe0005000 0xd8>;
		ranges = <0 0 0xff800000 0x0800000
			  1 0 0x60000000 0x0001000
			  2 0 0x70000000 0x4000000>;

		flash@0,0 {
			compatible = "intel,PC28F640P30T85", "cfi-flash";
			reg = <0 0 0x800000>;
			bank-width = <2>;
			device-width = <1>;
		};

		upm@1,0 {
			compatible = "fsl,upm-nand";
			reg = <1 0 1>;
			fsl,upm-addr-offset = <16>;
			fsl,upm-cmd-offset = <8>;
			gpios = <&qe_pio_e 18 0>;

			flash {
				compatible = "stm,nand512-a";
			};
		};

		display@2,0 {
			device_type = "display";
			compatible = "fujitsu,MB86277", "fujitsu,mint";
			reg = <2 0 0x4000000>;
			fujitsu,sh3;
			little-endian;
			/* filled by u-boot */
			address = <0>;
			depth = <0>;
			width = <0>;
			height = <0>;
			linebytes = <0>;
			/* linux,opened; - added by uboot */
		};
	};

	pci0: pci@e0008500 {
		#address-cells = <3>;
		#size-cells = <2>;
		#interrupt-cells = <1>;
		device_type = "pci";
		compatible = "fsl,mpc8360-pci", "fsl,mpc8349-pci";
		reg = <0xe0008500 0x100		/* internal registers */
		       0xe0008300 0x8>;		/* config space access registers */
		ranges = <0x02000000 0 0x90000000 0x90000000 0 0x10000000
			  0x42000000 0 0x80000000 0x80000000 0 0x10000000
			  0x01000000 0 0xe0300000 0xe0300000 0 0x00100000>;
		interrupts = <66 8>;
		interrupt-parent = <&ipic>;
		interrupt-map-mask = <0xf800 0 0 7>;
		interrupt-map = </* miniPCI0 IDSEL 0x14 AD20 */
				 0xa000 0 0 1 &ipic 18 8
				 0xa000 0 0 2 &ipic 19 8

				 /* PCI1 IDSEL 0x15 AD21 */
				 0xa800 0 0 1 &ipic 19 8
				 0xa800 0 0 2 &ipic 20 8
				 0xa800 0 0 3 &ipic 21 8
				 0xa800 0 0 4 &ipic 18 8>;
		sleep = <&pmc 0x00010000>;
		/* filled by u-boot */
		bus-range = <0 0>;
		clock-frequency = <0>;
	};
};
