/*
 * Copyright 2014 Raphaël Poggi
 * Copyright 2011 Freescale Semiconductor, Inc.
 * Copyright 2011 Linaro Ltd.
 *
 * The code contained herein is licensed under the GNU General Public
 * License. You may obtain a copy of the GNU General Public License
 * Version 2 or later at the following locations:
 *
 * http://www.opensource.org/licenses/gpl-license.html
 * http://www.gnu.org/copyleft/gpl.html
 */

#include <dt-bindings/gpio/gpio.h>
#include <dt-bindings/input/input.h>

/ {
	model = "Freescale i.MX6 UDOO Board";
	compatible = "udoo,imx6qdl-udoo", "fsl,imx6q";

	chosen {
		linux,stdout-path = &uart2;
	};

	memory {
		reg = <0x10000000 0x40000000>;
	};

	regulators {
		compatible = "simple-bus";
		#address-cells = <1>;
		#size-cells = <0>;

		reg_2p5v: regulator@0 {
			compatible = "regulator-fixed";
			reg = <0>;
			regulator-name = "2P5V";
			regulator-min-microvolt = <2500000>;
			regulator-max-microvolt = <2500000>;
			regulator-always-on;
		};

		reg_3p3v: regulator@1 {
			compatible = "regulator-fixed";
			reg = <1>;
			regulator-name = "3P3V";
			regulator-min-microvolt = <3300000>;
			regulator-max-microvolt = <3300000>;
			regulator-always-on;
		};

		reg_usb_otg_vbus: regulator@2 {
			compatible = "regulator-fixed";
			reg = <2>;
			regulator-name = "usb_otg_vbus";
			regulator-min-microvolt = <5000000>;
			regulator-max-microvolt = <5000000>;
			gpio = <&gpio3 22 GPIO_ACTIVE_HIGH>;
			enable-active-high;
		};
	};
};

&fec {
	pinctrl-names = "default";
	pinctrl-0 = <&pinctrl_enet>;
	phy-reset-gpios = <&gpio3 23 GPIO_ACTIVE_LOW>;
	status = "okay";
};

&i2c1 {
	clock-frequency = <100000>;
	pinctrl-names = "default";
	pinctrl-0 = <&pinctrl_i2c1>;
	status = "okay";
};

&iomuxc {
	pinctrl-names = "default";
	pinctrl-0 = <&pinctrl_hog>;

	imx6q-udoo {
		pinctrl_hog: hoggrp {
			fsl,pins = <
				/* SGTL5000 sys_mclk */
				MX6QDL_PAD_GPIO_0__CCM_CLKO1    0x030b0
			>;
		};

		pinctrl_enet: enetgrp {
			fsl,pins = <
				MX6QDL_PAD_RGMII_RXC__RGMII_RXC		0x1b0b0
				MX6QDL_PAD_RGMII_RD0__RGMII_RD0		0x1b0b0
				MX6QDL_PAD_RGMII_RD1__RGMII_RD1		0x1b0b0
				MX6QDL_PAD_RGMII_RD2__RGMII_RD2		0x1b0b0
				MX6QDL_PAD_RGMII_RD3__RGMII_RD3		0x1b0b0
				MX6QDL_PAD_RGMII_RX_CTL__RGMII_RX_CTL	0x1b0b0
				MX6QDL_PAD_RGMII_TXC__RGMII_TXC		0x1b0b0
				MX6QDL_PAD_RGMII_TD0__RGMII_TD0		0x1b0b0
				MX6QDL_PAD_RGMII_TD1__RGMII_TD1		0x1b0b0
				MX6QDL_PAD_RGMII_TD2__RGMII_TD2		0x1b0b0
				MX6QDL_PAD_RGMII_TD3__RGMII_TD3		0x1b0b0
				MX6QDL_PAD_RGMII_TX_CTL__RGMII_TX_CTL	0x1b0b0
				MX6QDL_PAD_ENET_REF_CLK__ENET_TX_CLK	0x1b0b0
				MX6QDL_PAD_ENET_MDIO__ENET_MDIO		0x1b0b0
				MX6QDL_PAD_ENET_MDC__ENET_MDC		0x1b0b0
			>;
		};

		pinctrl_i2c1: i2c1grp {
			fsl,pins = <
				MX6QDL_PAD_EIM_D21__I2C1_SCL		0x4001b8b1
				MX6QDL_PAD_EIM_D28__I2C1_SDA		0x4001b8b1
			>;
		};

		pinctrl_uart2: uart2grp {
			fsl,pins = <
				MX6QDL_PAD_EIM_D26__UART2_TX_DATA	0x1b0b1
				MX6QDL_PAD_EIM_D27__UART2_RX_DATA	0x1b0b1
			>;
		};

		pinctrl_usdhc3: usdhc3grp {
			fsl,pins = <
				MX6QDL_PAD_SD3_CMD__SD3_CMD		0x17059
				MX6QDL_PAD_SD3_CLK__SD3_CLK		0x10059
				MX6QDL_PAD_SD3_DAT0__SD3_DATA0		0x17059
				MX6QDL_PAD_SD3_DAT1__SD3_DATA1		0x17059
				MX6QDL_PAD_SD3_DAT2__SD3_DATA2		0x17059
				MX6QDL_PAD_SD3_DAT3__SD3_DATA3		0x17059
			>;
		};
	};
};

&uart2 {
	pinctrl-names = "default";
	pinctrl-0 = <&pinctrl_uart2>;
	status = "okay";
};

&usdhc3 {
	pinctrl-names = "default";
	pinctrl-0 = <&pinctrl_usdhc3>;
	status = "okay";
};
