/*
 * Copyright 2013 Gateworks Corporation
 *
 * The code contained herein is licensed under the GNU General Public
 * License. You may obtain a copy of the GNU General Public License
 * Version 2 or later at the following locations:
 *
 * http://www.opensource.org/licenses/gpl-license.html
 * http://www.gnu.org/copyleft/gpl.html
 */

/ {
	/* these are used by bootloader for disabling nodes */
	aliases {
		can0 = &can1;
		ethernet0 = &fec;
		led0 = &led0;
		led1 = &led1;
		nand = &gpmi;
		usb0 = &usbh1;
		usb1 = &usbotg;
	};

	chosen {
		bootargs = "console=ttymxc1,115200";
	};

	leds {
		compatible = "gpio-leds";

		led0: user1 {
			label = "user1";
			gpios = <&gpio4 6 0>; /* 102 -> MX6_PANLEDG */
			default-state = "on";
			linux,default-trigger = "heartbeat";
		};

		led1: user2 {
			label = "user2";
			gpios = <&gpio4 7 0>; /* 103 -> MX6_PANLEDR */
			default-state = "off";
		};
	};

	memory {
		reg = <0x10000000 0x20000000>;
	};

	pps {
		compatible = "pps-gpio";
		gpios = <&gpio1 26 0>;
		status = "okay";
	};

	regulators {
		compatible = "simple-bus";
		#address-cells = <1>;
		#size-cells = <0>;

		reg_3p3v: regulator@0 {
			compatible = "regulator-fixed";
			reg = <0>;
			regulator-name = "3P3V";
			regulator-min-microvolt = <3300000>;
			regulator-max-microvolt = <3300000>;
			regulator-always-on;
		};

		reg_5p0v: regulator@1 {
			compatible = "regulator-fixed";
			reg = <1>;
			regulator-name = "5P0V";
			regulator-min-microvolt = <5000000>;
			regulator-max-microvolt = <5000000>;
			regulator-always-on;
		};

		reg_usb_otg_vbus: regulator@2 {
			compatible = "regulator-fixed";
			reg = <2>;
			regulator-name = "usb_otg_vbus";
			regulator-min-microvolt = <5000000>;
			regulator-max-microvolt = <5000000>;
			gpio = <&gpio3 22 0>;
			enable-active-high;
		};
	};
};

&fec {
	pinctrl-names = "default";
	pinctrl-0 = <&pinctrl_enet>;
	phy-mode = "rgmii";
	phy-reset-gpios = <&gpio1 30 0>;
	status = "okay";
};

&gpmi {
	pinctrl-names = "default";
	pinctrl-0 = <&pinctrl_gpmi_nand>;
	status = "okay";
};

&hdmi {
	ddc-i2c-bus = <&i2c3>;
	status = "okay";
};

&i2c1 {
	clock-frequency = <100000>;
	pinctrl-names = "default";
	pinctrl-0 = <&pinctrl_i2c1>;
	status = "okay";

	eeprom1: eeprom@50 {
		compatible = "atmel,24c02";
		reg = <0x50>;
		pagesize = <16>;
	};

	eeprom2: eeprom@51 {
		compatible = "atmel,24c02";
		reg = <0x51>;
		pagesize = <16>;
	};

	eeprom3: eeprom@52 {
		compatible = "atmel,24c02";
		reg = <0x52>;
		pagesize = <16>;
	};

	eeprom4: eeprom@53 {
		compatible = "atmel,24c02";
		reg = <0x53>;
		pagesize = <16>;
	};

	gpio: pca9555@23 {
		compatible = "nxp,pca9555";
		reg = <0x23>;
		gpio-controller;
		#gpio-cells = <2>;
	};

	hwmon: gsc@29 {
		compatible = "gw,gsp";
		reg = <0x29>;
	};

	rtc: ds1672@68 {
		compatible = "dallas,ds1672";
		reg = <0x68>;
	};
};

&i2c2 {
	clock-frequency = <100000>;
	pinctrl-names = "default";
	pinctrl-0 = <&pinctrl_i2c2>;
	status = "okay";

	pmic: ltc3676@3c {
		compatible = "ltc,ltc3676";
		reg = <0x3c>;

		regulators {
			sw1_reg: ltc3676__sw1 {
				regulator-min-microvolt = <1175000>;
				regulator-max-microvolt = <1175000>;
				regulator-boot-on;
				regulator-always-on;
			};

			sw2_reg: ltc3676__sw2 {
				regulator-min-microvolt = <1800000>;
				regulator-max-microvolt = <1800000>;
				regulator-boot-on;
				regulator-always-on;
			};

			sw3_reg: ltc3676__sw3 {
				regulator-min-microvolt = <1175000>;
				regulator-max-microvolt = <1175000>;
				regulator-boot-on;
				regulator-always-on;
			};

			sw4_reg: ltc3676__sw4 {
				regulator-min-microvolt = <1500000>;
				regulator-max-microvolt = <1500000>;
				regulator-boot-on;
				regulator-always-on;
			};

			ldo2_reg: ltc3676__ldo2 {
				regulator-min-microvolt = <2500000>;
				regulator-max-microvolt = <2500000>;
				regulator-boot-on;
				regulator-always-on;
			};

			ldo4_reg: ltc3676__ldo4 {
				regulator-min-microvolt = <3000000>;
				regulator-max-microvolt = <3000000>;
			};
		};
	};
};

&i2c3 {
	clock-frequency = <100000>;
	pinctrl-names = "default";
	pinctrl-0 = <&pinctrl_i2c3>;
	status = "okay";

	videoin: adv7180@20 {
		compatible = "adi,adv7180";
		reg = <0x20>;
	};
};

&iomuxc {
	pinctrl-names = "default";
	pinctrl-0 = <&pinctrl_hog>;

	imx6qdl-gw51xx {
		pinctrl_hog: hoggrp {
			fsl,pins = <
				MX6QDL_PAD_EIM_A19__GPIO2_IO19   0x80000000 /* MEZZ_DIO0 */
				MX6QDL_PAD_EIM_A20__GPIO2_IO18   0x80000000 /* MEZZ_DIO1 */
				MX6QDL_PAD_EIM_D22__GPIO3_IO22   0x80000000 /* OTG_PWR_EN */
				MX6QDL_PAD_ENET_RXD1__GPIO1_IO26 0x80000000 /* GPS_PPS */
				MX6QDL_PAD_ENET_TXD0__GPIO1_IO30 0x80000000 /* PHY Reset */
				MX6QDL_PAD_GPIO_0__GPIO1_IO00    0x80000000 /* PCIE_RST# */
				MX6QDL_PAD_KEY_COL0__GPIO4_IO06  0x80000000 /* user1 led */
				MX6QDL_PAD_KEY_ROW0__GPIO4_IO07  0x80000000 /* user2 led */
			 >;
		};

		pinctrl_enet: enetgrp {
			fsl,pins = <
				MX6QDL_PAD_RGMII_RXC__RGMII_RXC		0x1b0b0
				MX6QDL_PAD_RGMII_RD0__RGMII_RD0		0x1b0b0
				MX6QDL_PAD_RGMII_RD1__RGMII_RD1		0x1b0b0
				MX6QDL_PAD_RGMII_RD2__RGMII_RD2		0x1b0b0
				MX6QDL_PAD_RGMII_RD3__RGMII_RD3		0x1b0b0
				MX6QDL_PAD_RGMII_RX_CTL__RGMII_RX_CTL	0x1b0b0
				MX6QDL_PAD_RGMII_TXC__RGMII_TXC		0x1b0b0
				MX6QDL_PAD_RGMII_TD0__RGMII_TD0		0x1b0b0
				MX6QDL_PAD_RGMII_TD1__RGMII_TD1		0x1b0b0
				MX6QDL_PAD_RGMII_TD2__RGMII_TD2		0x1b0b0
				MX6QDL_PAD_RGMII_TD3__RGMII_TD3		0x1b0b0
				MX6QDL_PAD_RGMII_TX_CTL__RGMII_TX_CTL	0x1b0b0
				MX6QDL_PAD_ENET_REF_CLK__ENET_TX_CLK	0x1b0b0
				MX6QDL_PAD_ENET_MDIO__ENET_MDIO		0x1b0b0
				MX6QDL_PAD_ENET_MDC__ENET_MDC		0x1b0b0
				MX6QDL_PAD_GPIO_16__ENET_REF_CLK	0x4001b0a8
			>;
		};

		pinctrl_gpmi_nand: gpminandgrp {
			fsl,pins = <
				MX6QDL_PAD_NANDF_CLE__NAND_CLE		0xb0b1
				MX6QDL_PAD_NANDF_ALE__NAND_ALE		0xb0b1
				MX6QDL_PAD_NANDF_WP_B__NAND_WP_B	0xb0b1
				MX6QDL_PAD_NANDF_RB0__NAND_READY_B	0xb000
				MX6QDL_PAD_NANDF_CS0__NAND_CE0_B	0xb0b1
				MX6QDL_PAD_NANDF_CS1__NAND_CE1_B	0xb0b1
				MX6QDL_PAD_SD4_CMD__NAND_RE_B		0xb0b1
				MX6QDL_PAD_SD4_CLK__NAND_WE_B		0xb0b1
				MX6QDL_PAD_NANDF_D0__NAND_DATA00	0xb0b1
				MX6QDL_PAD_NANDF_D1__NAND_DATA01	0xb0b1
				MX6QDL_PAD_NANDF_D2__NAND_DATA02	0xb0b1
				MX6QDL_PAD_NANDF_D3__NAND_DATA03	0xb0b1
				MX6QDL_PAD_NANDF_D4__NAND_DATA04	0xb0b1
				MX6QDL_PAD_NANDF_D5__NAND_DATA05	0xb0b1
				MX6QDL_PAD_NANDF_D6__NAND_DATA06	0xb0b1
				MX6QDL_PAD_NANDF_D7__NAND_DATA07	0xb0b1
			>;
		};

		pinctrl_i2c1: i2c1grp {
			fsl,pins = <
				MX6QDL_PAD_EIM_D21__I2C1_SCL		0x4001b8b1
				MX6QDL_PAD_EIM_D28__I2C1_SDA		0x4001b8b1
			>;
		};

		pinctrl_i2c2: i2c2grp {
			fsl,pins = <
				MX6QDL_PAD_KEY_COL3__I2C2_SCL		0x4001b8b1
				MX6QDL_PAD_KEY_ROW3__I2C2_SDA		0x4001b8b1
			>;
		};

		pinctrl_i2c3: i2c3grp {
			fsl,pins = <
				MX6QDL_PAD_GPIO_3__I2C3_SCL		0x4001b8b1
				MX6QDL_PAD_GPIO_6__I2C3_SDA		0x4001b8b1
			>;
		};

		pinctrl_uart1: uart1grp {
			fsl,pins = <
				MX6QDL_PAD_SD3_DAT7__UART1_TX_DATA	0x1b0b1
				MX6QDL_PAD_SD3_DAT6__UART1_RX_DATA	0x1b0b1
			>;
		};

		pinctrl_uart2: uart2grp {
			fsl,pins = <
				MX6QDL_PAD_SD4_DAT7__UART2_TX_DATA	0x1b0b1
				MX6QDL_PAD_SD4_DAT4__UART2_RX_DATA	0x1b0b1
			>;
		};

		pinctrl_uart3: uart3grp {
			fsl,pins = <
				MX6QDL_PAD_EIM_D24__UART3_TX_DATA	0x1b0b1
				MX6QDL_PAD_EIM_D25__UART3_RX_DATA	0x1b0b1
			>;
		};

		pinctrl_uart5: uart5grp {
			fsl,pins = <
				MX6QDL_PAD_KEY_COL1__UART5_TX_DATA	0x1b0b1
				MX6QDL_PAD_KEY_ROW1__UART5_RX_DATA	0x1b0b1
			>;
		};

		pinctrl_usbotg: usbotggrp {
			fsl,pins = <
				MX6QDL_PAD_GPIO_1__USB_OTG_ID		0x17059
			>;
		};
	};
};

&pcie {
	reset-gpio = <&gpio1 0 0>;
	status = "okay";
};

&uart1 {
	pinctrl-names = "default";
	pinctrl-0 = <&pinctrl_uart1>;
	status = "okay";
};

&uart2 {
	pinctrl-names = "default";
	pinctrl-0 = <&pinctrl_uart2>;
	status = "okay";
};

&uart3 {
	pinctrl-names = "default";
	pinctrl-0 = <&pinctrl_uart3>;
	status = "okay";
};

&uart5 {
	pinctrl-names = "default";
	pinctrl-0 = <&pinctrl_uart5>;
	status = "okay";
};

&usbotg {
	vbus-supply = <&reg_usb_otg_vbus>;
	pinctrl-names = "default";
	pinctrl-0 = <&pinctrl_usbotg>;
	disable-over-current;
	status = "okay";
};

&usbh1 {
	status = "okay";
};
