/*
 * at91-cosino.dtsi - Device Tree file for Cosino core module
 *
 * Copyright (C) 2013 - Rodolfo Giometti <giometti@linux.it>
 *			HCE Engineering
 *
 * Derived from at91sam9x5ek.dtsi by:
 *	Copyright (C) 2012 Atmel,
 *	2012 Nicolas Ferre <nicolas.ferre@atmel.com>
 *
 * Licensed under GPLv2 or later.
 */

#include "at91sam9g35.dtsi"

/ {
	model = "HCE Cosino core module";
	compatible = "hce,cosino", "atmel,at91sam9x5", "atmel,at91sam9";

	chosen {
		bootargs = "console=ttyS0,115200 root=/dev/mmcblk0p2 rw rootfstype=ext3 rootwait";
	};

	memory {
		reg = <0x20000000 0x8000000>;
	};

	clocks {
		#address-cells = <1>;
		#size-cells = <1>;
		ranges;

		main_clock: clock@0 {
			compatible = "atmel,osc", "fixed-clock";
			clock-frequency = <12000000>;
		};
	};

	ahb {
		apb {
			mmc0: mmc@f0008000 {
				pinctrl-0 = <
					&pinctrl_board_mmc0
					&pinctrl_mmc0_slot0_clk_cmd_dat0
					&pinctrl_mmc0_slot0_dat1_3>;
				status = "okay";
				slot@0 {
					reg = <0>;
					bus-width = <4>;
					cd-gpios = <&pioD 15 GPIO_ACTIVE_HIGH>;
				};
			};

			dbgu: serial@fffff200 {
				status = "okay";
			};

			usart0: serial@f801c000 {
				status = "okay";
			};

			i2c0: i2c@f8010000 {
				status = "okay";
			};

			adc0: adc@f804c000 {
				atmel,adc-ts-wires = <4>;
				atmel,adc-ts-pressure-threshold = <10000>;
				status = "okay";
			};

			pinctrl@fffff400 {
				mmc0 {
					pinctrl_board_mmc0: mmc0-board {
						atmel,pins =
							<AT91_PIOD 15 AT91_PERIPH_GPIO AT91_PINCTRL_PULL_UP_DEGLITCH>;	/* PD15 gpio CD pin pull up and deglitch */
					};
				};
			};

			watchdog@fffffe40 {
				status = "okay";
			};
		};

		nand0: nand@40000000 {
			nand-bus-width = <8>;
			nand-ecc-mode = "hw";
			atmel,has-pmecc;	/* Enable PMECC */
			atmel,pmecc-cap = <4>;
			atmel,pmecc-sector-size = <512>;
			nand-on-flash-bbt;
			status = "okay";

			at91bootstrap@0 {
				label = "at91bootstrap";
				reg = <0x0 0x40000>;
			};

			uboot@40000 {
				label = "u-boot";
				reg = <0x40000 0x80000>;
			};

			ubootenv@c0000 {
				label = "U-Boot Env";
				reg = <0xc0000 0x140000>;
			};

			kernel@200000 {
				label = "kernel";
				reg = <0x200000 0x600000>;
			};

			rootfs@800000 {
				label = "rootfs";
				reg = <0x800000 0x0f800000>;
			};
		};
	};
};
