/*
 * phyCORE-MPC5200B-tiny (pcm030) board Device Tree Source
 *
 * Copyright 2006 Pengutronix
 * Sascha Hauer <s.hauer@pengutronix.de>
 * Copyright 2007 Pengutronix
 * Juergen Beisert <j.beisert@pengutronix.de>
 *
 * This program is free software; you can redistribute  it and/or modify it
 * under  the terms of  the GNU General  Public License as published by the
 * Free Software Foundation;  either version 2 of the  License, or (at your
 * option) any later version.
 */

/include/ "mpc5200b.dtsi"

&gpt0 { fsl,has-wdt; };
&gpt2 { gpio-controller; };
&gpt3 { gpio-controller; };
&gpt4 { gpio-controller; };
&gpt5 { gpio-controller; };
&gpt6 { gpio-controller; };
&gpt7 { gpio-controller; };

/ {
	model = "phytec,pcm030";
	compatible = "phytec,pcm030";

	soc5200@f0000000 {
		audioplatform: psc@2000 { /* PSC1 in ac97 mode */
			compatible = "mpc5200b-psc-ac97","fsl,mpc5200b-psc-ac97";
			cell-index = <0>;
		};

		/* PSC2 port is used by CAN1/2 */
		psc@2200 {
			status = "disabled";
		};

		psc@2400 { /* PSC3 in UART mode */
			compatible = "fsl,mpc5200b-psc-uart","fsl,mpc5200-psc-uart";
		};

		/* PSC4 is ??? */
		psc@2600 {
			status = "disabled";
		};

		/* PSC5 is ??? */
		psc@2800 {
			status = "disabled";
		};

		psc@2c00 { /* PSC6 in UART mode */
			compatible = "fsl,mpc5200b-psc-uart","fsl,mpc5200-psc-uart";
		};

		ethernet@3000 {
			phy-handle = <&phy0>;
		};

		mdio@3000 {
			phy0: ethernet-phy@0 {
				reg = <0>;
			};
		};

		i2c@3d40 {
			rtc@51 {
				compatible = "nxp,pcf8563";
				reg = <0x51>;
			};
			eeprom@52 {
				compatible = "catalyst,24c32";
				reg = <0x52>;
				pagesize = <32>;
			};
		};

		sram@8000 {
			compatible = "fsl,mpc5200b-sram","fsl,mpc5200-sram";
			reg = <0x8000 0x4000>;
		};
	};

	pci@f0000d00 {
		interrupt-map-mask = <0xf800 0 0 7>;
		interrupt-map = <0xc000 0 0 1 &mpc5200_pic 0 0 3 // 1st slot
				 0xc000 0 0 2 &mpc5200_pic 1 1 3
				 0xc000 0 0 3 &mpc5200_pic 1 2 3
				 0xc000 0 0 4 &mpc5200_pic 1 3 3

				 0xc800 0 0 1 &mpc5200_pic 1 1 3 // 2nd slot
				 0xc800 0 0 2 &mpc5200_pic 1 2 3
				 0xc800 0 0 3 &mpc5200_pic 1 3 3
				 0xc800 0 0 4 &mpc5200_pic 0 0 3>;
		ranges = <0x42000000 0 0x80000000 0x80000000 0 0x20000000
			  0x02000000 0 0xa0000000 0xa0000000 0 0x10000000
			  0x01000000 0 0x00000000 0xb0000000 0 0x01000000>;
	};

	localbus {
		status = "disabled";
	};

	sound {
		compatible = "phytec,pcm030-audio-fabric";
		asoc-platform = <&audioplatform>;
	};
};
