/*
 * OCA4080 Device Tree Source
 *
 * Copyright 2014 Prodrive Technologies B.V.
 *
 * Based on:
 * P4080DS Device Tree Source
 * Copyright 2009-2011 Freescale Semiconductor Inc.
 *
 * Redistribution and use in source and binary forms, with or without
 * modification, are permitted provided that the following conditions are met:
 *     * Redistributions of source code must retain the above copyright
 *       notice, this list of conditions and the following disclaimer.
 *     * Redistributions in binary form must reproduce the above copyright
 *       notice, this list of conditions and the following disclaimer in the
 *       documentation and/or other materials provided with the distribution.
 *     * Neither the name of Freescale Semiconductor nor the
 *       names of its contributors may be used to endorse or promote products
 *       derived from this software without specific prior written permission.
 *
 *
 * ALTERNATIVELY, this software may be distributed under the terms of the
 * GNU General Public License ("GPL") as published by the Free Software
 * Foundation, either version 2 of that License or (at your option) any
 * later version.
 *
 * THIS SOFTWARE IS PROVIDED BY Freescale Semiconductor ``AS IS'' AND ANY
 * EXPRESS OR IMPLIED WARRANTIES, INCLUDING, BUT NOT LIMITED TO, THE IMPLIED
 * WARRANTIES OF MERCHANTABILITY AND FITNESS FOR A PARTICULAR PURPOSE ARE
 * DISCLAIMED. IN NO EVENT SHALL Freescale Semiconductor BE LIABLE FOR ANY
 * DIRECT, INDIRECT, INCIDENTAL, SPECIAL, EXEMPLARY, OR CONSEQUENTIAL DAMAGES
 * (INCLUDING, BUT NOT LIMITED TO, PROCUREMENT OF SUBSTITUTE GOODS OR SERVICES;
 * LOSS OF USE, DATA, OR PROFITS; OR BUSINESS INTERRUPTION) HOWEVER CAUSED AND
 * ON ANY THEORY OF LIABILITY, WHETHER IN CONTRACT, STRICT LIABILITY, OR TORT
 * (INCLUDING NEGLIGENCE OR OTHERWISE) ARISING IN ANY WAY OUT OF THE USE OF THIS
 * SOFTWARE, EVEN IF ADVISED OF THE POSSIBILITY OF SUCH DAMAGE.
 */

/include/ "fsl/p4080si-pre.dtsi"

/ {
	model = "fsl,OCA4080";
	compatible = "fsl,OCA4080";
	#address-cells = <2>;
	#size-cells = <2>;
	interrupt-parent = <&mpic>;

	memory {
		device_type = "memory";
	};

	dcsr: dcsr@f00000000 {
		ranges = <0x00000000 0xf 0x00000000 0x01008000>;
	};

	soc: soc@ffe000000 {
		ranges = <0x00000000 0xf 0xfe000000 0x1000000>;
		reg = <0xf 0xfe000000 0 0x00001000>;

		i2c@118000 {
			status = "disabled";
		};

		i2c@118100 {
			status = "disabled";
		};

		i2c@119000 {
			status = "disabled";
		};

		i2c@119100 {
			status = "disabled";
		};

		usb0: usb@210000 {
			status = "disabled";
		};

		usb1: usb@211000 {
			status = "disabled";
		};
	};

	rio: rapidio@ffe0c0000 {
		reg = <0xf 0xfe0c0000 0 0x11000>;

		port1 {
			ranges = <0 0 0xc 0x20000000 0 0x10000000>;
		};
	};

	lbc: localbus@ffe124000 {
		reg = <0xf 0xfe124000 0 0x1000>;
		ranges = <0 0 0xf 0xef800000 0x800000>;

		flash@0,0 {
			compatible = "cfi-flash";
			reg = <0 0 0x00800000>;
			bank-width = <2>;
			device-width = <2>;
		};
	};

	pci0: pcie@ffe200000 {
		status = "disabled";
	};

	pci1: pcie@ffe201000 {
		status = "disabled";
	};

	pci2: pcie@ffe202000 {
		status = "disabled";
	};
};

/include/ "fsl/p4080si-post.dtsi"
