/*
 * Copyright 2014 Hans de Goede <hdegoede@redhat.com>
 *
 * The code contained herein is licensed under the GNU General Public
 * License. You may obtain a copy of the GNU General Public License
 * Version 2 or later at the following locations:
 *
 * http://www.opensource.org/licenses/gpl-license.html
 * http://www.gnu.org/copyleft/gpl.html
 */

/dts-v1/;
/include/ "sun5i-a10s.dtsi"
/include/ "sunxi-common-regulators.dtsi"

/ {
	model = "R7 A10s hdmi tv-stick";
	compatible = "allwinner,r7-tv-dongle", "allwinner,sun5i-a10s";

	soc@01c00000 {
		mmc0: mmc@01c0f000 {
			pinctrl-names = "default";
			pinctrl-0 = <&mmc0_pins_a>, <&mmc0_cd_pin_r7>;
			vmmc-supply = <&reg_vcc3v3>;
			bus-width = <4>;
			cd-gpios = <&pio 6 1 0>; /* PG1 */
			cd-inverted;
			status = "okay";
		};

		mmc1: mmc@01c10000 {
			pinctrl-names = "default";
			pinctrl-0 = <&mmc1_pins_a>;
			vmmc-supply = <&reg_vcc3v3>;
			bus-width = <4>;
			non-removable;
			status = "okay";
		};

		usbphy: phy@01c13400 {
			usb1_vbus-supply = <&reg_usb1_vbus>;
			status = "okay";
		};

		ehci0: usb@01c14000 {
			status = "okay";
		};

		ohci0: usb@01c14400 {
			status = "okay";
		};

		pinctrl@01c20800 {
			mmc0_cd_pin_r7: mmc0_cd_pin@0 {
				allwinner,pins = "PG1";
				allwinner,function = "gpio_in";
				allwinner,drive = <0>;
				allwinner,pull = <1>;
			};

			led_pins_r7: led_pins@0 {
				allwinner,pins = "PB2";
				allwinner,function = "gpio_out";
				allwinner,drive = <1>;
				allwinner,pull = <0>;
			};

			usb1_vbus_pin_r7: usb1_vbus_pin@0 {
				allwinner,pins = "PG13";
				allwinner,function = "gpio_out";
				allwinner,drive = <0>;
				allwinner,pull = <0>;
			};
		};

		uart0: serial@01c28000 {
			pinctrl-names = "default";
			pinctrl-0 = <&uart0_pins_a>;
			status = "okay";
		};
	};

	leds {
		compatible = "gpio-leds";
		pinctrl-names = "default";
		pinctrl-0 = <&led_pins_r7>;

		green {
			label = "r7-tv-dongle:green:usr";
			gpios = <&pio 1 2 0>;
			default-state = "on";
		};
	};

	reg_usb1_vbus: usb1-vbus {
		pinctrl-0 = <&usb1_vbus_pin_r7>;
		gpio = <&pio 6 13 0>;
		status = "okay";
	};
};
