/dts-v1/;

#include "skeleton.dtsi"
#include <dt-bindings/clock/qcom,gcc-msm8960.h>
#include <dt-bindings/soc/qcom,gsbi.h>

/ {
	model = "Qualcomm APQ8064";
	compatible = "qcom,apq8064";
	interrupt-parent = <&intc>;

	cpus {
		#address-cells = <1>;
		#size-cells = <0>;

		cpu@0 {
			compatible = "qcom,krait";
			enable-method = "qcom,kpss-acc-v1";
			device_type = "cpu";
			reg = <0>;
			next-level-cache = <&L2>;
			qcom,acc = <&acc0>;
			qcom,saw = <&saw0>;
		};

		cpu@1 {
			compatible = "qcom,krait";
			enable-method = "qcom,kpss-acc-v1";
			device_type = "cpu";
			reg = <1>;
			next-level-cache = <&L2>;
			qcom,acc = <&acc1>;
			qcom,saw = <&saw1>;
		};

		cpu@2 {
			compatible = "qcom,krait";
			enable-method = "qcom,kpss-acc-v1";
			device_type = "cpu";
			reg = <2>;
			next-level-cache = <&L2>;
			qcom,acc = <&acc2>;
			qcom,saw = <&saw2>;
		};

		cpu@3 {
			compatible = "qcom,krait";
			enable-method = "qcom,kpss-acc-v1";
			device_type = "cpu";
			reg = <3>;
			next-level-cache = <&L2>;
			qcom,acc = <&acc3>;
			qcom,saw = <&saw3>;
		};

		L2: l2-cache {
			compatible = "cache";
			cache-level = <2>;
		};
	};

	cpu-pmu {
		compatible = "qcom,krait-pmu";
		interrupts = <1 10 0x304>;
	};

	soc: soc {
		#address-cells = <1>;
		#size-cells = <1>;
		ranges;
		compatible = "simple-bus";

		intc: interrupt-controller@2000000 {
			compatible = "qcom,msm-qgic2";
			interrupt-controller;
			#interrupt-cells = <3>;
			reg = <0x02000000 0x1000>,
			      <0x02002000 0x1000>;
		};

		timer@200a000 {
			compatible = "qcom,kpss-timer", "qcom,msm-timer";
			interrupts = <1 1 0x301>,
				     <1 2 0x301>,
				     <1 3 0x301>;
			reg = <0x0200a000 0x100>;
			clock-frequency = <27000000>,
					  <32768>;
			cpu-offset = <0x80000>;
		};

		acc0: clock-controller@2088000 {
			compatible = "qcom,kpss-acc-v1";
			reg = <0x02088000 0x1000>, <0x02008000 0x1000>;
		};

		acc1: clock-controller@2098000 {
			compatible = "qcom,kpss-acc-v1";
			reg = <0x02098000 0x1000>, <0x02008000 0x1000>;
		};

		acc2: clock-controller@20a8000 {
			compatible = "qcom,kpss-acc-v1";
			reg = <0x020a8000 0x1000>, <0x02008000 0x1000>;
		};

		acc3: clock-controller@20b8000 {
			compatible = "qcom,kpss-acc-v1";
			reg = <0x020b8000 0x1000>, <0x02008000 0x1000>;
		};

		saw0: regulator@2089000 {
			compatible = "qcom,saw2";
			reg = <0x02089000 0x1000>, <0x02009000 0x1000>;
			regulator;
		};

		saw1: regulator@2099000 {
			compatible = "qcom,saw2";
			reg = <0x02099000 0x1000>, <0x02009000 0x1000>;
			regulator;
		};

		saw2: regulator@20a9000 {
			compatible = "qcom,saw2";
			reg = <0x020a9000 0x1000>, <0x02009000 0x1000>;
			regulator;
		};

		saw3: regulator@20b9000 {
			compatible = "qcom,saw2";
			reg = <0x020b9000 0x1000>, <0x02009000 0x1000>;
			regulator;
		};

		gsbi7: gsbi@16600000 {
			status = "disabled";
			compatible = "qcom,gsbi-v1.0.0";
			reg = <0x16600000 0x100>;
			clocks = <&gcc GSBI7_H_CLK>;
			clock-names = "iface";
			#address-cells = <1>;
			#size-cells = <1>;
			ranges;

			serial@16640000 {
				compatible = "qcom,msm-uartdm-v1.3", "qcom,msm-uartdm";
				reg = <0x16640000 0x1000>,
				      <0x16600000 0x1000>;
				interrupts = <0 158 0x0>;
				clocks = <&gcc GSBI7_UART_CLK>, <&gcc GSBI7_H_CLK>;
				clock-names = "core", "iface";
				status = "disabled";
			};
		};

		qcom,ssbi@500000 {
			compatible = "qcom,ssbi";
			reg = <0x00500000 0x1000>;
			qcom,controller-type = "pmic-arbiter";
		};

		gcc: clock-controller@900000 {
			compatible = "qcom,gcc-apq8064";
			reg = <0x00900000 0x4000>;
			#clock-cells = <1>;
			#reset-cells = <1>;
		};
	};
};
