/*
 * Copyright 2013 Freescale Semiconductor, Inc.
 *
 * This program is free software; you can redistribute it and/or modify
 * it under the terms of the GNU General Public License as published by
 * the Free Software Foundation; either version 2 of the License, or
 * (at your option) any later version.
 */

#include "skeleton.dtsi"
#include "vf610-pinfunc.h"
#include <dt-bindings/clock/vf610-clock.h>
#include <dt-bindings/interrupt-controller/irq.h>

/ {
	aliases {
		serial0 = &uart0;
		serial1 = &uart1;
		serial2 = &uart2;
		serial3 = &uart3;
		serial4 = &uart4;
		serial5 = &uart5;
		gpio0 = &gpio1;
		gpio1 = &gpio2;
		gpio2 = &gpio3;
		gpio3 = &gpio4;
		gpio4 = &gpio5;
	};

	cpus {
		#address-cells = <1>;
		#size-cells = <0>;

		cpu@0 {
			compatible = "arm,cortex-a5";
			device_type = "cpu";
			reg = <0x0>;
			next-level-cache = <&L2>;
		};
	};

	clocks {
		#address-cells = <1>;
		#size-cells = <0>;

		sxosc {
			compatible = "fixed-clock";
			#clock-cells = <0>;
			clock-frequency = <32768>;
		};

		fxosc {
			compatible = "fixed-clock";
			#clock-cells = <0>;
			clock-frequency = <24000000>;
		};
	};

	soc {
		#address-cells = <1>;
		#size-cells = <1>;
		compatible = "simple-bus";
		interrupt-parent = <&intc>;
		ranges;

		aips0: aips-bus@40000000 {
			compatible = "fsl,aips-bus", "simple-bus";
			#address-cells = <1>;
			#size-cells = <1>;
			interrupt-parent = <&intc>;
			reg = <0x40000000 0x70000>;
			ranges;

			intc: interrupt-controller@40002000 {
				compatible = "arm,cortex-a9-gic";
				#interrupt-cells = <3>;
				interrupt-controller;
				reg = <0x40003000 0x1000>,
				      <0x40002100 0x100>;
			};

			L2: l2-cache@40006000 {
				compatible = "arm,pl310-cache";
				reg = <0x40006000 0x1000>;
				cache-unified;
				cache-level = <2>;
				arm,data-latency = <1 1 1>;
				arm,tag-latency = <2 2 2>;
			};

			edma0: dma-controller@40018000 {
				#dma-cells = <2>;
				compatible = "fsl,vf610-edma";
				reg = <0x40018000 0x2000>,
					<0x40024000 0x1000>,
					<0x40025000 0x1000>;
				interrupts = <0 8 IRQ_TYPE_LEVEL_HIGH>,
						<0 9 IRQ_TYPE_LEVEL_HIGH>;
				interrupt-names = "edma-tx", "edma-err";
				dma-channels = <32>;
				clock-names = "dmamux0", "dmamux1";
				clocks = <&clks VF610_CLK_DMAMUX0>,
					<&clks VF610_CLK_DMAMUX1>;
			};

			uart0: serial@40027000 {
				compatible = "fsl,vf610-lpuart";
				reg = <0x40027000 0x1000>;
				interrupts = <0 61 IRQ_TYPE_LEVEL_HIGH>;
				clocks = <&clks VF610_CLK_UART0>;
				clock-names = "ipg";
				dmas = <&edma0 0 2>,
					<&edma0 0 3>;
				dma-names = "rx","tx";
				status = "disabled";
			};

			uart1: serial@40028000 {
				compatible = "fsl,vf610-lpuart";
				reg = <0x40028000 0x1000>;
				interrupts = <0 62 IRQ_TYPE_LEVEL_HIGH>;
				clocks = <&clks VF610_CLK_UART1>;
				clock-names = "ipg";
				dmas = <&edma0 0 4>,
					<&edma0 0 5>;
				dma-names = "rx","tx";
				status = "disabled";
			};

			uart2: serial@40029000 {
				compatible = "fsl,vf610-lpuart";
				reg = <0x40029000 0x1000>;
				interrupts = <0 63 IRQ_TYPE_LEVEL_HIGH>;
				clocks = <&clks VF610_CLK_UART2>;
				clock-names = "ipg";
				dmas = <&edma0 0 6>,
					<&edma0 0 7>;
				dma-names = "rx","tx";
				status = "disabled";
			};

			uart3: serial@4002a000 {
				compatible = "fsl,vf610-lpuart";
				reg = <0x4002a000 0x1000>;
				interrupts = <0 64 IRQ_TYPE_LEVEL_HIGH>;
				clocks = <&clks VF610_CLK_UART3>;
				clock-names = "ipg";
				dmas = <&edma0 0 8>,
					<&edma0 0 9>;
				dma-names = "rx","tx";
				status = "disabled";
			};

			dspi0: dspi0@4002c000 {
				#address-cells = <1>;
				#size-cells = <0>;
				compatible = "fsl,vf610-dspi";
				reg = <0x4002c000 0x1000>;
				interrupts = <0 67 IRQ_TYPE_LEVEL_HIGH>;
				clocks = <&clks VF610_CLK_DSPI0>;
				clock-names = "dspi";
				spi-num-chipselects = <5>;
				status = "disabled";
			};

			sai2: sai@40031000 {
				compatible = "fsl,vf610-sai";
				reg = <0x40031000 0x1000>;
				interrupts = <0 86 IRQ_TYPE_LEVEL_HIGH>;
				clocks = <&clks VF610_CLK_SAI2>;
				clock-names = "sai";
				dma-names = "tx", "rx";
				dmas = <&edma0 0 21>,
					<&edma0 0 20>;
				status = "disabled";
			};

			pit: pit@40037000 {
				compatible = "fsl,vf610-pit";
				reg = <0x40037000 0x1000>;
				interrupts = <0 39 IRQ_TYPE_LEVEL_HIGH>;
				clocks = <&clks VF610_CLK_PIT>;
				clock-names = "pit";
			};

			pwm0: pwm@40038000 {
				compatible = "fsl,vf610-ftm-pwm";
				#pwm-cells = <3>;
				reg = <0x40038000 0x1000>;
				clock-names = "ftm_sys", "ftm_ext",
					      "ftm_fix", "ftm_cnt_clk_en";
				clocks = <&clks VF610_CLK_FTM0>,
					<&clks VF610_CLK_FTM0_EXT_SEL>,
					<&clks VF610_CLK_FTM0_FIX_SEL>,
					<&clks VF610_CLK_FTM0_EXT_FIX_EN>;
				status = "disabled";
			};

			adc0: adc@4003b000 {
				compatible = "fsl,vf610-adc";
				reg = <0x4003b000 0x1000>;
				interrupts = <0 53 0x04>;
				clocks = <&clks VF610_CLK_ADC0>;
				clock-names = "adc";
				status = "disabled";
			};

			wdog@4003e000 {
				compatible = "fsl,vf610-wdt", "fsl,imx21-wdt";
				reg = <0x4003e000 0x1000>;
				clocks = <&clks VF610_CLK_WDT>;
				clock-names = "wdog";
			};

			qspi0: quadspi@40044000 {
				#address-cells = <1>;
				#size-cells = <0>;
				compatible = "fsl,vf610-qspi";
				reg = <0x40044000 0x1000>;
				interrupts = <0 24 IRQ_TYPE_LEVEL_HIGH>;
				clocks = <&clks VF610_CLK_QSPI0_EN>,
					<&clks VF610_CLK_QSPI0>;
				clock-names = "qspi_en", "qspi";
				status = "disabled";
			};

			iomuxc: iomuxc@40048000 {
				compatible = "fsl,vf610-iomuxc";
				reg = <0x40048000 0x1000>;
				#gpio-range-cells = <3>;
			};

			gpio1: gpio@40049000 {
				compatible = "fsl,vf610-gpio";
				reg = <0x40049000 0x1000 0x400ff000 0x40>;
				interrupts = <0 107 IRQ_TYPE_LEVEL_HIGH>;
				gpio-controller;
				#gpio-cells = <2>;
				interrupt-controller;
				#interrupt-cells = <2>;
				gpio-ranges = <&iomuxc 0 0 32>;
			};

			gpio2: gpio@4004a000 {
				compatible = "fsl,vf610-gpio";
				reg = <0x4004a000 0x1000 0x400ff040 0x40>;
				interrupts = <0 108 IRQ_TYPE_LEVEL_HIGH>;
				gpio-controller;
				#gpio-cells = <2>;
				interrupt-controller;
				#interrupt-cells = <2>;
				gpio-ranges = <&iomuxc 0 32 32>;
			};

			gpio3: gpio@4004b000 {
				compatible = "fsl,vf610-gpio";
				reg = <0x4004b000 0x1000 0x400ff080 0x40>;
				interrupts = <0 109 IRQ_TYPE_LEVEL_HIGH>;
				gpio-controller;
				#gpio-cells = <2>;
				interrupt-controller;
				#interrupt-cells = <2>;
				gpio-ranges = <&iomuxc 0 64 32>;
			};

			gpio4: gpio@4004c000 {
				compatible = "fsl,vf610-gpio";
				reg = <0x4004c000 0x1000 0x400ff0c0 0x40>;
				interrupts = <0 110 IRQ_TYPE_LEVEL_HIGH>;
				gpio-controller;
				#gpio-cells = <2>;
				interrupt-controller;
				#interrupt-cells = <2>;
				gpio-ranges = <&iomuxc 0 96 32>;
			};

			gpio5: gpio@4004d000 {
				compatible = "fsl,vf610-gpio";
				reg = <0x4004d000 0x1000 0x400ff100 0x40>;
				interrupts = <0 111 IRQ_TYPE_LEVEL_HIGH>;
				gpio-controller;
				#gpio-cells = <2>;
				interrupt-controller;
				#interrupt-cells = <2>;
				gpio-ranges = <&iomuxc 0 128 7>;
			};

			anatop@40050000 {
				compatible = "fsl,vf610-anatop";
				reg = <0x40050000 0x1000>;
			};

			i2c0: i2c@40066000 {
				#address-cells = <1>;
				#size-cells = <0>;
				compatible = "fsl,vf610-i2c";
				reg = <0x40066000 0x1000>;
				interrupts =<0 71 IRQ_TYPE_LEVEL_HIGH>;
				clocks = <&clks VF610_CLK_I2C0>;
				clock-names = "ipg";
				dmas = <&edma0 0 50>,
					<&edma0 0 51>;
				dma-names = "rx","tx";
				status = "disabled";
			};

			clks: ccm@4006b000 {
				compatible = "fsl,vf610-ccm";
				reg = <0x4006b000 0x1000>;
				#clock-cells = <1>;
			};
		};

		aips1: aips-bus@40080000 {
			compatible = "fsl,aips-bus", "simple-bus";
			#address-cells = <1>;
			#size-cells = <1>;
			reg = <0x40080000 0x80000>;
			ranges;

			edma1: dma-controller@40098000 {
				#dma-cells = <2>;
				compatible = "fsl,vf610-edma";
				reg = <0x40098000 0x2000>,
					<0x400a1000 0x1000>,
					<0x400a2000 0x1000>;
				interrupts = <0 10 IRQ_TYPE_LEVEL_HIGH>,
						<0 11 IRQ_TYPE_LEVEL_HIGH>;
				interrupt-names = "edma-tx", "edma-err";
				dma-channels = <32>;
				clock-names = "dmamux0", "dmamux1";
				clocks = <&clks VF610_CLK_DMAMUX2>,
					<&clks VF610_CLK_DMAMUX3>;
			};

			uart4: serial@400a9000 {
				compatible = "fsl,vf610-lpuart";
				reg = <0x400a9000 0x1000>;
				interrupts = <0 65 IRQ_TYPE_LEVEL_HIGH>;
				clocks = <&clks VF610_CLK_UART4>;
				clock-names = "ipg";
				status = "disabled";
			};

			uart5: serial@400aa000 {
				compatible = "fsl,vf610-lpuart";
				reg = <0x400aa000 0x1000>;
				interrupts = <0 66 IRQ_TYPE_LEVEL_HIGH>;
				clocks = <&clks VF610_CLK_UART5>;
				clock-names = "ipg";
				status = "disabled";
			};

			adc1: adc@400bb000 {
				compatible = "fsl,vf610-adc";
				reg = <0x400bb000 0x1000>;
				interrupts = <0 54 0x04>;
				clocks = <&clks VF610_CLK_ADC1>;
				clock-names = "adc";
				status = "disabled";
			};

			esdhc1: esdhc@400b2000 {
				compatible = "fsl,imx53-esdhc";
				reg = <0x400b2000 0x4000>;
				interrupts = <0 28 0x04>;
				clocks = <&clks VF610_CLK_IPG_BUS>,
					<&clks VF610_CLK_PLATFORM_BUS>,
					<&clks VF610_CLK_ESDHC1>;
				clock-names = "ipg", "ahb", "per";
				status = "disabled";
			};

			ftm: ftm@400b8000 {
				compatible = "fsl,ftm-timer";
				reg = <0x400b8000 0x1000 0x400b9000 0x1000>;
				interrupts = <0 44 IRQ_TYPE_LEVEL_HIGH>;
				clock-names = "ftm-evt", "ftm-src",
					"ftm-evt-counter-en", "ftm-src-counter-en";
				clocks = <&clks VF610_CLK_FTM2>,
					<&clks VF610_CLK_FTM3>,
					<&clks VF610_CLK_FTM2_EXT_FIX_EN>,
					<&clks VF610_CLK_FTM3_EXT_FIX_EN>;
				status = "disabled";
			};

			fec0: ethernet@400d0000 {
				compatible = "fsl,mvf600-fec";
				reg = <0x400d0000 0x1000>;
				interrupts = <0 78 IRQ_TYPE_LEVEL_HIGH>;
				clocks = <&clks VF610_CLK_ENET0>,
					<&clks VF610_CLK_ENET0>,
					<&clks VF610_CLK_ENET>;
				clock-names = "ipg", "ahb", "ptp";
				status = "disabled";
			};

			fec1: ethernet@400d1000 {
				compatible = "fsl,mvf600-fec";
				reg = <0x400d1000 0x1000>;
				interrupts = <0 79 IRQ_TYPE_LEVEL_HIGH>;
				clocks = <&clks VF610_CLK_ENET1>,
					<&clks VF610_CLK_ENET1>,
					<&clks VF610_CLK_ENET>;
				clock-names = "ipg", "ahb", "ptp";
				status = "disabled";
			};
		};
	};
};
