/*
 * Device Tree Source for OMAP243x SoC
 *
 * Copyright (C) 2012 Texas Instruments Incorporated - http://www.ti.com/
 *
 * This file is licensed under the terms of the GNU General Public License
 * version 2.  This program is licensed "as is" without any warranty of any
 * kind, whether express or implied.
 */

#include "omap2.dtsi"

/ {
	compatible = "ti,omap2430", "ti,omap2";

	ocp {
		prcm: prcm@49006000 {
			compatible = "ti,omap2-prcm";
			reg = <0x49006000 0x1000>;

			prcm_clocks: clocks {
				#address-cells = <1>;
				#size-cells = <0>;
			};

			prcm_clockdomains: clockdomains {
			};
		};

		scrm: scrm@49002000 {
			compatible = "ti,omap2-scrm";
			reg = <0x49002000 0x1000>;

			scrm_clocks: clocks {
				#address-cells = <1>;
				#size-cells = <0>;
			};

			scrm_clockdomains: clockdomains {
			};
		};

		counter32k: counter@49020000 {
			compatible = "ti,omap-counter32k";
			reg = <0x49020000 0x20>;
			ti,hwmods = "counter_32k";
		};

		omap2430_pmx: pinmux@49002030 {
			compatible = "ti,omap2430-padconf", "pinctrl-single";
			reg = <0x49002030 0x0154>;
			#address-cells = <1>;
			#size-cells = <0>;
			pinctrl-single,register-width = <8>;
			pinctrl-single,function-mask = <0x3f>;
		};

		omap2_scm_general: tisyscon@49002270 {
			compatible = "syscon";
			reg = <0x49002270 0x240>;
		};

		pbias_regulator: pbias_regulator {
			compatible = "ti,pbias-omap";
			reg = <0x230 0x4>;
			syscon = <&omap2_scm_general>;
			pbias_mmc_reg: pbias_mmc_omap2430 {
				regulator-name = "pbias_mmc_omap2430";
				regulator-min-microvolt = <1800000>;
				regulator-max-microvolt = <3000000>;
			};
		};

		gpio1: gpio@4900c000 {
			compatible = "ti,omap2-gpio";
			reg = <0x4900c000 0x200>;
			interrupts = <29>;
			ti,hwmods = "gpio1";
			ti,gpio-always-on;
			#gpio-cells = <2>;
			gpio-controller;
			#interrupt-cells = <2>;
			interrupt-controller;
		};

		gpio2: gpio@4900e000 {
			compatible = "ti,omap2-gpio";
			reg = <0x4900e000 0x200>;
			interrupts = <30>;
			ti,hwmods = "gpio2";
			ti,gpio-always-on;
			#gpio-cells = <2>;
			gpio-controller;
			#interrupt-cells = <2>;
			interrupt-controller;
		};

		gpio3: gpio@49010000 {
			compatible = "ti,omap2-gpio";
			reg = <0x49010000 0x200>;
			interrupts = <31>;
			ti,hwmods = "gpio3";
			ti,gpio-always-on;
			#gpio-cells = <2>;
			gpio-controller;
			#interrupt-cells = <2>;
			interrupt-controller;
		};

		gpio4: gpio@49012000 {
			compatible = "ti,omap2-gpio";
			reg = <0x49012000 0x200>;
			interrupts = <32>;
			ti,hwmods = "gpio4";
			ti,gpio-always-on;
			#gpio-cells = <2>;
			gpio-controller;
			#interrupt-cells = <2>;
			interrupt-controller;
		};

		gpio5: gpio@480b6000 {
			compatible = "ti,omap2-gpio";
			reg = <0x480b6000 0x200>;
			interrupts = <33>;
			ti,hwmods = "gpio5";
			#gpio-cells = <2>;
			gpio-controller;
			#interrupt-cells = <2>;
			interrupt-controller;
		};

		gpmc: gpmc@6e000000 {
			compatible = "ti,omap2430-gpmc";
			reg = <0x6e000000 0x1000>;
			#address-cells = <2>;
			#size-cells = <1>;
			interrupts = <20>;
			gpmc,num-cs = <8>;
			gpmc,num-waitpins = <4>;
			ti,hwmods = "gpmc";
		};

		mcbsp1: mcbsp@48074000 {
			compatible = "ti,omap2430-mcbsp";
			reg = <0x48074000 0xff>;
			reg-names = "mpu";
			interrupts = <64>, /* OCP compliant interrupt */
				     <59>, /* TX interrupt */
				     <60>, /* RX interrupt */
				     <61>; /* RX overflow interrupt */
			interrupt-names = "common", "tx", "rx", "rx_overflow";
			ti,buffer-size = <128>;
			ti,hwmods = "mcbsp1";
			dmas = <&sdma 31>,
			       <&sdma 32>;
			dma-names = "tx", "rx";
			status = "disabled";
		};

		mcbsp2: mcbsp@48076000 {
			compatible = "ti,omap2430-mcbsp";
			reg = <0x48076000 0xff>;
			reg-names = "mpu";
			interrupts = <16>, /* OCP compliant interrupt */
				     <62>, /* TX interrupt */
				     <63>; /* RX interrupt */
			interrupt-names = "common", "tx", "rx";
			ti,buffer-size = <128>;
			ti,hwmods = "mcbsp2";
			dmas = <&sdma 33>,
			       <&sdma 34>;
			dma-names = "tx", "rx";
			status = "disabled";
		};

		mcbsp3: mcbsp@4808c000 {
			compatible = "ti,omap2430-mcbsp";
			reg = <0x4808c000 0xff>;
			reg-names = "mpu";
			interrupts = <17>, /* OCP compliant interrupt */
				     <89>, /* TX interrupt */
				     <90>; /* RX interrupt */
			interrupt-names = "common", "tx", "rx";
			ti,buffer-size = <128>;
			ti,hwmods = "mcbsp3";
			dmas = <&sdma 17>,
			       <&sdma 18>;
			dma-names = "tx", "rx";
			status = "disabled";
		};

		mcbsp4: mcbsp@4808e000 {
			compatible = "ti,omap2430-mcbsp";
			reg = <0x4808e000 0xff>;
			reg-names = "mpu";
			interrupts = <18>, /* OCP compliant interrupt */
				     <54>, /* TX interrupt */
				     <55>; /* RX interrupt */
			interrupt-names = "common", "tx", "rx";
			ti,buffer-size = <128>;
			ti,hwmods = "mcbsp4";
			dmas = <&sdma 19>,
			       <&sdma 20>;
			dma-names = "tx", "rx";
			status = "disabled";
		};

		mcbsp5: mcbsp@48096000 {
			compatible = "ti,omap2430-mcbsp";
			reg = <0x48096000 0xff>;
			reg-names = "mpu";
			interrupts = <19>, /* OCP compliant interrupt */
				     <81>, /* TX interrupt */
				     <82>; /* RX interrupt */
			interrupt-names = "common", "tx", "rx";
			ti,buffer-size = <128>;
			ti,hwmods = "mcbsp5";
			dmas = <&sdma 21>,
			       <&sdma 22>;
			dma-names = "tx", "rx";
			status = "disabled";
		};

		mmc1: mmc@4809c000 {
			compatible = "ti,omap2-hsmmc";
			reg = <0x4809c000 0x200>;
			interrupts = <83>;
			ti,hwmods = "mmc1";
			ti,dual-volt;
			dmas = <&sdma 61>, <&sdma 62>;
			dma-names = "tx", "rx";
			pbias-supply = <&pbias_mmc_reg>;
		};

		mmc2: mmc@480b4000 {
			compatible = "ti,omap2-hsmmc";
			reg = <0x480b4000 0x200>;
			interrupts = <86>;
			ti,hwmods = "mmc2";
			dmas = <&sdma 47>, <&sdma 48>;
			dma-names = "tx", "rx";
		};

		mailbox: mailbox@48094000 {
			compatible = "ti,omap2-mailbox";
			reg = <0x48094000 0x200>;
			interrupts = <26>;
			ti,hwmods = "mailbox";
		};

		timer1: timer@49018000 {
			compatible = "ti,omap2420-timer";
			reg = <0x49018000 0x400>;
			interrupts = <37>;
			ti,hwmods = "timer1";
			ti,timer-alwon;
		};

		mcspi3: mcspi@480b8000 {
			compatible = "ti,omap2-mcspi";
			ti,hwmods = "mcspi3";
			reg = <0x480b8000 0x100>;
			interrupts = <91>;
			dmas = <&sdma 15 &sdma 16 &sdma 23 &sdma 24>;
			dma-names = "tx0", "rx0", "tx1", "rx1";
		};

		usb_otg_hs: usb_otg_hs@480ac000 {
			compatible = "ti,omap2-musb";
			ti,hwmods = "usb_otg_hs";
			reg = <0x480ac000 0x1000>;
			interrupts = <93>;
		};

		wd_timer2: wdt@49016000 {
			compatible = "ti,omap2-wdt";
			ti,hwmods = "wd_timer2";
			reg = <0x49016000 0x80>;
		};
	};
};

&i2c1 {
	compatible = "ti,omap2430-i2c";
};

&i2c2 {
	compatible = "ti,omap2430-i2c";
};
