/dts-v1/;

#include "tegra30.dtsi"

/ {
	model = "NVIDIA Tegra30 Beaver evaluation board";
	compatible = "nvidia,beaver", "nvidia,tegra30";

	aliases {
		rtc0 = "/i2c@7000d000/tps65911@2d";
		rtc1 = "/rtc@7000e000";
	};

	memory {
		reg = <0x80000000 0x7ff00000>;
	};

	pcie-controller@00003000 {
		status = "okay";
		pex-clk-supply = <&sys_3v3_pexs_reg>;
		vdd-supply = <&ldo1_reg>;
		avdd-supply = <&ldo2_reg>;

		pci@1,0 {
			status = "okay";
			nvidia,num-lanes = <2>;
		};

		pci@2,0 {
			nvidia,num-lanes = <2>;
		};

		pci@3,0 {
			status = "okay";
			nvidia,num-lanes = <2>;
		};
	};

	host1x@50000000 {
		hdmi@54280000 {
			status = "okay";

			hdmi-supply = <&vdd_5v0_hdmi>;
			vdd-supply = <&sys_3v3_reg>;
			pll-supply = <&vio_reg>;

			nvidia,hpd-gpio =
				<&gpio TEGRA_GPIO(N, 7) GPIO_ACTIVE_HIGH>;
			nvidia,ddc-i2c-bus = <&hdmiddc>;
		};
	};

	pinmux@70000868 {
		pinctrl-names = "default";
		pinctrl-0 = <&state_default>;

		state_default: pinmux {
			sdmmc1_clk_pz0 {
				nvidia,pins = "sdmmc1_clk_pz0";
				nvidia,function = "sdmmc1";
				nvidia,pull = <TEGRA_PIN_PULL_NONE>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
			};
			sdmmc1_cmd_pz1 {
				nvidia,pins =	"sdmmc1_cmd_pz1",
						"sdmmc1_dat0_py7",
						"sdmmc1_dat1_py6",
						"sdmmc1_dat2_py5",
						"sdmmc1_dat3_py4";
				nvidia,function = "sdmmc1";
				nvidia,pull = <TEGRA_PIN_PULL_UP>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
			};
			sdmmc3_clk_pa6 {
				nvidia,pins = "sdmmc3_clk_pa6";
				nvidia,function = "sdmmc3";
				nvidia,pull = <TEGRA_PIN_PULL_NONE>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
			};
			sdmmc3_cmd_pa7 {
				nvidia,pins =	"sdmmc3_cmd_pa7",
						"sdmmc3_dat0_pb7",
						"sdmmc3_dat1_pb6",
						"sdmmc3_dat2_pb5",
						"sdmmc3_dat3_pb4";
				nvidia,function = "sdmmc3";
				nvidia,pull = <TEGRA_PIN_PULL_UP>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
			};
			sdmmc4_clk_pcc4 {
				nvidia,pins =	"sdmmc4_clk_pcc4",
						"sdmmc4_rst_n_pcc3";
				nvidia,function = "sdmmc4";
				nvidia,pull = <TEGRA_PIN_PULL_NONE>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
			};
			sdmmc4_dat0_paa0 {
				nvidia,pins =	"sdmmc4_dat0_paa0",
						"sdmmc4_dat1_paa1",
						"sdmmc4_dat2_paa2",
						"sdmmc4_dat3_paa3",
						"sdmmc4_dat4_paa4",
						"sdmmc4_dat5_paa5",
						"sdmmc4_dat6_paa6",
						"sdmmc4_dat7_paa7";
				nvidia,function = "sdmmc4";
				nvidia,pull = <TEGRA_PIN_PULL_UP>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
			};
			dap2_fs_pa2 {
				nvidia,pins =	"dap2_fs_pa2",
						"dap2_sclk_pa3",
						"dap2_din_pa4",
						"dap2_dout_pa5";
				nvidia,function = "i2s1";
				nvidia,pull = <TEGRA_PIN_PULL_NONE>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
			};
			pex_l1_prsnt_n_pdd4 {
				nvidia,pins =	"pex_l1_prsnt_n_pdd4",
						"pex_l1_clkreq_n_pdd6";
				nvidia,pull = <TEGRA_PIN_PULL_UP>;
			};
			sdio3 {
				nvidia,pins = "drive_sdio3";
				nvidia,high-speed-mode = <TEGRA_PIN_DISABLE>;
				nvidia,schmitt = <TEGRA_PIN_DISABLE>;
				nvidia,pull-down-strength = <46>;
				nvidia,pull-up-strength = <42>;
				nvidia,slew-rate-rising = <1>;
				nvidia,slew-rate-falling = <1>;
			};
			gpv {
				nvidia,pins = "drive_gpv";
				nvidia,pull-up-strength = <16>;
			};
		};
	};

	serial@70006000 {
		status = "okay";
	};

	i2c@7000c000 {
		status = "okay";
		clock-frequency = <100000>;
	};

	i2c@7000c400 {
		status = "okay";
		clock-frequency = <100000>;
	};

	i2c@7000c500 {
		status = "okay";
		clock-frequency = <100000>;
	};

	hdmiddc: i2c@7000c700 {
		status = "okay";
		clock-frequency = <100000>;
	};

	i2c@7000d000 {
		status = "okay";
		clock-frequency = <100000>;

		rt5640: rt5640@1c {
			compatible = "realtek,rt5640";
			reg = <0x1c>;
			interrupt-parent = <&gpio>;
			interrupts = <TEGRA_GPIO(X, 3) GPIO_ACTIVE_HIGH>;
			realtek,ldo1-en-gpios =
				<&gpio TEGRA_GPIO(X, 2) GPIO_ACTIVE_HIGH>;
		};

		pmic: tps65911@2d {
			compatible = "ti,tps65911";
			reg = <0x2d>;

			interrupts = <GIC_SPI 86 IRQ_TYPE_LEVEL_HIGH>;
			#interrupt-cells = <2>;
			interrupt-controller;

			ti,system-power-controller;

			#gpio-cells = <2>;
			gpio-controller;

			vcc1-supply = <&vdd_5v_in_reg>;
			vcc2-supply = <&vdd_5v_in_reg>;
			vcc3-supply = <&vio_reg>;
			vcc4-supply = <&vdd_5v_in_reg>;
			vcc5-supply = <&vdd_5v_in_reg>;
			vcc6-supply = <&vdd2_reg>;
			vcc7-supply = <&vdd_5v_in_reg>;
			vccio-supply = <&vdd_5v_in_reg>;

			regulators {
				#address-cells = <1>;
				#size-cells = <0>;

				vdd1_reg: vdd1 {
					regulator-name = "vddio_ddr_1v2";
					regulator-min-microvolt = <1200000>;
					regulator-max-microvolt = <1200000>;
					regulator-always-on;
				};

				vdd2_reg: vdd2 {
					regulator-name = "vdd_1v5_gen";
					regulator-min-microvolt = <1500000>;
					regulator-max-microvolt = <1500000>;
					regulator-always-on;
				};

				vddctrl_reg: vddctrl {
					regulator-name = "vdd_cpu,vdd_sys";
					regulator-min-microvolt = <1000000>;
					regulator-max-microvolt = <1000000>;
					regulator-always-on;
				};

				vio_reg: vio {
					regulator-name = "vdd_1v8_gen";
					regulator-min-microvolt = <1800000>;
					regulator-max-microvolt = <1800000>;
					regulator-always-on;
				};

				ldo1_reg: ldo1 {
					regulator-name = "vdd_pexa,vdd_pexb";
					regulator-min-microvolt = <1050000>;
					regulator-max-microvolt = <1050000>;
				};

				ldo2_reg: ldo2 {
					regulator-name = "vdd_sata,avdd_plle";
					regulator-min-microvolt = <1050000>;
					regulator-max-microvolt = <1050000>;
				};

				/* LDO3 is not connected to anything */

				ldo4_reg: ldo4 {
					regulator-name = "vdd_rtc";
					regulator-min-microvolt = <1200000>;
					regulator-max-microvolt = <1200000>;
					regulator-always-on;
				};

				ldo5_reg: ldo5 {
					regulator-name = "vddio_sdmmc,avdd_vdac";
					regulator-min-microvolt = <3300000>;
					regulator-max-microvolt = <3300000>;
					regulator-always-on;
				};

				ldo6_reg: ldo6 {
					regulator-name = "avdd_dsi_csi,pwrdet_mipi";
					regulator-min-microvolt = <1200000>;
					regulator-max-microvolt = <1200000>;
				};

				ldo7_reg: ldo7 {
					regulator-name = "vdd_pllm,x,u,a_p_c_s";
					regulator-min-microvolt = <1200000>;
					regulator-max-microvolt = <1200000>;
					regulator-always-on;
				};

				ldo8_reg: ldo8 {
					regulator-name = "vdd_ddr_hs";
					regulator-min-microvolt = <1000000>;
					regulator-max-microvolt = <1000000>;
					regulator-always-on;
				};
			};
		};

		tps62361@60 {
			compatible = "ti,tps62361";
			reg = <0x60>;

			regulator-name = "tps62361-vout";
			regulator-min-microvolt = <500000>;
			regulator-max-microvolt = <1500000>;
			regulator-boot-on;
			regulator-always-on;
			ti,vsel0-state-high;
			ti,vsel1-state-high;
		};
	};

	spi@7000da00 {
		status = "okay";
		spi-max-frequency = <25000000>;
		spi-flash@1 {
			compatible = "winbond,w25q32";
			reg = <1>;
			spi-max-frequency = <20000000>;
		};
	};

	pmc@7000e400 {
		status = "okay";
		nvidia,invert-interrupt;
		nvidia,suspend-mode = <1>;
		nvidia,cpu-pwr-good-time = <2000>;
		nvidia,cpu-pwr-off-time = <200>;
		nvidia,core-pwr-good-time = <3845 3845>;
		nvidia,core-pwr-off-time = <0>;
		nvidia,core-power-req-active-high;
		nvidia,sys-clock-req-active-high;
	};

	ahub@70080000 {
		i2s@70080400 {
			status = "okay";
		};
	};

	sdhci@78000000 {
		status = "okay";
		cd-gpios = <&gpio TEGRA_GPIO(I, 5) GPIO_ACTIVE_LOW>;
		wp-gpios = <&gpio TEGRA_GPIO(T, 3) GPIO_ACTIVE_HIGH>;
		power-gpios = <&gpio TEGRA_GPIO(D, 7) GPIO_ACTIVE_HIGH>;
		bus-width = <4>;
	};

	sdhci@78000600 {
		status = "okay";
		bus-width = <8>;
		non-removable;
	};

	usb@7d004000 {
		status = "okay";
	};

	phy2: usb-phy@7d004000 {
		vbus-supply = <&sys_3v3_reg>;
		status = "okay";
	};

	usb@7d008000 {
		status = "okay";
	};

	usb-phy@7d008000 {
		vbus-supply = <&usb3_vbus_reg>;
		status = "okay";
	};

	clocks {
		compatible = "simple-bus";
		#address-cells = <1>;
		#size-cells = <0>;

		clk32k_in: clock@0 {
			compatible = "fixed-clock";
			reg=<0>;
			#clock-cells = <0>;
			clock-frequency = <32768>;
		};
	};

	gpio-leds {
		compatible = "gpio-leds";

		gpled1 {
			label = "LED1"; /* CR5A1 (blue) */
			gpios = <&gpio TEGRA_GPIO(L, 1) GPIO_ACTIVE_HIGH>;
		};
		gpled2 {
			label = "LED2"; /* CR4A2 (green) */
			gpios = <&gpio TEGRA_GPIO(L, 0) GPIO_ACTIVE_HIGH>;
		};
	};

	regulators {
		compatible = "simple-bus";
		#address-cells = <1>;
		#size-cells = <0>;

		vdd_5v_in_reg: regulator@0 {
			compatible = "regulator-fixed";
			reg = <0>;
			regulator-name = "vdd_5v_in";
			regulator-min-microvolt = <5000000>;
			regulator-max-microvolt = <5000000>;
			regulator-always-on;
		};

		chargepump_5v_reg: regulator@1 {
			compatible = "regulator-fixed";
			reg = <1>;
			regulator-name = "chargepump_5v";
			regulator-min-microvolt = <5000000>;
			regulator-max-microvolt = <5000000>;
			regulator-boot-on;
			regulator-always-on;
			enable-active-high;
			gpio = <&pmic 0 GPIO_ACTIVE_HIGH>;
		};

		ddr_reg: regulator@2 {
			compatible = "regulator-fixed";
			reg = <2>;
			regulator-name = "vdd_ddr";
			regulator-min-microvolt = <1500000>;
			regulator-max-microvolt = <1500000>;
			regulator-always-on;
			regulator-boot-on;
			enable-active-high;
			gpio = <&pmic 7 GPIO_ACTIVE_HIGH>;
			vin-supply = <&vdd_5v_in_reg>;
		};

		vdd_5v_sata_reg: regulator@3 {
			compatible = "regulator-fixed";
			reg = <3>;
			regulator-name = "vdd_5v_sata";
			regulator-min-microvolt = <5000000>;
			regulator-max-microvolt = <5000000>;
			regulator-always-on;
			regulator-boot-on;
			enable-active-high;
			gpio = <&gpio TEGRA_GPIO(D, 6) GPIO_ACTIVE_HIGH>;
			vin-supply = <&vdd_5v_in_reg>;
		};

		usb1_vbus_reg: regulator@4 {
			compatible = "regulator-fixed";
			reg = <4>;
			regulator-name = "usb1_vbus";
			regulator-min-microvolt = <5000000>;
			regulator-max-microvolt = <5000000>;
			enable-active-high;
			gpio = <&gpio TEGRA_GPIO(DD, 6) GPIO_ACTIVE_HIGH>;
			gpio-open-drain;
			vin-supply = <&vdd_5v_in_reg>;
		};

		usb3_vbus_reg: regulator@5 {
			compatible = "regulator-fixed";
			reg = <5>;
			regulator-name = "usb3_vbus";
			regulator-min-microvolt = <5000000>;
			regulator-max-microvolt = <5000000>;
			enable-active-high;
			gpio = <&gpio TEGRA_GPIO(DD, 4) GPIO_ACTIVE_HIGH>;
			gpio-open-drain;
			vin-supply = <&vdd_5v_in_reg>;
		};

		sys_3v3_reg: regulator@6 {
			compatible = "regulator-fixed";
			reg = <6>;
			regulator-name = "sys_3v3,vdd_3v3_alw";
			regulator-min-microvolt = <3300000>;
			regulator-max-microvolt = <3300000>;
			regulator-always-on;
			regulator-boot-on;
			enable-active-high;
			gpio = <&pmic 6 GPIO_ACTIVE_HIGH>;
			vin-supply = <&vdd_5v_in_reg>;
		};

		sys_3v3_pexs_reg: regulator@7 {
			compatible = "regulator-fixed";
			reg = <7>;
			regulator-name = "sys_3v3_pexs";
			regulator-min-microvolt = <3300000>;
			regulator-max-microvolt = <3300000>;
			regulator-always-on;
			regulator-boot-on;
			enable-active-high;
			gpio = <&gpio TEGRA_GPIO(L, 7) GPIO_ACTIVE_HIGH>;
			vin-supply = <&sys_3v3_reg>;
		};

		vdd_5v0_hdmi: regulator@8 {
			compatible = "regulator-fixed";
			reg = <8>;
			regulator-name = "+VDD_5V_HDMI";
			regulator-min-microvolt = <5000000>;
			regulator-max-microvolt = <5000000>;
			regulator-always-on;
			regulator-boot-on;
			vin-supply = <&sys_3v3_reg>;
		};
	};

	sound {
		compatible = "nvidia,tegra-audio-rt5640-beaver",
			     "nvidia,tegra-audio-rt5640";
		nvidia,model = "NVIDIA Tegra Beaver";

		nvidia,audio-routing =
			"Headphones", "HPOR",
			"Headphones", "HPOL",
			"Mic Jack", "MICBIAS1",
			"IN2P", "Mic Jack";

		nvidia,i2s-controller = <&tegra_i2s1>;
		nvidia,audio-codec = <&rt5640>;

		nvidia,hp-det-gpios = <&gpio TEGRA_GPIO(W, 2) GPIO_ACTIVE_HIGH>;

		clocks = <&tegra_car TEGRA30_CLK_PLL_A>,
			 <&tegra_car TEGRA30_CLK_PLL_A_OUT0>,
			 <&tegra_car TEGRA30_CLK_EXTERN1>;
		clock-names = "pll_a", "pll_a_out0", "mclk";
	};
};
