/*
 * Copyright 2013 Freescale Semiconductor, Inc.
 * Copyright 2013 Linaro Limited
 *
 * This program is free software; you can redistribute it and/or modify
 * it under the terms of the GNU General Public License as published by
 * the Free Software Foundation; either version 2 of the License, or
 * (at your option) any later version.
 */

/dts-v1/;
#include "vf610.dtsi"

/ {
	model = "PHYTEC Cosmic/Cosmic+ Board";
	compatible = "phytec,vf610-cosmic", "fsl,vf610";

	chosen {
		bootargs = "console=ttyLP1,115200";
	};

	memory {
		reg = <0x80000000 0x10000000>;
	};

	clocks {
		enet_ext {
			compatible = "fixed-clock";
			#clock-cells = <0>;
			clock-frequency = <50000000>;
		};
	};

};

&fec1 {
	phy-mode = "rmii";
	pinctrl-names = "default";
	pinctrl-0 = <&pinctrl_fec1>;
	status = "okay";
};

&iomuxc {
	vf610-cosmic {
		pinctrl_fec1: fec1grp {
			fsl,pins = <
				VF610_PAD_PTC9__ENET_RMII1_MDC		0x30d2
				VF610_PAD_PTC10__ENET_RMII1_MDIO	0x30d3
				VF610_PAD_PTC11__ENET_RMII1_CRS		0x30d1
				VF610_PAD_PTC12__ENET_RMII_RXD1		0x30d1
				VF610_PAD_PTC13__ENET_RMII1_RXD0	0x30d1
				VF610_PAD_PTC14__ENET_RMII1_RXER	0x30d1
				VF610_PAD_PTC15__ENET_RMII1_TXD1	0x30d2
				VF610_PAD_PTC16__ENET_RMII1_TXD0	0x30d2
				VF610_PAD_PTC17__ENET_RMII1_TXEN	0x30d2
			>;
		};

		pinctrl_uart1: uart1grp {
			fsl,pins = <
				VF610_PAD_PTB4__UART1_TX		0x21a2
				VF610_PAD_PTB5__UART1_RX		0x21a1
			>;
		};
	};
};

&uart1 {
	pinctrl-names = "default";
	pinctrl-0 = <&pinctrl_uart1>;
	status = "okay";
};
