/*
 * Copyright 2012 Sascha Hauer <s.hauer@pengutronix.de>, Pengutronix
 * Copyright 2012 Steffen Trumtrar <s.trumtrar@pengutronix.de>, Pengutronix
 *
 * The code contained herein is licensed under the GNU General Public
 * License. You may obtain a copy of the GNU General Public License
 * Version 2 or later at the following locations:
 *
 * http://www.opensource.org/licenses/gpl-license.html
 * http://www.gnu.org/copyleft/gpl.html
 */

#include <arm/imx53-mba53.dts>

/ {
	chosen {
		linux,stdout-path = &uart2;

		environment-sd {
			compatible = "barebox,environment";
			device-path = &esdhc2, "partname:environment";
			status = "disabled";
		};
	};
};

&esdhc2 {
	#address-cells = <1>;
	#size-cells = <1>;

	partition@0 {
		label = "environment";
		reg = <0x80000 0x80000>;
	};
};

&usbh1 {
	phy_type = "utmi";
};

&usbotg {
	phy_type = "utmi";
};
