/*
 * Copyright 2013 ST-Ericsson AB
 *
 * The code contained herein is licensed under the GNU General Public
 * License. You may obtain a copy of the GNU General Public License
 * Version 2 or later at the following locations:
 *
 * http://www.opensource.org/licenses/gpl-license.html
 * http://www.gnu.org/copyleft/gpl.html
 */

/dts-v1/;
#include "ste-dbx5x0.dtsi"
#include "ste-ccu8540-pinctrl.dtsi"

/ {
	model = "ST-Ericsson U8540 platform with Device Tree";
	compatible = "st-ericsson,ccu8540", "st-ericsson,u8540";

	memory@0 {
		device_type = "memory";
		reg = <0x20000000 0x1f000000>, <0xc0000000 0x3f000000>;
	};

	soc {
		pinctrl {
			compatible = "stericsson,db8540-pinctrl";
		};

		prcmu@80157000 {
			reg = <0x80157000 0x2000>, <0x801b0000 0x8000>, <0x801b8000 0x3000>;
			reg-names = "prcmu", "prcmu-tcpm", "prcmu-tcdm";
		};

		uart@80120000 {
			pinctrl-names = "default", "sleep";
			pinctrl-0 = <&uart0_default_mux>, <&uart0_default_mode>;
			pinctrl-1 = <&uart0_sleep_mode>;
			status = "okay";
		};

		uart@80121000 {
			status = "okay";
		};

		uart@80007000 {
			pinctrl-names = "default", "sleep";
			pinctrl-0 = <&uart2_default_mode>;
			pinctrl-1 = <&uart2_sleep_mode>;
			status = "okay";
		};

		i2c0: i2c@80004000 {
			pinctrl-names = "default","sleep";
			pinctrl-0 = <&i2c0_default_mux>, <&i2c0_default_mode>;
			pinctrl-1 = <&i2c0_sleep_mode>;
		};

		i2c1: i2c@80122000 {
			pinctrl-names = "default","sleep";
			pinctrl-0 = <&i2c1_default_mux>, <&i2c1_default_mode>;
			pinctrl-1 = <&i2c1_sleep_mode>;
		};

		i2c2: i2c@80128000 {
			pinctrl-names = "default","sleep";
			pinctrl-0 = <&i2c2_default_mux>, <&i2c2_default_mode>;
			pinctrl-1 = <&i2c2_sleep_mode>;
		};

		i2c3: i2c@80110000 {
			status = "disabled";
		};

		i2c4: i2c@8012a000 {
			pinctrl-names = "default","sleep";
			pinctrl-0 = <&i2c4_default_mux>, <&i2c4_default_mode>;
			pinctrl-1 = <&i2c4_sleep_mode>;
		};

		i2c5: i2c@80001000 {
			pinctrl-names = "default","sleep";
			pinctrl-0 = <&i2c5_default_mux>, <&i2c5_default_mode>;
			pinctrl-1 = <&i2c5_sleep_mode>;
		};
	};
};
