/*
 * Device Tree Source for the Lager board
 *
 * Copyright (C) 2013-2014 Renesas Solutions Corp.
 * Copyright (C) 2014 Cogent Embedded, Inc.
 *
 * This file is licensed under the terms of the GNU General Public License
 * version 2.  This program is licensed "as is" without any warranty of any
 * kind, whether express or implied.
 */

/dts-v1/;
#include "r8a7790.dtsi"
#include <dt-bindings/gpio/gpio.h>
#include <dt-bindings/input/input.h>

/ {
	model = "Lager";
	compatible = "renesas,lager", "renesas,r8a7790";

	aliases {
		serial6 = &scif0;
		serial7 = &scif1;
	};

	chosen {
		bootargs = "console=ttySC6,115200 ignore_loglevel rw root=/dev/nfs ip=dhcp";
	};

	memory@40000000 {
		device_type = "memory";
		reg = <0 0x40000000 0 0x80000000>;
	};

	memory@180000000 {
		device_type = "memory";
		reg = <1 0x80000000 0 0x80000000>;
	};

	lbsc {
		#address-cells = <1>;
		#size-cells = <1>;
	};

	gpio_keys {
		compatible = "gpio-keys";

		button@1 {
			linux,code = <KEY_1>;
			label = "SW2-1";
			gpio-key,wakeup;
			debounce-interval = <20>;
			gpios = <&gpio1 14 GPIO_ACTIVE_LOW>;
		};
		button@2 {
			linux,code = <KEY_2>;
			label = "SW2-2";
			gpio-key,wakeup;
			debounce-interval = <20>;
			gpios = <&gpio1 24 GPIO_ACTIVE_LOW>;
		};
		button@3 {
			linux,code = <KEY_3>;
			label = "SW2-3";
			gpio-key,wakeup;
			debounce-interval = <20>;
			gpios = <&gpio1 26 GPIO_ACTIVE_LOW>;
		};
		button@4 {
			linux,code = <KEY_4>;
			label = "SW2-4";
			gpio-key,wakeup;
			debounce-interval = <20>;
			gpios = <&gpio1 28 GPIO_ACTIVE_LOW>;
		};
	};

	leds {
		compatible = "gpio-leds";
		led6 {
			gpios = <&gpio4 22 GPIO_ACTIVE_HIGH>;
		};
		led7 {
			gpios = <&gpio4 23 GPIO_ACTIVE_HIGH>;
		};
		led8 {
			gpios = <&gpio5 17 GPIO_ACTIVE_HIGH>;
		};
	};

	fixedregulator3v3: fixedregulator@0 {
		compatible = "regulator-fixed";
		regulator-name = "fixed-3.3V";
		regulator-min-microvolt = <3300000>;
		regulator-max-microvolt = <3300000>;
		regulator-boot-on;
		regulator-always-on;
	};

	vcc_sdhi0: regulator@1 {
		compatible = "regulator-fixed";

		regulator-name = "SDHI0 Vcc";
		regulator-min-microvolt = <3300000>;
		regulator-max-microvolt = <3300000>;

		gpio = <&gpio5 24 GPIO_ACTIVE_HIGH>;
		enable-active-high;
	};

	vccq_sdhi0: regulator@2 {
		compatible = "regulator-gpio";

		regulator-name = "SDHI0 VccQ";
		regulator-min-microvolt = <1800000>;
		regulator-max-microvolt = <3300000>;

		gpios = <&gpio5 29 GPIO_ACTIVE_HIGH>;
		gpios-states = <1>;
		states = <3300000 1
			  1800000 0>;
	};

	vcc_sdhi2: regulator@3 {
		compatible = "regulator-fixed";

		regulator-name = "SDHI2 Vcc";
		regulator-min-microvolt = <3300000>;
		regulator-max-microvolt = <3300000>;

		gpio = <&gpio5 25 GPIO_ACTIVE_HIGH>;
		enable-active-high;
	};

	vccq_sdhi2: regulator@4 {
		compatible = "regulator-gpio";

		regulator-name = "SDHI2 VccQ";
		regulator-min-microvolt = <1800000>;
		regulator-max-microvolt = <3300000>;

		gpios = <&gpio5 30 GPIO_ACTIVE_HIGH>;
		gpios-states = <1>;
		states = <3300000 1
			  1800000 0>;
	};
};

&extal_clk {
	clock-frequency = <20000000>;
};

&pfc {
	pinctrl-0 = <&du_pins>;
	pinctrl-names = "default";

	du_pins: du {
		renesas,groups = "du_rgb666", "du_sync_1", "du_clk_out_0";
		renesas,function = "du";
	};

	scif0_pins: serial0 {
		renesas,groups = "scif0_data";
		renesas,function = "scif0";
	};

	ether_pins: ether {
		renesas,groups = "eth_link", "eth_mdio", "eth_rmii";
		renesas,function = "eth";
	};

	phy1_pins: phy1 {
		renesas,groups = "intc_irq0";
		renesas,function = "intc";
	};

	scif1_pins: serial1 {
		renesas,groups = "scif1_data";
		renesas,function = "scif1";
	};

	sdhi0_pins: sd0 {
		renesas,groups = "sdhi0_data4", "sdhi0_ctrl";
		renesas,function = "sdhi0";
	};

	sdhi2_pins: sd2 {
		renesas,groups = "sdhi2_data4", "sdhi2_ctrl";
		renesas,function = "sdhi2";
	};

	mmc1_pins: mmc1 {
		renesas,groups = "mmc1_data8", "mmc1_ctrl";
		renesas,function = "mmc1";
	};

	qspi_pins: spi0 {
		renesas,groups = "qspi_ctrl", "qspi_data4";
		renesas,function = "qspi";
	};

	msiof1_pins: spi2 {
		renesas,groups = "msiof1_clk", "msiof1_sync", "msiof1_rx",
				 "msiof1_tx";
		renesas,function = "msiof1";
	};
};

&ether {
	pinctrl-0 = <&ether_pins &phy1_pins>;
	pinctrl-names = "default";

	phy-handle = <&phy1>;
	renesas,ether-link-active-low;
	status = "ok";

	phy1: ethernet-phy@1 {
		reg = <1>;
		interrupt-parent = <&irqc0>;
		interrupts = <0 IRQ_TYPE_LEVEL_LOW>;
		micrel,led-mode = <1>;
	};
};

&mmcif1 {
	pinctrl-0 = <&mmc1_pins>;
	pinctrl-names = "default";

	vmmc-supply = <&fixedregulator3v3>;
	bus-width = <8>;
	non-removable;
	status = "okay";
};

&sata1 {
	status = "okay";
};

&qspi {
	pinctrl-0 = <&qspi_pins>;
	pinctrl-names = "default";

	status = "okay";

	flash: flash@0 {
		#address-cells = <1>;
		#size-cells = <1>;
		compatible = "spansion,s25fl512s";
		reg = <0>;
		spi-max-frequency = <30000000>;
		spi-tx-bus-width = <4>;
		spi-rx-bus-width = <4>;
		m25p,fast-read;

		partition@0 {
			label = "loader";
			reg = <0x00000000 0x00040000>;
			read-only;
		};
		partition@40000 {
			label = "user";
			reg = <0x00040000 0x00400000>;
			read-only;
		};
		partition@440000 {
			label = "flash";
			reg = <0x00440000 0x03bc0000>;
		};
	};
};

&scif0 {
	pinctrl-0 = <&scif0_pins>;
	pinctrl-names = "default";

	status = "okay";
};

&scif1 {
	pinctrl-0 = <&scif1_pins>;
	pinctrl-names = "default";

	status = "okay";
};

&msiof1 {
	pinctrl-0 = <&msiof1_pins>;
	pinctrl-names = "default";

	status = "okay";

	pmic: pmic@0 {
		compatible = "renesas,r2a11302ft";
		reg = <0>;
		spi-max-frequency = <6000000>;
		spi-cpol;
		spi-cpha;
	};
};

&sdhi0 {
	pinctrl-0 = <&sdhi0_pins>;
	pinctrl-names = "default";

	vmmc-supply = <&vcc_sdhi0>;
	vqmmc-supply = <&vccq_sdhi0>;
	cd-gpios = <&gpio3 6 GPIO_ACTIVE_LOW>;
	status = "okay";
};

&sdhi2 {
	pinctrl-0 = <&sdhi2_pins>;
	pinctrl-names = "default";

	vmmc-supply = <&vcc_sdhi2>;
	vqmmc-supply = <&vccq_sdhi2>;
	cd-gpios = <&gpio3 22 GPIO_ACTIVE_LOW>;
	status = "okay";
};
