/*
 * Copyright (C) 2012 Texas Instruments Incorporated - http://www.ti.com/
 *
 * This program is free software; you can redistribute it and/or modify
 * it under the terms of the GNU General Public License version 2 as
 * published by the Free Software Foundation.
 */

/ {
	chosen {
		linux,stdout-path = &uart0;
	};

	cpus {
		cpu@0 {
			cpu0-supply = <&dcdc2_reg>;
		};
	};

	leds {
		pinctrl-names = "default";
		pinctrl-0 = <&user_leds_s0>;

		compatible = "gpio-leds";

		led@2 {
			label = "beaglebone:green:heartbeat";
			gpios = <&gpio1 21 GPIO_ACTIVE_HIGH>;
			linux,default-trigger = "heartbeat";
			default-state = "off";
		};

		led@3 {
			label = "beaglebone:green:mmc0";
			gpios = <&gpio1 22 GPIO_ACTIVE_HIGH>;
			linux,default-trigger = "mmc0";
			default-state = "off";
		};

		led@4 {
			label = "beaglebone:green:usr2";
			gpios = <&gpio1 23 GPIO_ACTIVE_HIGH>;
			linux,default-trigger = "cpu0";
			default-state = "off";
		};

		led@5 {
			label = "beaglebone:green:usr3";
			gpios = <&gpio1 24 GPIO_ACTIVE_HIGH>;
			linux,default-trigger = "mmc1";
			default-state = "off";
		};
	};

	vmmcsd_fixed: fixedregulator@0 {
		compatible = "regulator-fixed";
		regulator-name = "vmmcsd_fixed";
		regulator-min-microvolt = <3300000>;
		regulator-max-microvolt = <3300000>;
	};
};

&am33xx_pinmux {
	pinctrl-names = "default";
	pinctrl-0 = <&clkout2_pin>;

	user_leds_s0: user_leds_s0 {
		pinctrl-single,pins = <
			0x54 (PIN_OUTPUT_PULLDOWN | MUX_MODE7)	/* gpmc_a5.gpio1_21 */
			0x58 (PIN_OUTPUT_PULLUP | MUX_MODE7)	/* gpmc_a6.gpio1_22 */
			0x5c (PIN_OUTPUT_PULLDOWN | MUX_MODE7)	/* gpmc_a7.gpio1_23 */
			0x60 (PIN_OUTPUT_PULLUP | MUX_MODE7)	/* gpmc_a8.gpio1_24 */
		>;
	};

	i2c0_pins: pinmux_i2c0_pins {
		pinctrl-single,pins = <
			0x188 (PIN_INPUT_PULLUP | MUX_MODE0)	/* i2c0_sda.i2c0_sda */
			0x18c (PIN_INPUT_PULLUP | MUX_MODE0)	/* i2c0_scl.i2c0_scl */
		>;
	};

	uart0_pins: pinmux_uart0_pins {
		pinctrl-single,pins = <
			0x170 (PIN_INPUT_PULLUP | MUX_MODE0)	/* uart0_rxd.uart0_rxd */
			0x174 (PIN_OUTPUT_PULLDOWN | MUX_MODE0)	/* uart0_txd.uart0_txd */
		>;
	};

	clkout2_pin: pinmux_clkout2_pin {
		pinctrl-single,pins = <
			0x1b4 (PIN_OUTPUT_PULLDOWN | MUX_MODE3)	/* xdma_event_intr1.clkout2 */
		>;
	};

	cpsw_default: cpsw_default {
		pinctrl-single,pins = <
			/* Slave 1 */
			0x110 (PIN_INPUT_PULLUP | MUX_MODE0)	/* mii1_rxerr.mii1_rxerr */
			0x114 (PIN_OUTPUT_PULLDOWN | MUX_MODE0)	/* mii1_txen.mii1_txen */
			0x118 (PIN_INPUT_PULLUP | MUX_MODE0)	/* mii1_rxdv.mii1_rxdv */
			0x11c (PIN_OUTPUT_PULLDOWN | MUX_MODE0)	/* mii1_txd3.mii1_txd3 */
			0x120 (PIN_OUTPUT_PULLDOWN | MUX_MODE0)	/* mii1_txd2.mii1_txd2 */
			0x124 (PIN_OUTPUT_PULLDOWN | MUX_MODE0)	/* mii1_txd1.mii1_txd1 */
			0x128 (PIN_OUTPUT_PULLDOWN | MUX_MODE0)	/* mii1_txd0.mii1_txd0 */
			0x12c (PIN_INPUT_PULLUP | MUX_MODE0)	/* mii1_txclk.mii1_txclk */
			0x130 (PIN_INPUT_PULLUP | MUX_MODE0)	/* mii1_rxclk.mii1_rxclk */
			0x134 (PIN_INPUT_PULLUP | MUX_MODE0)	/* mii1_rxd3.mii1_rxd3 */
			0x138 (PIN_INPUT_PULLUP | MUX_MODE0)	/* mii1_rxd2.mii1_rxd2 */
			0x13c (PIN_INPUT_PULLUP | MUX_MODE0)	/* mii1_rxd1.mii1_rxd1 */
			0x140 (PIN_INPUT_PULLUP | MUX_MODE0)	/* mii1_rxd0.mii1_rxd0 */
		>;
	};

	cpsw_sleep: cpsw_sleep {
		pinctrl-single,pins = <
			/* Slave 1 reset value */
			0x110 (PIN_INPUT_PULLDOWN | MUX_MODE7)
			0x114 (PIN_INPUT_PULLDOWN | MUX_MODE7)
			0x118 (PIN_INPUT_PULLDOWN | MUX_MODE7)
			0x11c (PIN_INPUT_PULLDOWN | MUX_MODE7)
			0x120 (PIN_INPUT_PULLDOWN | MUX_MODE7)
			0x124 (PIN_INPUT_PULLDOWN | MUX_MODE7)
			0x128 (PIN_INPUT_PULLDOWN | MUX_MODE7)
			0x12c (PIN_INPUT_PULLDOWN | MUX_MODE7)
			0x130 (PIN_INPUT_PULLDOWN | MUX_MODE7)
			0x134 (PIN_INPUT_PULLDOWN | MUX_MODE7)
			0x138 (PIN_INPUT_PULLDOWN | MUX_MODE7)
			0x13c (PIN_INPUT_PULLDOWN | MUX_MODE7)
			0x140 (PIN_INPUT_PULLDOWN | MUX_MODE7)
		>;
	};

	davinci_mdio_default: davinci_mdio_default {
		pinctrl-single,pins = <
			/* MDIO */
			0x148 (PIN_INPUT_PULLUP | SLEWCTRL_FAST | MUX_MODE0)	/* mdio_data.mdio_data */
			0x14c (PIN_OUTPUT_PULLUP | MUX_MODE0)			/* mdio_clk.mdio_clk */
		>;
	};

	davinci_mdio_sleep: davinci_mdio_sleep {
		pinctrl-single,pins = <
			/* MDIO reset value */
			0x148 (PIN_INPUT_PULLDOWN | MUX_MODE7)
			0x14c (PIN_INPUT_PULLDOWN | MUX_MODE7)
		>;
	};

	mmc1_pins: pinmux_mmc1_pins {
		pinctrl-single,pins = <
			0x160 (PIN_INPUT | MUX_MODE7) /* GPIO0_6 */
		>;
	};

	emmc_pins: pinmux_emmc_pins {
		pinctrl-single,pins = <
			0x80 (PIN_INPUT_PULLUP | MUX_MODE2) /* gpmc_csn1.mmc1_clk */
			0x84 (PIN_INPUT_PULLUP | MUX_MODE2) /* gpmc_csn2.mmc1_cmd */
			0x00 (PIN_INPUT_PULLUP | MUX_MODE1) /* gpmc_ad0.mmc1_dat0 */
			0x04 (PIN_INPUT_PULLUP | MUX_MODE1) /* gpmc_ad1.mmc1_dat1 */
			0x08 (PIN_INPUT_PULLUP | MUX_MODE1) /* gpmc_ad2.mmc1_dat2 */
			0x0c (PIN_INPUT_PULLUP | MUX_MODE1) /* gpmc_ad3.mmc1_dat3 */
			0x10 (PIN_INPUT_PULLUP | MUX_MODE1) /* gpmc_ad4.mmc1_dat4 */
			0x14 (PIN_INPUT_PULLUP | MUX_MODE1) /* gpmc_ad5.mmc1_dat5 */
			0x18 (PIN_INPUT_PULLUP | MUX_MODE1) /* gpmc_ad6.mmc1_dat6 */
			0x1c (PIN_INPUT_PULLUP | MUX_MODE1) /* gpmc_ad7.mmc1_dat7 */
		>;
	};
};

&uart0 {
	pinctrl-names = "default";
	pinctrl-0 = <&uart0_pins>;

	status = "okay";
};

&usb {
	status = "okay";

	control@44e10000 {
		status = "okay";
	};

	usb-phy@47401300 {
		status = "okay";
	};

	usb-phy@47401b00 {
		status = "okay";
	};

	usb@47401000 {
		status = "okay";
	};

	usb@47401800 {
		status = "okay";
		dr_mode = "host";
	};

	dma-controller@07402000  {
		status = "okay";
	};
};

&i2c0 {
	pinctrl-names = "default";
	pinctrl-0 = <&i2c0_pins>;

	status = "okay";
	clock-frequency = <400000>;

	tps: tps@24 {
		reg = <0x24>;
	};

};

/include/ "tps65217.dtsi"

&tps {
	regulators {
		dcdc1_reg: regulator@0 {
			regulator-always-on;
		};

		dcdc2_reg: regulator@1 {
			/* VDD_MPU voltage limits 0.95V - 1.26V with +/-4% tolerance */
			regulator-name = "vdd_mpu";
			regulator-min-microvolt = <925000>;
			regulator-max-microvolt = <1325000>;
			regulator-boot-on;
			regulator-always-on;
		};

		dcdc3_reg: regulator@2 {
			/* VDD_CORE voltage limits 0.95V - 1.1V with +/-4% tolerance */
			regulator-name = "vdd_core";
			regulator-min-microvolt = <925000>;
			regulator-max-microvolt = <1150000>;
			regulator-boot-on;
			regulator-always-on;
		};

		ldo1_reg: regulator@3 {
			regulator-always-on;
		};

		ldo2_reg: regulator@4 {
			regulator-always-on;
		};

		ldo3_reg: regulator@5 {
			regulator-always-on;
		};

		ldo4_reg: regulator@6 {
			regulator-always-on;
		};
	};
};

&cpsw_emac0 {
	phy_id = <&davinci_mdio>, <0>;
	phy-mode = "mii";
};

&cpsw_emac1 {
	phy_id = <&davinci_mdio>, <1>;
	phy-mode = "mii";
};

&mac {
	pinctrl-names = "default", "sleep";
	pinctrl-0 = <&cpsw_default>;
	pinctrl-1 = <&cpsw_sleep>;

};

&davinci_mdio {
	pinctrl-names = "default", "sleep";
	pinctrl-0 = <&davinci_mdio_default>;
	pinctrl-1 = <&davinci_mdio_sleep>;
};

&mmc1 {
	status = "okay";
	bus-width = <0x4>;
	pinctrl-names = "default";
	pinctrl-0 = <&mmc1_pins>;
	cd-gpios = <&gpio0 6 GPIO_ACTIVE_HIGH>;
	cd-inverted;
};
