/*
 * Copyright (C) 2012 Texas Instruments Incorporated - http://www.ti.com/
 *
 * This program is free software; you can redistribute it and/or modify
 * it under the terms of the GNU General Public License version 2 as
 * published by the Free Software Foundation.
 */
/dts-v1/;

#include "omap443x.dtsi"
#include "omap4-panda-common.dtsi"

/* Pandaboard Rev A4+ have external pullups on SCL & SDA */
&dss_hdmi_pins {
	pinctrl-single,pins = <
		0x5a (PIN_INPUT_PULLUP | MUX_MODE0)	/* hdmi_cec.hdmi_cec */
		0x5c (PIN_INPUT | MUX_MODE0)		/* hdmi_scl.hdmi_scl */
		0x5e (PIN_INPUT | MUX_MODE0)		/* hdmi_sda.hdmi_sda */
		>;
};
