/*
 * Device Tree Source for OMAP34xx/OMAP35xx SoC
 *
 * Copyright (C) 2013 Texas Instruments Incorporated - http://www.ti.com/
 *
 * This file is licensed under the terms of the GNU General Public License
 * version 2.  This program is licensed "as is" without any warranty of any
 * kind, whether express or implied.
 */

#include "omap3.dtsi"

/ {
	cpus {
		cpu@0 {
			/* OMAP343x/OMAP35xx variants OPP1-5 */
			operating-points = <
				/* kHz    uV */
				125000   975000
				250000  1075000
				500000  1200000
				550000  1270000
				600000  1350000
			>;
			clock-latency = <300000>; /* From legacy driver */
		};
	};

	ocp {
		omap3_pmx_core2: pinmux@480025d8 {
			compatible = "ti,omap3-padconf", "pinctrl-single";
			reg = <0x480025d8 0x24>;
			#address-cells = <1>;
			#size-cells = <0>;
			#interrupt-cells = <1>;
			interrupt-controller;
			pinctrl-single,register-width = <16>;
			pinctrl-single,function-mask = <0xff1f>;
		};
	};
};

&ssi {
	status = "ok";

	clocks = <&ssi_ssr_fck>,
		 <&ssi_sst_fck>,
		 <&ssi_ick>;
	clock-names = "ssi_ssr_fck",
		      "ssi_sst_fck",
		      "ssi_ick";
};

/include/ "omap34xx-omap36xx-clocks.dtsi"
/include/ "omap36xx-omap3430es2plus-clocks.dtsi"
/include/ "omap36xx-am35xx-omap3430es2plus-clocks.dtsi"
