/*
 * at91sama5d3_lcd.dtsi - Device Tree Include file for AT91SAM9x5 SoC with
 * LCD support
 *
 * Copyright (C) 2013 Boris BREZILLON <b.brezillon@overkiz.com>
 *
 * Licensed under GPLv2.
 */

#include <dt-bindings/pinctrl/at91.h>
#include <dt-bindings/interrupt-controller/irq.h>

/ {
	ahb {
		apb {
			pinctrl@fffff200 {
				lcd {
					pinctrl_lcd: lcd-0 {
						atmel,pins =
							<AT91_PIOA 24 AT91_PERIPH_A AT91_PINCTRL_NONE	/* PA24 periph A LCDPWM */
							 AT91_PIOA 26 AT91_PERIPH_A AT91_PINCTRL_NONE	/* PA26 periph A LCDVSYNC */
							 AT91_PIOA 27 AT91_PERIPH_A AT91_PINCTRL_NONE	/* PA27 periph A LCDHSYNC */
							 AT91_PIOA 25 AT91_PERIPH_A AT91_PINCTRL_NONE	/* PA25 periph A LCDDISP */
							 AT91_PIOA 29 AT91_PERIPH_A AT91_PINCTRL_NONE	/* PA29 periph A LCDDEN */
							 AT91_PIOA 28 AT91_PERIPH_A AT91_PINCTRL_NONE	/* PA28 periph A LCDPCK */
							 AT91_PIOA 0 AT91_PERIPH_A AT91_PINCTRL_NONE	/* PA0 periph A LCDD0 pin */
							 AT91_PIOA 1 AT91_PERIPH_A AT91_PINCTRL_NONE	/* PA1 periph A LCDD1 pin */
							 AT91_PIOA 2 AT91_PERIPH_A AT91_PINCTRL_NONE	/* PA2 periph A LCDD2 pin */
							 AT91_PIOA 3 AT91_PERIPH_A AT91_PINCTRL_NONE	/* PA3 periph A LCDD3 pin */
							 AT91_PIOA 4 AT91_PERIPH_A AT91_PINCTRL_NONE	/* PA4 periph A LCDD4 pin */
							 AT91_PIOA 5 AT91_PERIPH_A AT91_PINCTRL_NONE	/* PA5 periph A LCDD5 pin */
							 AT91_PIOA 6 AT91_PERIPH_A AT91_PINCTRL_NONE	/* PA6 periph A LCDD6 pin */
							 AT91_PIOA 7 AT91_PERIPH_A AT91_PINCTRL_NONE	/* PA7 periph A LCDD7 pin */
							 AT91_PIOA 8 AT91_PERIPH_A AT91_PINCTRL_NONE	/* PA8 periph A LCDD8 pin */
							 AT91_PIOA 9 AT91_PERIPH_A AT91_PINCTRL_NONE	/* PA9 periph A LCDD9 pin */
							 AT91_PIOA 10 AT91_PERIPH_A AT91_PINCTRL_NONE	/* PA10 periph A LCDD10 pin */
							 AT91_PIOA 11 AT91_PERIPH_A AT91_PINCTRL_NONE	/* PA11 periph A LCDD11 pin */
							 AT91_PIOA 12 AT91_PERIPH_A AT91_PINCTRL_NONE	/* PA12 periph A LCDD12 pin */
							 AT91_PIOA 13 AT91_PERIPH_A AT91_PINCTRL_NONE	/* PA13 periph A LCDD13 pin */
							 AT91_PIOA 14 AT91_PERIPH_A AT91_PINCTRL_NONE	/* PA14 periph A LCDD14 pin */
							 AT91_PIOA 15 AT91_PERIPH_A AT91_PINCTRL_NONE	/* PA15 periph A LCDD15 pin */
							 AT91_PIOC 14 AT91_PERIPH_C AT91_PINCTRL_NONE	/* PC14 periph C LCDD16 pin */
							 AT91_PIOC 13 AT91_PERIPH_C AT91_PINCTRL_NONE	/* PC13 periph C LCDD17 pin */
							 AT91_PIOC 12 AT91_PERIPH_C AT91_PINCTRL_NONE	/* PC12 periph C LCDD18 pin */
							 AT91_PIOC 11 AT91_PERIPH_C AT91_PINCTRL_NONE	/* PC11 periph C LCDD19 pin */
							 AT91_PIOC 10 AT91_PERIPH_C AT91_PINCTRL_NONE	/* PC10 periph C LCDD20 pin */
							 AT91_PIOC 15 AT91_PERIPH_C AT91_PINCTRL_NONE	/* PC15 periph C LCDD21 pin */
							 AT91_PIOE 27 AT91_PERIPH_C AT91_PINCTRL_NONE	/* PE27 periph C LCDD22 pin */
							 AT91_PIOE 28 AT91_PERIPH_C AT91_PINCTRL_NONE>;	/* PE28 periph C LCDD23 pin */
					};
				};
			};

			pmc: pmc@fffffc00 {
				periphck {
					lcdc_clk: lcdc_clk {
						#clock-cells = <0>;
						reg = <36>;
					};
				};

				systemck {
					lcdck: lcdck {
						#clock-cells = <0>;
						reg = <3>;
						clocks = <&mck>;
					};
				};
			};
		};
	};
};
