/dts-v1/;

#include "skeleton.dtsi"
#include <dt-bindings/clock/qcom,gcc-ipq806x.h>
#include <dt-bindings/soc/qcom,gsbi.h>

/ {
	model = "Qualcomm IPQ8064";
	compatible = "qcom,ipq8064";
	interrupt-parent = <&intc>;

	cpus {
		#address-cells = <1>;
		#size-cells = <0>;

		cpu@0 {
			compatible = "qcom,krait";
			enable-method = "qcom,kpss-acc-v1";
			device_type = "cpu";
			reg = <0>;
			next-level-cache = <&L2>;
			qcom,acc = <&acc0>;
			qcom,saw = <&saw0>;
		};

		cpu@1 {
			compatible = "qcom,krait";
			enable-method = "qcom,kpss-acc-v1";
			device_type = "cpu";
			reg = <1>;
			next-level-cache = <&L2>;
			qcom,acc = <&acc1>;
			qcom,saw = <&saw1>;
		};

		L2: l2-cache {
			compatible = "cache";
			cache-level = <2>;
		};
	};

	cpu-pmu {
		compatible = "qcom,krait-pmu";
		interrupts = <1 10 0x304>;
	};

	reserved-memory {
		#address-cells = <1>;
		#size-cells = <1>;
		ranges;

		nss@40000000 {
			reg = <0x40000000 0x1000000>;
			no-map;
		};

		smem@41000000 {
			reg = <0x41000000 0x200000>;
			no-map;
		};
	};

	soc: soc {
		#address-cells = <1>;
		#size-cells = <1>;
		ranges;
		compatible = "simple-bus";

		qcom_pinmux: pinmux@800000 {
			compatible = "qcom,ipq8064-pinctrl";
			reg = <0x800000 0x4000>;

			gpio-controller;
			#gpio-cells = <2>;
			interrupt-controller;
			#interrupt-cells = <2>;
			interrupts = <0 16 0x4>;
		};

		intc: interrupt-controller@2000000 {
			compatible = "qcom,msm-qgic2";
			interrupt-controller;
			#interrupt-cells = <3>;
			reg = <0x02000000 0x1000>,
			      <0x02002000 0x1000>;
		};

		timer@200a000 {
			compatible = "qcom,kpss-timer", "qcom,msm-timer";
			interrupts = <1 1 0x301>,
				     <1 2 0x301>,
				     <1 3 0x301>;
			reg = <0x0200a000 0x100>;
			clock-frequency = <25000000>,
					  <32768>;
			cpu-offset = <0x80000>;
		};

		acc0: clock-controller@2088000 {
			compatible = "qcom,kpss-acc-v1";
			reg = <0x02088000 0x1000>, <0x02008000 0x1000>;
		};

		acc1: clock-controller@2098000 {
			compatible = "qcom,kpss-acc-v1";
			reg = <0x02098000 0x1000>, <0x02008000 0x1000>;
		};

		saw0: regulator@2089000 {
			compatible = "qcom,saw2";
			reg = <0x02089000 0x1000>, <0x02009000 0x1000>;
			regulator;
		};

		saw1: regulator@2099000 {
			compatible = "qcom,saw2";
			reg = <0x02099000 0x1000>, <0x02009000 0x1000>;
			regulator;
		};

		gsbi2: gsbi@12480000 {
			compatible = "qcom,gsbi-v1.0.0";
			reg = <0x12480000 0x100>;
			clocks = <&gcc GSBI2_H_CLK>;
			clock-names = "iface";
			#address-cells = <1>;
			#size-cells = <1>;
			ranges;
			status = "disabled";

			serial@12490000 {
				compatible = "qcom,msm-uartdm-v1.3", "qcom,msm-uartdm";
				reg = <0x12490000 0x1000>,
				      <0x12480000 0x1000>;
				interrupts = <0 195 0x0>;
				clocks = <&gcc GSBI2_UART_CLK>, <&gcc GSBI2_H_CLK>;
				clock-names = "core", "iface";
				status = "disabled";
			};

			i2c@124a0000 {
				compatible = "qcom,i2c-qup-v1.1.1";
				reg = <0x124a0000 0x1000>;
				interrupts = <0 196 0>;

				clocks = <&gcc GSBI2_QUP_CLK>, <&gcc GSBI2_H_CLK>;
				clock-names = "core", "iface";
				status = "disabled";

				#address-cells = <1>;
				#size-cells = <0>;
			};

		};

		gsbi4: gsbi@16300000 {
			compatible = "qcom,gsbi-v1.0.0";
			reg = <0x16300000 0x100>;
			clocks = <&gcc GSBI4_H_CLK>;
			clock-names = "iface";
			#address-cells = <1>;
			#size-cells = <1>;
			ranges;
			status = "disabled";

			serial@16340000 {
				compatible = "qcom,msm-uartdm-v1.3", "qcom,msm-uartdm";
				reg = <0x16340000 0x1000>,
				      <0x16300000 0x1000>;
				interrupts = <0 152 0x0>;
				clocks = <&gcc GSBI4_UART_CLK>, <&gcc GSBI4_H_CLK>;
				clock-names = "core", "iface";
				status = "disabled";
			};

			i2c@16380000 {
				compatible = "qcom,i2c-qup-v1.1.1";
				reg = <0x16380000 0x1000>;
				interrupts = <0 153 0>;

				clocks = <&gcc GSBI4_QUP_CLK>, <&gcc GSBI4_H_CLK>;
				clock-names = "core", "iface";
				status = "disabled";

				#address-cells = <1>;
				#size-cells = <0>;
			};
		};

		gsbi5: gsbi@1a200000 {
			compatible = "qcom,gsbi-v1.0.0";
			reg = <0x1a200000 0x100>;
			clocks = <&gcc GSBI5_H_CLK>;
			clock-names = "iface";
			#address-cells = <1>;
			#size-cells = <1>;
			ranges;
			status = "disabled";

			serial@1a240000 {
				compatible = "qcom,msm-uartdm-v1.3", "qcom,msm-uartdm";
				reg = <0x1a240000 0x1000>,
				      <0x1a200000 0x1000>;
				interrupts = <0 154 0x0>;
				clocks = <&gcc GSBI5_UART_CLK>, <&gcc GSBI5_H_CLK>;
				clock-names = "core", "iface";
				status = "disabled";
			};

			i2c@1a280000 {
				compatible = "qcom,i2c-qup-v1.1.1";
				reg = <0x1a280000 0x1000>;
				interrupts = <0 155 0>;

				clocks = <&gcc GSBI5_QUP_CLK>, <&gcc GSBI5_H_CLK>;
				clock-names = "core", "iface";
				status = "disabled";

				#address-cells = <1>;
				#size-cells = <0>;
			};

			spi@1a280000 {
				compatible = "qcom,spi-qup-v1.1.1";
				reg = <0x1a280000 0x1000>;
				interrupts = <0 155 0>;

				clocks = <&gcc GSBI5_QUP_CLK>, <&gcc GSBI5_H_CLK>;
				clock-names = "core", "iface";
				status = "disabled";

				#address-cells = <1>;
				#size-cells = <0>;
			};
		};

		sata_phy: sata-phy@1b400000 {
			compatible = "qcom,ipq806x-sata-phy";
			reg = <0x1b400000 0x200>;

			clocks = <&gcc SATA_PHY_CFG_CLK>;
			clock-names = "cfg";

			#phy-cells = <0>;
			status = "disabled";
		};

		sata@29000000 {
			compatible = "qcom,ipq806x-ahci", "generic-ahci";
			reg = <0x29000000 0x180>;

			interrupts = <0 209 0x0>;

			clocks = <&gcc SFAB_SATA_S_H_CLK>,
				 <&gcc SATA_H_CLK>,
				 <&gcc SATA_A_CLK>,
				 <&gcc SATA_RXOOB_CLK>,
				 <&gcc SATA_PMALIVE_CLK>;
			clock-names = "slave_face", "iface", "core",
					"rxoob", "pmalive";

			assigned-clocks = <&gcc SATA_RXOOB_CLK>, <&gcc SATA_PMALIVE_CLK>;
			assigned-clock-rates = <100000000>, <100000000>;

			phys = <&sata_phy>;
			phy-names = "sata-phy";
			status = "disabled";
		};

		qcom,ssbi@500000 {
			compatible = "qcom,ssbi";
			reg = <0x00500000 0x1000>;
			qcom,controller-type = "pmic-arbiter";
		};

		gcc: clock-controller@900000 {
			compatible = "qcom,gcc-ipq8064";
			reg = <0x00900000 0x4000>;
			#clock-cells = <1>;
			#reset-cells = <1>;
		};
	};
};
