/*
 * Device Tree Source for the r8a7790 SoC
 *
 * Copyright (C) 2013-2014 Renesas Solutions Corp.
 * Copyright (C) 2014 Cogent Embedded Inc.
 *
 * This file is licensed under the terms of the GNU General Public License
 * version 2.  This program is licensed "as is" without any warranty of any
 * kind, whether express or implied.
 */

#include <dt-bindings/clock/r8a7790-clock.h>
#include <dt-bindings/interrupt-controller/arm-gic.h>
#include <dt-bindings/interrupt-controller/irq.h>

/ {
	compatible = "renesas,r8a7790";
	interrupt-parent = <&gic>;
	#address-cells = <2>;
	#size-cells = <2>;

	aliases {
		i2c0 = &i2c0;
		i2c1 = &i2c1;
		i2c2 = &i2c2;
		i2c3 = &i2c3;
		i2c4 = &iic0;
		i2c5 = &iic1;
		i2c6 = &iic2;
		i2c7 = &iic3;
		spi0 = &qspi;
		spi1 = &msiof0;
		spi2 = &msiof1;
		spi3 = &msiof2;
		spi4 = &msiof3;
		vin0 = &vin0;
		vin1 = &vin1;
		vin2 = &vin2;
		vin3 = &vin3;
	};

	cpus {
		#address-cells = <1>;
		#size-cells = <0>;

		cpu0: cpu@0 {
			device_type = "cpu";
			compatible = "arm,cortex-a15";
			reg = <0>;
			clock-frequency = <1300000000>;
			voltage-tolerance = <1>; /* 1% */
			clocks = <&cpg_clocks R8A7790_CLK_Z>;
			clock-latency = <300000>; /* 300 us */

			/* kHz - uV - OPPs unknown yet */
			operating-points = <1400000 1000000>,
					   <1225000 1000000>,
					   <1050000 1000000>,
					   < 875000 1000000>,
					   < 700000 1000000>,
					   < 350000 1000000>;
		};

		cpu1: cpu@1 {
			device_type = "cpu";
			compatible = "arm,cortex-a15";
			reg = <1>;
			clock-frequency = <1300000000>;
		};

		cpu2: cpu@2 {
			device_type = "cpu";
			compatible = "arm,cortex-a15";
			reg = <2>;
			clock-frequency = <1300000000>;
		};

		cpu3: cpu@3 {
			device_type = "cpu";
			compatible = "arm,cortex-a15";
			reg = <3>;
			clock-frequency = <1300000000>;
		};

		cpu4: cpu@4 {
			device_type = "cpu";
			compatible = "arm,cortex-a7";
			reg = <0x100>;
			clock-frequency = <780000000>;
		};

		cpu5: cpu@5 {
			device_type = "cpu";
			compatible = "arm,cortex-a7";
			reg = <0x101>;
			clock-frequency = <780000000>;
		};

		cpu6: cpu@6 {
			device_type = "cpu";
			compatible = "arm,cortex-a7";
			reg = <0x102>;
			clock-frequency = <780000000>;
		};

		cpu7: cpu@7 {
			device_type = "cpu";
			compatible = "arm,cortex-a7";
			reg = <0x103>;
			clock-frequency = <780000000>;
		};
	};

	gic: interrupt-controller@f1001000 {
		compatible = "arm,cortex-a15-gic";
		#interrupt-cells = <3>;
		#address-cells = <0>;
		interrupt-controller;
		reg = <0 0xf1001000 0 0x1000>,
			<0 0xf1002000 0 0x1000>,
			<0 0xf1004000 0 0x2000>,
			<0 0xf1006000 0 0x2000>;
		interrupts = <1 9 (GIC_CPU_MASK_SIMPLE(4) | IRQ_TYPE_LEVEL_HIGH)>;
	};

	gpio0: gpio@e6050000 {
		compatible = "renesas,gpio-r8a7790", "renesas,gpio-rcar";
		reg = <0 0xe6050000 0 0x50>;
		interrupts = <0 4 IRQ_TYPE_LEVEL_HIGH>;
		#gpio-cells = <2>;
		gpio-controller;
		gpio-ranges = <&pfc 0 0 32>;
		#interrupt-cells = <2>;
		interrupt-controller;
		clocks = <&mstp9_clks R8A7790_CLK_GPIO0>;
	};

	gpio1: gpio@e6051000 {
		compatible = "renesas,gpio-r8a7790", "renesas,gpio-rcar";
		reg = <0 0xe6051000 0 0x50>;
		interrupts = <0 5 IRQ_TYPE_LEVEL_HIGH>;
		#gpio-cells = <2>;
		gpio-controller;
		gpio-ranges = <&pfc 0 32 32>;
		#interrupt-cells = <2>;
		interrupt-controller;
		clocks = <&mstp9_clks R8A7790_CLK_GPIO1>;
	};

	gpio2: gpio@e6052000 {
		compatible = "renesas,gpio-r8a7790", "renesas,gpio-rcar";
		reg = <0 0xe6052000 0 0x50>;
		interrupts = <0 6 IRQ_TYPE_LEVEL_HIGH>;
		#gpio-cells = <2>;
		gpio-controller;
		gpio-ranges = <&pfc 0 64 32>;
		#interrupt-cells = <2>;
		interrupt-controller;
		clocks = <&mstp9_clks R8A7790_CLK_GPIO2>;
	};

	gpio3: gpio@e6053000 {
		compatible = "renesas,gpio-r8a7790", "renesas,gpio-rcar";
		reg = <0 0xe6053000 0 0x50>;
		interrupts = <0 7 IRQ_TYPE_LEVEL_HIGH>;
		#gpio-cells = <2>;
		gpio-controller;
		gpio-ranges = <&pfc 0 96 32>;
		#interrupt-cells = <2>;
		interrupt-controller;
		clocks = <&mstp9_clks R8A7790_CLK_GPIO3>;
	};

	gpio4: gpio@e6054000 {
		compatible = "renesas,gpio-r8a7790", "renesas,gpio-rcar";
		reg = <0 0xe6054000 0 0x50>;
		interrupts = <0 8 IRQ_TYPE_LEVEL_HIGH>;
		#gpio-cells = <2>;
		gpio-controller;
		gpio-ranges = <&pfc 0 128 32>;
		#interrupt-cells = <2>;
		interrupt-controller;
		clocks = <&mstp9_clks R8A7790_CLK_GPIO4>;
	};

	gpio5: gpio@e6055000 {
		compatible = "renesas,gpio-r8a7790", "renesas,gpio-rcar";
		reg = <0 0xe6055000 0 0x50>;
		interrupts = <0 9 IRQ_TYPE_LEVEL_HIGH>;
		#gpio-cells = <2>;
		gpio-controller;
		gpio-ranges = <&pfc 0 160 32>;
		#interrupt-cells = <2>;
		interrupt-controller;
		clocks = <&mstp9_clks R8A7790_CLK_GPIO5>;
	};

	thermal@e61f0000 {
		compatible = "renesas,thermal-r8a7790", "renesas,rcar-thermal";
		reg = <0 0xe61f0000 0 0x14>, <0 0xe61f0100 0 0x38>;
		interrupts = <0 69 IRQ_TYPE_LEVEL_HIGH>;
		clocks = <&mstp5_clks R8A7790_CLK_THERMAL>;
	};

	timer {
		compatible = "arm,armv7-timer";
		interrupts = <1 13 (GIC_CPU_MASK_SIMPLE(4) | IRQ_TYPE_LEVEL_LOW)>,
			     <1 14 (GIC_CPU_MASK_SIMPLE(4) | IRQ_TYPE_LEVEL_LOW)>,
			     <1 11 (GIC_CPU_MASK_SIMPLE(4) | IRQ_TYPE_LEVEL_LOW)>,
			     <1 10 (GIC_CPU_MASK_SIMPLE(4) | IRQ_TYPE_LEVEL_LOW)>;
	};

	cmt0: timer@ffca0000 {
		compatible = "renesas,cmt-48-r8a7790", "renesas,cmt-48-gen2";
		reg = <0 0xffca0000 0 0x1004>;
		interrupts = <0 142 IRQ_TYPE_LEVEL_HIGH>,
			     <0 143 IRQ_TYPE_LEVEL_HIGH>;
		clocks = <&mstp1_clks R8A7790_CLK_CMT0>;
		clock-names = "fck";

		renesas,channels-mask = <0x60>;

		status = "disabled";
	};

	cmt1: timer@e6130000 {
		compatible = "renesas,cmt-48-r8a7790", "renesas,cmt-48-gen2";
		reg = <0 0xe6130000 0 0x1004>;
		interrupts = <0 120 IRQ_TYPE_LEVEL_HIGH>,
			     <0 121 IRQ_TYPE_LEVEL_HIGH>,
			     <0 122 IRQ_TYPE_LEVEL_HIGH>,
			     <0 123 IRQ_TYPE_LEVEL_HIGH>,
			     <0 124 IRQ_TYPE_LEVEL_HIGH>,
			     <0 125 IRQ_TYPE_LEVEL_HIGH>,
			     <0 126 IRQ_TYPE_LEVEL_HIGH>,
			     <0 127 IRQ_TYPE_LEVEL_HIGH>;
		clocks = <&mstp3_clks R8A7790_CLK_CMT1>;
		clock-names = "fck";

		renesas,channels-mask = <0xff>;

		status = "disabled";
	};

	irqc0: interrupt-controller@e61c0000 {
		compatible = "renesas,irqc-r8a7790", "renesas,irqc";
		#interrupt-cells = <2>;
		interrupt-controller;
		reg = <0 0xe61c0000 0 0x200>;
		interrupts = <0 0 IRQ_TYPE_LEVEL_HIGH>,
			     <0 1 IRQ_TYPE_LEVEL_HIGH>,
			     <0 2 IRQ_TYPE_LEVEL_HIGH>,
			     <0 3 IRQ_TYPE_LEVEL_HIGH>;
	};

	dmac0: dma-controller@e6700000 {
		compatible = "renesas,rcar-dmac";
		reg = <0 0xe6700000 0 0x20000>;
		interrupts = <0 197 IRQ_TYPE_LEVEL_HIGH
			      0 200 IRQ_TYPE_LEVEL_HIGH
			      0 201 IRQ_TYPE_LEVEL_HIGH
			      0 202 IRQ_TYPE_LEVEL_HIGH
			      0 203 IRQ_TYPE_LEVEL_HIGH
			      0 204 IRQ_TYPE_LEVEL_HIGH
			      0 205 IRQ_TYPE_LEVEL_HIGH
			      0 206 IRQ_TYPE_LEVEL_HIGH
			      0 207 IRQ_TYPE_LEVEL_HIGH
			      0 208 IRQ_TYPE_LEVEL_HIGH
			      0 209 IRQ_TYPE_LEVEL_HIGH
			      0 210 IRQ_TYPE_LEVEL_HIGH
			      0 211 IRQ_TYPE_LEVEL_HIGH
			      0 212 IRQ_TYPE_LEVEL_HIGH
			      0 213 IRQ_TYPE_LEVEL_HIGH
			      0 214 IRQ_TYPE_LEVEL_HIGH>;
		interrupt-names = "error",
				"ch0", "ch1", "ch2", "ch3",
				"ch4", "ch5", "ch6", "ch7",
				"ch8", "ch9", "ch10", "ch11",
				"ch12", "ch13", "ch14";
		clocks = <&mstp2_clks R8A7790_CLK_SYS_DMAC0>;
		clock-names = "fck";
		#dma-cells = <1>;
		dma-channels = <15>;
	};

	dmac1: dma-controller@e6720000 {
		compatible = "renesas,rcar-dmac";
		reg = <0 0xe6720000 0 0x20000>;
		interrupts = <0 220 IRQ_TYPE_LEVEL_HIGH
			      0 216 IRQ_TYPE_LEVEL_HIGH
			      0 217 IRQ_TYPE_LEVEL_HIGH
			      0 218 IRQ_TYPE_LEVEL_HIGH
			      0 219 IRQ_TYPE_LEVEL_HIGH
			      0 308 IRQ_TYPE_LEVEL_HIGH
			      0 309 IRQ_TYPE_LEVEL_HIGH
			      0 310 IRQ_TYPE_LEVEL_HIGH
			      0 311 IRQ_TYPE_LEVEL_HIGH
			      0 312 IRQ_TYPE_LEVEL_HIGH
			      0 313 IRQ_TYPE_LEVEL_HIGH
			      0 314 IRQ_TYPE_LEVEL_HIGH
			      0 315 IRQ_TYPE_LEVEL_HIGH
			      0 316 IRQ_TYPE_LEVEL_HIGH
			      0 317 IRQ_TYPE_LEVEL_HIGH
			      0 318 IRQ_TYPE_LEVEL_HIGH>;
		interrupt-names = "error",
				"ch0", "ch1", "ch2", "ch3",
				"ch4", "ch5", "ch6", "ch7",
				"ch8", "ch9", "ch10", "ch11",
				"ch12", "ch13", "ch14";
		clocks = <&mstp2_clks R8A7790_CLK_SYS_DMAC1>;
		clock-names = "fck";
		#dma-cells = <1>;
		dma-channels = <15>;
	};

	audma0: dma-controller@ec700000 {
		compatible = "renesas,rcar-dmac";
		reg = <0 0xec700000 0 0x10000>;
		interrupts =	<0 346 IRQ_TYPE_LEVEL_HIGH
				 0 320 IRQ_TYPE_LEVEL_HIGH
				 0 321 IRQ_TYPE_LEVEL_HIGH
				 0 322 IRQ_TYPE_LEVEL_HIGH
				 0 323 IRQ_TYPE_LEVEL_HIGH
				 0 324 IRQ_TYPE_LEVEL_HIGH
				 0 325 IRQ_TYPE_LEVEL_HIGH
				 0 326 IRQ_TYPE_LEVEL_HIGH
				 0 327 IRQ_TYPE_LEVEL_HIGH
				 0 328 IRQ_TYPE_LEVEL_HIGH
				 0 329 IRQ_TYPE_LEVEL_HIGH
				 0 330 IRQ_TYPE_LEVEL_HIGH
				 0 331 IRQ_TYPE_LEVEL_HIGH
				 0 332 IRQ_TYPE_LEVEL_HIGH>;
		interrupt-names = "error",
				"ch0", "ch1", "ch2", "ch3",
				"ch4", "ch5", "ch6", "ch7",
				"ch8", "ch9", "ch10", "ch11",
				"ch12";
		clocks = <&mstp5_clks R8A7790_CLK_AUDIO_DMAC0>;
		clock-names = "fck";
		#dma-cells = <1>;
		dma-channels = <13>;
	};

	audma1: dma-controller@ec720000 {
		compatible = "renesas,rcar-dmac";
		reg = <0 0xec720000 0 0x10000>;
		interrupts =	<0 347 IRQ_TYPE_LEVEL_HIGH
				 0 333 IRQ_TYPE_LEVEL_HIGH
				 0 334 IRQ_TYPE_LEVEL_HIGH
				 0 335 IRQ_TYPE_LEVEL_HIGH
				 0 336 IRQ_TYPE_LEVEL_HIGH
				 0 337 IRQ_TYPE_LEVEL_HIGH
				 0 338 IRQ_TYPE_LEVEL_HIGH
				 0 339 IRQ_TYPE_LEVEL_HIGH
				 0 340 IRQ_TYPE_LEVEL_HIGH
				 0 341 IRQ_TYPE_LEVEL_HIGH
				 0 342 IRQ_TYPE_LEVEL_HIGH
				 0 343 IRQ_TYPE_LEVEL_HIGH
				 0 344 IRQ_TYPE_LEVEL_HIGH
				 0 345 IRQ_TYPE_LEVEL_HIGH>;
		interrupt-names = "error",
				"ch0", "ch1", "ch2", "ch3",
				"ch4", "ch5", "ch6", "ch7",
				"ch8", "ch9", "ch10", "ch11",
				"ch12";
		clocks = <&mstp5_clks R8A7790_CLK_AUDIO_DMAC1>;
		clock-names = "fck";
		#dma-cells = <1>;
		dma-channels = <13>;
	};

	audmapp: dma-controller@ec740000 {
		compatible = "renesas,rcar-audmapp";
		#dma-cells = <1>;

		reg = <0 0xec740000 0 0x200>;
	};

	i2c0: i2c@e6508000 {
		#address-cells = <1>;
		#size-cells = <0>;
		compatible = "renesas,i2c-r8a7790";
		reg = <0 0xe6508000 0 0x40>;
		interrupts = <0 287 IRQ_TYPE_LEVEL_HIGH>;
		clocks = <&mstp9_clks R8A7790_CLK_I2C0>;
		status = "disabled";
	};

	i2c1: i2c@e6518000 {
		#address-cells = <1>;
		#size-cells = <0>;
		compatible = "renesas,i2c-r8a7790";
		reg = <0 0xe6518000 0 0x40>;
		interrupts = <0 288 IRQ_TYPE_LEVEL_HIGH>;
		clocks = <&mstp9_clks R8A7790_CLK_I2C1>;
		status = "disabled";
	};

	i2c2: i2c@e6530000 {
		#address-cells = <1>;
		#size-cells = <0>;
		compatible = "renesas,i2c-r8a7790";
		reg = <0 0xe6530000 0 0x40>;
		interrupts = <0 286 IRQ_TYPE_LEVEL_HIGH>;
		clocks = <&mstp9_clks R8A7790_CLK_I2C2>;
		status = "disabled";
	};

	i2c3: i2c@e6540000 {
		#address-cells = <1>;
		#size-cells = <0>;
		compatible = "renesas,i2c-r8a7790";
		reg = <0 0xe6540000 0 0x40>;
		interrupts = <0 290 IRQ_TYPE_LEVEL_HIGH>;
		clocks = <&mstp9_clks R8A7790_CLK_I2C3>;
		status = "disabled";
	};

	iic0: i2c@e6500000 {
		#address-cells = <1>;
		#size-cells = <0>;
		compatible = "renesas,iic-r8a7790", "renesas,rmobile-iic";
		reg = <0 0xe6500000 0 0x425>;
		interrupts = <0 174 IRQ_TYPE_LEVEL_HIGH>;
		clocks = <&mstp3_clks R8A7790_CLK_IIC0>;
		dmas = <&dmac0 0x61>, <&dmac0 0x62>;
		dma-names = "tx", "rx";
		status = "disabled";
	};

	iic1: i2c@e6510000 {
		#address-cells = <1>;
		#size-cells = <0>;
		compatible = "renesas,iic-r8a7790", "renesas,rmobile-iic";
		reg = <0 0xe6510000 0 0x425>;
		interrupts = <0 175 IRQ_TYPE_LEVEL_HIGH>;
		clocks = <&mstp3_clks R8A7790_CLK_IIC1>;
		dmas = <&dmac0 0x65>, <&dmac0 0x66>;
		dma-names = "tx", "rx";
		status = "disabled";
	};

	iic2: i2c@e6520000 {
		#address-cells = <1>;
		#size-cells = <0>;
		compatible = "renesas,iic-r8a7790", "renesas,rmobile-iic";
		reg = <0 0xe6520000 0 0x425>;
		interrupts = <0 176 IRQ_TYPE_LEVEL_HIGH>;
		clocks = <&mstp3_clks R8A7790_CLK_IIC2>;
		dmas = <&dmac0 0x69>, <&dmac0 0x6a>;
		dma-names = "tx", "rx";
		status = "disabled";
	};

	iic3: i2c@e60b0000 {
		#address-cells = <1>;
		#size-cells = <0>;
		compatible = "renesas,iic-r8a7790", "renesas,rmobile-iic";
		reg = <0 0xe60b0000 0 0x425>;
		interrupts = <0 173 IRQ_TYPE_LEVEL_HIGH>;
		clocks = <&mstp9_clks R8A7790_CLK_IICDVFS>;
		dmas = <&dmac0 0x77>, <&dmac0 0x78>;
		dma-names = "tx", "rx";
		status = "disabled";
	};

	mmcif0: mmc@ee200000 {
		compatible = "renesas,mmcif-r8a7790", "renesas,sh-mmcif";
		reg = <0 0xee200000 0 0x80>;
		interrupts = <0 169 IRQ_TYPE_LEVEL_HIGH>;
		clocks = <&mstp3_clks R8A7790_CLK_MMCIF0>;
		dmas = <&dmac0 0xd1>, <&dmac0 0xd2>;
		dma-names = "tx", "rx";
		reg-io-width = <4>;
		status = "disabled";
	};

	mmcif1: mmc@ee220000 {
		compatible = "renesas,mmcif-r8a7790", "renesas,sh-mmcif";
		reg = <0 0xee220000 0 0x80>;
		interrupts = <0 170 IRQ_TYPE_LEVEL_HIGH>;
		clocks = <&mstp3_clks R8A7790_CLK_MMCIF1>;
		dmas = <&dmac0 0xe1>, <&dmac0 0xe2>;
		dma-names = "tx", "rx";
		reg-io-width = <4>;
		status = "disabled";
	};

	pfc: pfc@e6060000 {
		compatible = "renesas,pfc-r8a7790";
		reg = <0 0xe6060000 0 0x250>;
	};

	sdhi0: sd@ee100000 {
		compatible = "renesas,sdhi-r8a7790";
		reg = <0 0xee100000 0 0x200>;
		interrupts = <0 165 IRQ_TYPE_LEVEL_HIGH>;
		clocks = <&mstp3_clks R8A7790_CLK_SDHI0>;
		status = "disabled";
	};

	sdhi1: sd@ee120000 {
		compatible = "renesas,sdhi-r8a7790";
		reg = <0 0xee120000 0 0x200>;
		interrupts = <0 166 IRQ_TYPE_LEVEL_HIGH>;
		clocks = <&mstp3_clks R8A7790_CLK_SDHI1>;
		status = "disabled";
	};

	sdhi2: sd@ee140000 {
		compatible = "renesas,sdhi-r8a7790";
		reg = <0 0xee140000 0 0x100>;
		interrupts = <0 167 IRQ_TYPE_LEVEL_HIGH>;
		clocks = <&mstp3_clks R8A7790_CLK_SDHI2>;
		status = "disabled";
	};

	sdhi3: sd@ee160000 {
		compatible = "renesas,sdhi-r8a7790";
		reg = <0 0xee160000 0 0x100>;
		interrupts = <0 168 IRQ_TYPE_LEVEL_HIGH>;
		clocks = <&mstp3_clks R8A7790_CLK_SDHI3>;
		status = "disabled";
	};

	scifa0: serial@e6c40000 {
		compatible = "renesas,scifa-r8a7790", "renesas,scifa";
		reg = <0 0xe6c40000 0 64>;
		interrupts = <0 144 IRQ_TYPE_LEVEL_HIGH>;
		clocks = <&mstp2_clks R8A7790_CLK_SCIFA0>;
		clock-names = "sci_ick";
		status = "disabled";
	};

	scifa1: serial@e6c50000 {
		compatible = "renesas,scifa-r8a7790", "renesas,scifa";
		reg = <0 0xe6c50000 0 64>;
		interrupts = <0 145 IRQ_TYPE_LEVEL_HIGH>;
		clocks = <&mstp2_clks R8A7790_CLK_SCIFA1>;
		clock-names = "sci_ick";
		status = "disabled";
	};

	scifa2: serial@e6c60000 {
		compatible = "renesas,scifa-r8a7790", "renesas,scifa";
		reg = <0 0xe6c60000 0 64>;
		interrupts = <0 151 IRQ_TYPE_LEVEL_HIGH>;
		clocks = <&mstp2_clks R8A7790_CLK_SCIFA2>;
		clock-names = "sci_ick";
		status = "disabled";
	};

	scifb0: serial@e6c20000 {
		compatible = "renesas,scifb-r8a7790", "renesas,scifb";
		reg = <0 0xe6c20000 0 64>;
		interrupts = <0 148 IRQ_TYPE_LEVEL_HIGH>;
		clocks = <&mstp2_clks R8A7790_CLK_SCIFB0>;
		clock-names = "sci_ick";
		status = "disabled";
	};

	scifb1: serial@e6c30000 {
		compatible = "renesas,scifb-r8a7790", "renesas,scifb";
		reg = <0 0xe6c30000 0 64>;
		interrupts = <0 149 IRQ_TYPE_LEVEL_HIGH>;
		clocks = <&mstp2_clks R8A7790_CLK_SCIFB1>;
		clock-names = "sci_ick";
		status = "disabled";
	};

	scifb2: serial@e6ce0000 {
		compatible = "renesas,scifb-r8a7790", "renesas,scifb";
		reg = <0 0xe6ce0000 0 64>;
		interrupts = <0 150 IRQ_TYPE_LEVEL_HIGH>;
		clocks = <&mstp2_clks R8A7790_CLK_SCIFB2>;
		clock-names = "sci_ick";
		status = "disabled";
	};

	scif0: serial@e6e60000 {
		compatible = "renesas,scif-r8a7790", "renesas,scif";
		reg = <0 0xe6e60000 0 64>;
		interrupts = <0 152 IRQ_TYPE_LEVEL_HIGH>;
		clocks = <&mstp7_clks R8A7790_CLK_SCIF0>;
		clock-names = "sci_ick";
		status = "disabled";
	};

	scif1: serial@e6e68000 {
		compatible = "renesas,scif-r8a7790", "renesas,scif";
		reg = <0 0xe6e68000 0 64>;
		interrupts = <0 153 IRQ_TYPE_LEVEL_HIGH>;
		clocks = <&mstp7_clks R8A7790_CLK_SCIF1>;
		clock-names = "sci_ick";
		status = "disabled";
	};

	hscif0: serial@e62c0000 {
		compatible = "renesas,hscif-r8a7790", "renesas,hscif";
		reg = <0 0xe62c0000 0 96>;
		interrupts = <0 154 IRQ_TYPE_LEVEL_HIGH>;
		clocks = <&mstp7_clks R8A7790_CLK_HSCIF0>;
		clock-names = "sci_ick";
		status = "disabled";
	};

	hscif1: serial@e62c8000 {
		compatible = "renesas,hscif-r8a7790", "renesas,hscif";
		reg = <0 0xe62c8000 0 96>;
		interrupts = <0 155 IRQ_TYPE_LEVEL_HIGH>;
		clocks = <&mstp7_clks R8A7790_CLK_HSCIF1>;
		clock-names = "sci_ick";
		status = "disabled";
	};

	ether: ethernet@ee700000 {
		compatible = "renesas,ether-r8a7790";
		reg = <0 0xee700000 0 0x400>;
		interrupts = <0 162 IRQ_TYPE_LEVEL_HIGH>;
		clocks = <&mstp8_clks R8A7790_CLK_ETHER>;
		phy-mode = "rmii";
		#address-cells = <1>;
		#size-cells = <0>;
		status = "disabled";
	};

	sata0: sata@ee300000 {
		compatible = "renesas,sata-r8a7790";
		reg = <0 0xee300000 0 0x2000>;
		interrupts = <0 105 IRQ_TYPE_LEVEL_HIGH>;
		clocks = <&mstp8_clks R8A7790_CLK_SATA0>;
		status = "disabled";
	};

	sata1: sata@ee500000 {
		compatible = "renesas,sata-r8a7790";
		reg = <0 0xee500000 0 0x2000>;
		interrupts = <0 106 IRQ_TYPE_LEVEL_HIGH>;
		clocks = <&mstp8_clks R8A7790_CLK_SATA1>;
		status = "disabled";
	};

	hsusb: usb@e6590000 {
		compatible = "renesas,usbhs-r8a7790";
		reg = <0 0xe6590000 0 0x100>;
		interrupts = <0 107 IRQ_TYPE_LEVEL_HIGH>;
		clocks = <&mstp7_clks R8A7790_CLK_HSUSB>;
		renesas,buswait = <4>;
		phys = <&usb0 1>;
		phy-names = "usb";
		status = "disabled";
	};

	usbphy: usb-phy@e6590100 {
		compatible = "renesas,usb-phy-r8a7790";
		reg = <0 0xe6590100 0 0x100>;
		#address-cells = <1>;
		#size-cells = <0>;
		clocks = <&mstp7_clks R8A7790_CLK_HSUSB>;
		clock-names = "usbhs";
		status = "disabled";

		usb0: usb-channel@0 {
			reg = <0>;
			#phy-cells = <1>;
		};
		usb2: usb-channel@2 {
			reg = <2>;
			#phy-cells = <1>;
		};
	};

	vin0: video@e6ef0000 {
		compatible = "renesas,vin-r8a7790";
		clocks = <&mstp8_clks R8A7790_CLK_VIN0>;
		reg = <0 0xe6ef0000 0 0x1000>;
		interrupts = <0 188 IRQ_TYPE_LEVEL_HIGH>;
		status = "disabled";
	};

	vin1: video@e6ef1000 {
		compatible = "renesas,vin-r8a7790";
		clocks = <&mstp8_clks R8A7790_CLK_VIN1>;
		reg = <0 0xe6ef1000 0 0x1000>;
		interrupts = <0 189 IRQ_TYPE_LEVEL_HIGH>;
		status = "disabled";
	};

	vin2: video@e6ef2000 {
		compatible = "renesas,vin-r8a7790";
		clocks = <&mstp8_clks R8A7790_CLK_VIN2>;
		reg = <0 0xe6ef2000 0 0x1000>;
		interrupts = <0 190 IRQ_TYPE_LEVEL_HIGH>;
		status = "disabled";
	};

	vin3: video@e6ef3000 {
		compatible = "renesas,vin-r8a7790";
		clocks = <&mstp8_clks R8A7790_CLK_VIN3>;
		reg = <0 0xe6ef3000 0 0x1000>;
		interrupts = <0 191 IRQ_TYPE_LEVEL_HIGH>;
		status = "disabled";
	};

	vsp1@fe920000 {
		compatible = "renesas,vsp1";
		reg = <0 0xfe920000 0 0x8000>;
		interrupts = <0 266 IRQ_TYPE_LEVEL_HIGH>;
		clocks = <&mstp1_clks R8A7790_CLK_VSP1_R>;

		renesas,has-sru;
		renesas,#rpf = <5>;
		renesas,#uds = <1>;
		renesas,#wpf = <4>;
	};

	vsp1@fe928000 {
		compatible = "renesas,vsp1";
		reg = <0 0xfe928000 0 0x8000>;
		interrupts = <0 267 IRQ_TYPE_LEVEL_HIGH>;
		clocks = <&mstp1_clks R8A7790_CLK_VSP1_S>;

		renesas,has-lut;
		renesas,has-sru;
		renesas,#rpf = <5>;
		renesas,#uds = <3>;
		renesas,#wpf = <4>;
	};

	vsp1@fe930000 {
		compatible = "renesas,vsp1";
		reg = <0 0xfe930000 0 0x8000>;
		interrupts = <0 246 IRQ_TYPE_LEVEL_HIGH>;
		clocks = <&mstp1_clks R8A7790_CLK_VSP1_DU0>;

		renesas,has-lif;
		renesas,has-lut;
		renesas,#rpf = <4>;
		renesas,#uds = <1>;
		renesas,#wpf = <4>;
	};

	vsp1@fe938000 {
		compatible = "renesas,vsp1";
		reg = <0 0xfe938000 0 0x8000>;
		interrupts = <0 247 IRQ_TYPE_LEVEL_HIGH>;
		clocks = <&mstp1_clks R8A7790_CLK_VSP1_DU1>;

		renesas,has-lif;
		renesas,has-lut;
		renesas,#rpf = <4>;
		renesas,#uds = <1>;
		renesas,#wpf = <4>;
	};

	du: display@feb00000 {
		compatible = "renesas,du-r8a7790";
		reg = <0 0xfeb00000 0 0x70000>,
		      <0 0xfeb90000 0 0x1c>,
		      <0 0xfeb94000 0 0x1c>;
		reg-names = "du", "lvds.0", "lvds.1";
		interrupts = <0 256 IRQ_TYPE_LEVEL_HIGH>,
			     <0 268 IRQ_TYPE_LEVEL_HIGH>,
			     <0 269 IRQ_TYPE_LEVEL_HIGH>;
		clocks = <&mstp7_clks R8A7790_CLK_DU0>,
			 <&mstp7_clks R8A7790_CLK_DU1>,
			 <&mstp7_clks R8A7790_CLK_DU2>,
			 <&mstp7_clks R8A7790_CLK_LVDS0>,
			 <&mstp7_clks R8A7790_CLK_LVDS1>;
		clock-names = "du.0", "du.1", "du.2", "lvds.0", "lvds.1";
		status = "disabled";

		ports {
			#address-cells = <1>;
			#size-cells = <0>;

			port@0 {
				reg = <0>;
				du_out_rgb: endpoint {
				};
			};
			port@1 {
				reg = <1>;
				du_out_lvds0: endpoint {
				};
			};
			port@2 {
				reg = <2>;
				du_out_lvds1: endpoint {
				};
			};
		};
	};

	clocks {
		#address-cells = <2>;
		#size-cells = <2>;
		ranges;

		/* External root clock */
		extal_clk: extal_clk {
			compatible = "fixed-clock";
			#clock-cells = <0>;
			/* This value must be overriden by the board. */
			clock-frequency = <0>;
			clock-output-names = "extal";
		};

		/* External PCIe clock - can be overridden by the board */
		pcie_bus_clk: pcie_bus_clk {
			compatible = "fixed-clock";
			#clock-cells = <0>;
			clock-frequency = <100000000>;
			clock-output-names = "pcie_bus";
			status = "disabled";
		};

		/*
		 * The external audio clocks are configured as 0 Hz fixed frequency clocks by
		 * default. Boards that provide audio clocks should override them.
		 */
		audio_clk_a: audio_clk_a {
			compatible = "fixed-clock";
			#clock-cells = <0>;
			clock-frequency = <0>;
			clock-output-names = "audio_clk_a";
		};
		audio_clk_b: audio_clk_b {
			compatible = "fixed-clock";
			#clock-cells = <0>;
			clock-frequency = <0>;
			clock-output-names = "audio_clk_b";
		};
		audio_clk_c: audio_clk_c {
			compatible = "fixed-clock";
			#clock-cells = <0>;
			clock-frequency = <0>;
			clock-output-names = "audio_clk_c";
		};

		/* Special CPG clocks */
		cpg_clocks: cpg_clocks@e6150000 {
			compatible = "renesas,r8a7790-cpg-clocks",
				     "renesas,rcar-gen2-cpg-clocks";
			reg = <0 0xe6150000 0 0x1000>;
			clocks = <&extal_clk>;
			#clock-cells = <1>;
			clock-output-names = "main", "pll0", "pll1", "pll3",
					     "lb", "qspi", "sdh", "sd0", "sd1",
					     "z";
		};

		/* Variable factor clocks */
		sd2_clk: sd2_clk@e6150078 {
			compatible = "renesas,r8a7790-div6-clock", "renesas,cpg-div6-clock";
			reg = <0 0xe6150078 0 4>;
			clocks = <&pll1_div2_clk>;
			#clock-cells = <0>;
			clock-output-names = "sd2";
		};
		sd3_clk: sd3_clk@e615026c {
			compatible = "renesas,r8a7790-div6-clock", "renesas,cpg-div6-clock";
			reg = <0 0xe615026c 0 4>;
			clocks = <&pll1_div2_clk>;
			#clock-cells = <0>;
			clock-output-names = "sd3";
		};
		mmc0_clk: mmc0_clk@e6150240 {
			compatible = "renesas,r8a7790-div6-clock", "renesas,cpg-div6-clock";
			reg = <0 0xe6150240 0 4>;
			clocks = <&pll1_div2_clk>;
			#clock-cells = <0>;
			clock-output-names = "mmc0";
		};
		mmc1_clk: mmc1_clk@e6150244 {
			compatible = "renesas,r8a7790-div6-clock", "renesas,cpg-div6-clock";
			reg = <0 0xe6150244 0 4>;
			clocks = <&pll1_div2_clk>;
			#clock-cells = <0>;
			clock-output-names = "mmc1";
		};
		ssp_clk: ssp_clk@e6150248 {
			compatible = "renesas,r8a7790-div6-clock", "renesas,cpg-div6-clock";
			reg = <0 0xe6150248 0 4>;
			clocks = <&pll1_div2_clk>;
			#clock-cells = <0>;
			clock-output-names = "ssp";
		};
		ssprs_clk: ssprs_clk@e615024c {
			compatible = "renesas,r8a7790-div6-clock", "renesas,cpg-div6-clock";
			reg = <0 0xe615024c 0 4>;
			clocks = <&pll1_div2_clk>;
			#clock-cells = <0>;
			clock-output-names = "ssprs";
		};

		/* Fixed factor clocks */
		pll1_div2_clk: pll1_div2_clk {
			compatible = "fixed-factor-clock";
			clocks = <&cpg_clocks R8A7790_CLK_PLL1>;
			#clock-cells = <0>;
			clock-div = <2>;
			clock-mult = <1>;
			clock-output-names = "pll1_div2";
		};
		z2_clk: z2_clk {
			compatible = "fixed-factor-clock";
			clocks = <&cpg_clocks R8A7790_CLK_PLL1>;
			#clock-cells = <0>;
			clock-div = <2>;
			clock-mult = <1>;
			clock-output-names = "z2";
		};
		zg_clk: zg_clk {
			compatible = "fixed-factor-clock";
			clocks = <&cpg_clocks R8A7790_CLK_PLL1>;
			#clock-cells = <0>;
			clock-div = <3>;
			clock-mult = <1>;
			clock-output-names = "zg";
		};
		zx_clk: zx_clk {
			compatible = "fixed-factor-clock";
			clocks = <&cpg_clocks R8A7790_CLK_PLL1>;
			#clock-cells = <0>;
			clock-div = <3>;
			clock-mult = <1>;
			clock-output-names = "zx";
		};
		zs_clk: zs_clk {
			compatible = "fixed-factor-clock";
			clocks = <&cpg_clocks R8A7790_CLK_PLL1>;
			#clock-cells = <0>;
			clock-div = <6>;
			clock-mult = <1>;
			clock-output-names = "zs";
		};
		hp_clk: hp_clk {
			compatible = "fixed-factor-clock";
			clocks = <&cpg_clocks R8A7790_CLK_PLL1>;
			#clock-cells = <0>;
			clock-div = <12>;
			clock-mult = <1>;
			clock-output-names = "hp";
		};
		i_clk: i_clk {
			compatible = "fixed-factor-clock";
			clocks = <&cpg_clocks R8A7790_CLK_PLL1>;
			#clock-cells = <0>;
			clock-div = <2>;
			clock-mult = <1>;
			clock-output-names = "i";
		};
		b_clk: b_clk {
			compatible = "fixed-factor-clock";
			clocks = <&cpg_clocks R8A7790_CLK_PLL1>;
			#clock-cells = <0>;
			clock-div = <12>;
			clock-mult = <1>;
			clock-output-names = "b";
		};
		p_clk: p_clk {
			compatible = "fixed-factor-clock";
			clocks = <&cpg_clocks R8A7790_CLK_PLL1>;
			#clock-cells = <0>;
			clock-div = <24>;
			clock-mult = <1>;
			clock-output-names = "p";
		};
		cl_clk: cl_clk {
			compatible = "fixed-factor-clock";
			clocks = <&cpg_clocks R8A7790_CLK_PLL1>;
			#clock-cells = <0>;
			clock-div = <48>;
			clock-mult = <1>;
			clock-output-names = "cl";
		};
		m2_clk: m2_clk {
			compatible = "fixed-factor-clock";
			clocks = <&cpg_clocks R8A7790_CLK_PLL1>;
			#clock-cells = <0>;
			clock-div = <8>;
			clock-mult = <1>;
			clock-output-names = "m2";
		};
		imp_clk: imp_clk {
			compatible = "fixed-factor-clock";
			clocks = <&cpg_clocks R8A7790_CLK_PLL1>;
			#clock-cells = <0>;
			clock-div = <4>;
			clock-mult = <1>;
			clock-output-names = "imp";
		};
		rclk_clk: rclk_clk {
			compatible = "fixed-factor-clock";
			clocks = <&cpg_clocks R8A7790_CLK_PLL1>;
			#clock-cells = <0>;
			clock-div = <(48 * 1024)>;
			clock-mult = <1>;
			clock-output-names = "rclk";
		};
		oscclk_clk: oscclk_clk {
			compatible = "fixed-factor-clock";
			clocks = <&cpg_clocks R8A7790_CLK_PLL1>;
			#clock-cells = <0>;
			clock-div = <(12 * 1024)>;
			clock-mult = <1>;
			clock-output-names = "oscclk";
		};
		zb3_clk: zb3_clk {
			compatible = "fixed-factor-clock";
			clocks = <&cpg_clocks R8A7790_CLK_PLL3>;
			#clock-cells = <0>;
			clock-div = <4>;
			clock-mult = <1>;
			clock-output-names = "zb3";
		};
		zb3d2_clk: zb3d2_clk {
			compatible = "fixed-factor-clock";
			clocks = <&cpg_clocks R8A7790_CLK_PLL3>;
			#clock-cells = <0>;
			clock-div = <8>;
			clock-mult = <1>;
			clock-output-names = "zb3d2";
		};
		ddr_clk: ddr_clk {
			compatible = "fixed-factor-clock";
			clocks = <&cpg_clocks R8A7790_CLK_PLL3>;
			#clock-cells = <0>;
			clock-div = <8>;
			clock-mult = <1>;
			clock-output-names = "ddr";
		};
		mp_clk: mp_clk {
			compatible = "fixed-factor-clock";
			clocks = <&pll1_div2_clk>;
			#clock-cells = <0>;
			clock-div = <15>;
			clock-mult = <1>;
			clock-output-names = "mp";
		};
		cp_clk: cp_clk {
			compatible = "fixed-factor-clock";
			clocks = <&extal_clk>;
			#clock-cells = <0>;
			clock-div = <2>;
			clock-mult = <1>;
			clock-output-names = "cp";
		};

		/* Gate clocks */
		mstp0_clks: mstp0_clks@e6150130 {
			compatible = "renesas,r8a7790-mstp-clocks", "renesas,cpg-mstp-clocks";
			reg = <0 0xe6150130 0 4>, <0 0xe6150030 0 4>;
			clocks = <&mp_clk>;
			#clock-cells = <1>;
			clock-indices = <R8A7790_CLK_MSIOF0>;
			clock-output-names = "msiof0";
		};
		mstp1_clks: mstp1_clks@e6150134 {
			compatible = "renesas,r8a7790-mstp-clocks", "renesas,cpg-mstp-clocks";
			reg = <0 0xe6150134 0 4>, <0 0xe6150038 0 4>;
			clocks = <&zs_clk>, <&zs_clk>, <&zs_clk>, <&zs_clk>, <&m2_clk>,
				 <&zs_clk>, <&p_clk>, <&zg_clk>, <&zs_clk>, <&zs_clk>,
				 <&zs_clk>, <&zs_clk>, <&p_clk>, <&p_clk>, <&rclk_clk>,
				 <&cp_clk>, <&zs_clk>, <&zs_clk>, <&zs_clk>, <&zs_clk>;
			#clock-cells = <1>;
			clock-indices = <
				R8A7790_CLK_VCP1 R8A7790_CLK_VCP0 R8A7790_CLK_VPC1
				R8A7790_CLK_VPC0 R8A7790_CLK_JPU R8A7790_CLK_SSP1
				R8A7790_CLK_TMU1 R8A7790_CLK_3DG R8A7790_CLK_2DDMAC
				R8A7790_CLK_FDP1_2 R8A7790_CLK_FDP1_1 R8A7790_CLK_FDP1_0
				R8A7790_CLK_TMU3 R8A7790_CLK_TMU2 R8A7790_CLK_CMT0
				R8A7790_CLK_TMU0 R8A7790_CLK_VSP1_DU1 R8A7790_CLK_VSP1_DU0
				R8A7790_CLK_VSP1_R R8A7790_CLK_VSP1_S
			>;
			clock-output-names =
				"vcp1", "vcp0", "vpc1", "vpc0", "jpu", "ssp1",
				"tmu1", "3dg", "2ddmac", "fdp1-2", "fdp1-1",
				"fdp1-0", "tmu3", "tmu2", "cmt0", "tmu0",
				"vsp1-du1", "vsp1-du0", "vsp1-rt", "vsp1-sy";
		};
		mstp2_clks: mstp2_clks@e6150138 {
			compatible = "renesas,r8a7790-mstp-clocks", "renesas,cpg-mstp-clocks";
			reg = <0 0xe6150138 0 4>, <0 0xe6150040 0 4>;
			clocks = <&mp_clk>, <&mp_clk>, <&mp_clk>, <&mp_clk>, <&mp_clk>,
				 <&mp_clk>, <&mp_clk>, <&mp_clk>, <&mp_clk>, <&zs_clk>,
				 <&zs_clk>;
			#clock-cells = <1>;
			clock-indices = <
				R8A7790_CLK_SCIFA2 R8A7790_CLK_SCIFA1 R8A7790_CLK_SCIFA0
				R8A7790_CLK_MSIOF2 R8A7790_CLK_SCIFB0 R8A7790_CLK_SCIFB1
				R8A7790_CLK_MSIOF1 R8A7790_CLK_MSIOF3 R8A7790_CLK_SCIFB2
				R8A7790_CLK_SYS_DMAC1 R8A7790_CLK_SYS_DMAC0
			>;
			clock-output-names =
				"scifa2", "scifa1", "scifa0", "msiof2", "scifb0",
				"scifb1", "msiof1", "msiof3", "scifb2",
				"sys-dmac1", "sys-dmac0";
		};
		mstp3_clks: mstp3_clks@e615013c {
			compatible = "renesas,r8a7790-mstp-clocks", "renesas,cpg-mstp-clocks";
			reg = <0 0xe615013c 0 4>, <0 0xe6150048 0 4>;
			clocks = <&hp_clk>, <&cp_clk>, <&mmc1_clk>, <&sd3_clk>,
				 <&sd2_clk>, <&cpg_clocks R8A7790_CLK_SD1>, <&cpg_clocks R8A7790_CLK_SD0>, <&mmc0_clk>,
				 <&hp_clk>, <&mp_clk>, <&hp_clk>, <&mp_clk>, <&rclk_clk>,
				 <&hp_clk>, <&hp_clk>;
			#clock-cells = <1>;
			clock-indices = <
				R8A7790_CLK_IIC2 R8A7790_CLK_TPU0 R8A7790_CLK_MMCIF1 R8A7790_CLK_SDHI3
				R8A7790_CLK_SDHI2 R8A7790_CLK_SDHI1 R8A7790_CLK_SDHI0 R8A7790_CLK_MMCIF0
				R8A7790_CLK_IIC0 R8A7790_CLK_PCIEC R8A7790_CLK_IIC1 R8A7790_CLK_SSUSB R8A7790_CLK_CMT1
				R8A7790_CLK_USBDMAC0 R8A7790_CLK_USBDMAC1
			>;
			clock-output-names =
				"iic2", "tpu0", "mmcif1", "sdhi3",
				"sdhi2", "sdhi1", "sdhi0", "mmcif0",
				"iic0", "pciec", "iic1", "ssusb", "cmt1",
				"usbdmac0", "usbdmac1";
		};
		mstp5_clks: mstp5_clks@e6150144 {
			compatible = "renesas,r8a7790-mstp-clocks", "renesas,cpg-mstp-clocks";
			reg = <0 0xe6150144 0 4>, <0 0xe615003c 0 4>;
			clocks = <&hp_clk>, <&hp_clk>, <&extal_clk>, <&p_clk>;
			#clock-cells = <1>;
			clock-indices = <
				R8A7790_CLK_AUDIO_DMAC0 R8A7790_CLK_AUDIO_DMAC1
				R8A7790_CLK_THERMAL R8A7790_CLK_PWM
			>;
			clock-output-names = "audmac0", "audmac1", "thermal", "pwm";
		};
		mstp7_clks: mstp7_clks@e615014c {
			compatible = "renesas,r8a7790-mstp-clocks", "renesas,cpg-mstp-clocks";
			reg = <0 0xe615014c 0 4>, <0 0xe61501c4 0 4>;
			clocks = <&mp_clk>, <&mp_clk>, <&zs_clk>, <&zs_clk>, <&p_clk>,
				 <&p_clk>, <&zx_clk>, <&zx_clk>, <&zx_clk>, <&zx_clk>,
				 <&zx_clk>;
			#clock-cells = <1>;
			clock-indices = <
				R8A7790_CLK_EHCI R8A7790_CLK_HSUSB R8A7790_CLK_HSCIF1
				R8A7790_CLK_HSCIF0 R8A7790_CLK_SCIF1 R8A7790_CLK_SCIF0
				R8A7790_CLK_DU2 R8A7790_CLK_DU1 R8A7790_CLK_DU0
				R8A7790_CLK_LVDS1 R8A7790_CLK_LVDS0
			>;
			clock-output-names =
				"ehci", "hsusb", "hscif1", "hscif0", "scif1",
				"scif0", "du2", "du1", "du0", "lvds1", "lvds0";
		};
		mstp8_clks: mstp8_clks@e6150990 {
			compatible = "renesas,r8a7790-mstp-clocks", "renesas,cpg-mstp-clocks";
			reg = <0 0xe6150990 0 4>, <0 0xe61509a0 0 4>;
			clocks = <&hp_clk>, <&zg_clk>, <&zg_clk>, <&zg_clk>,
			         <&zg_clk>, <&p_clk>, <&zs_clk>, <&zs_clk>;
			#clock-cells = <1>;
			clock-indices = <
				R8A7790_CLK_MLB R8A7790_CLK_VIN3 R8A7790_CLK_VIN2
				R8A7790_CLK_VIN1 R8A7790_CLK_VIN0 R8A7790_CLK_ETHER
				R8A7790_CLK_SATA1 R8A7790_CLK_SATA0
			>;
			clock-output-names =
				"mlb", "vin3", "vin2", "vin1", "vin0", "ether",
				"sata1", "sata0";
		};
		mstp9_clks: mstp9_clks@e6150994 {
			compatible = "renesas,r8a7790-mstp-clocks", "renesas,cpg-mstp-clocks";
			reg = <0 0xe6150994 0 4>, <0 0xe61509a4 0 4>;
			clocks = <&cp_clk>, <&cp_clk>, <&cp_clk>,
				 <&cp_clk>, <&cp_clk>, <&cp_clk>,
				 <&p_clk>, <&p_clk>, <&cpg_clocks R8A7790_CLK_QSPI>, <&cp_clk>,
				 <&hp_clk>, <&hp_clk>, <&hp_clk>, <&hp_clk>;
			#clock-cells = <1>;
			clock-indices = <
				R8A7790_CLK_GPIO5 R8A7790_CLK_GPIO4 R8A7790_CLK_GPIO3
				R8A7790_CLK_GPIO2 R8A7790_CLK_GPIO1 R8A7790_CLK_GPIO0
				R8A7790_CLK_RCAN1 R8A7790_CLK_RCAN0 R8A7790_CLK_QSPI_MOD R8A7790_CLK_IICDVFS
				R8A7790_CLK_I2C3 R8A7790_CLK_I2C2 R8A7790_CLK_I2C1 R8A7790_CLK_I2C0
			>;
			clock-output-names =
				"gpio5", "gpio4", "gpio3", "gpio2", "gpio1", "gpio0",
				"rcan1", "rcan0", "qspi_mod", "iic3",
				"i2c3", "i2c2", "i2c1", "i2c0";
		};
		mstp10_clks: mstp10_clks@e6150998 {
			compatible = "renesas,r8a7790-mstp-clocks", "renesas,cpg-mstp-clocks";
			reg = <0 0xe6150998 0 4>, <0 0xe61509a8 0 4>;
			clocks = <&p_clk>,
				<&p_clk>, <&p_clk>, <&p_clk>, <&p_clk>, <&p_clk>,
				<&p_clk>, <&p_clk>, <&p_clk>, <&p_clk>, <&p_clk>,
				<&p_clk>,
				<&mstp10_clks R8A7790_CLK_SCU_ALL>, <&mstp10_clks R8A7790_CLK_SCU_ALL>,
				<&mstp10_clks R8A7790_CLK_SCU_ALL>, <&mstp10_clks R8A7790_CLK_SCU_ALL>,
				<&mstp10_clks R8A7790_CLK_SCU_ALL>, <&mstp10_clks R8A7790_CLK_SCU_ALL>,
				<&mstp10_clks R8A7790_CLK_SCU_ALL>, <&mstp10_clks R8A7790_CLK_SCU_ALL>,
				<&mstp10_clks R8A7790_CLK_SCU_ALL>, <&mstp10_clks R8A7790_CLK_SCU_ALL>,
				<&mstp10_clks R8A7790_CLK_SCU_ALL>, <&mstp10_clks R8A7790_CLK_SCU_ALL>;

			#clock-cells = <1>;
			clock-indices = <
				R8A7790_CLK_SSI_ALL
				R8A7790_CLK_SSI9 R8A7790_CLK_SSI8 R8A7790_CLK_SSI7 R8A7790_CLK_SSI6 R8A7790_CLK_SSI5
				R8A7790_CLK_SSI4 R8A7790_CLK_SSI3 R8A7790_CLK_SSI2 R8A7790_CLK_SSI1 R8A7790_CLK_SSI0
				R8A7790_CLK_SCU_ALL
				R8A7790_CLK_SCU_DVC1 R8A7790_CLK_SCU_DVC0
				R8A7790_CLK_SCU_SRC9 R8A7790_CLK_SCU_SRC8 R8A7790_CLK_SCU_SRC7 R8A7790_CLK_SCU_SRC6 R8A7790_CLK_SCU_SRC5
				R8A7790_CLK_SCU_SRC4 R8A7790_CLK_SCU_SRC3 R8A7790_CLK_SCU_SRC2 R8A7790_CLK_SCU_SRC1 R8A7790_CLK_SCU_SRC0
			>;
			clock-output-names =
				"ssi-all",
				"ssi9", "ssi8", "ssi7", "ssi6", "ssi5",
				"ssi4", "ssi3", "ssi2", "ssi1", "ssi0",
				"scu-all",
				"scu-dvc1", "scu-dvc0",
				"scu-src9", "scu-src8", "scu-src7", "scu-src6", "scu-src5",
				"scu-src4", "scu-src3", "scu-src2", "scu-src1", "scu-src0";
		};
	};

	qspi: spi@e6b10000 {
		compatible = "renesas,qspi-r8a7790", "renesas,qspi";
		reg = <0 0xe6b10000 0 0x2c>;
		interrupts = <0 184 IRQ_TYPE_LEVEL_HIGH>;
		clocks = <&mstp9_clks R8A7790_CLK_QSPI_MOD>;
		dmas = <&dmac0 0x17>, <&dmac0 0x18>;
		dma-names = "tx", "rx";
		num-cs = <1>;
		#address-cells = <1>;
		#size-cells = <0>;
		status = "disabled";
	};

	msiof0: spi@e6e20000 {
		compatible = "renesas,msiof-r8a7790";
		reg = <0 0xe6e20000 0 0x0064>, <0 0xe7e20000 0 0x0064>;
		interrupts = <0 156 IRQ_TYPE_LEVEL_HIGH>;
		clocks = <&mstp0_clks R8A7790_CLK_MSIOF0>;
		dmas = <&dmac0 0x51>, <&dmac0 0x52>;
		dma-names = "tx", "rx";
		#address-cells = <1>;
		#size-cells = <0>;
		status = "disabled";
	};

	msiof1: spi@e6e10000 {
		compatible = "renesas,msiof-r8a7790";
		reg = <0 0xe6e10000 0 0x0064>, <0 0xe7e10000 0 0x0064>;
		interrupts = <0 157 IRQ_TYPE_LEVEL_HIGH>;
		clocks = <&mstp2_clks R8A7790_CLK_MSIOF1>;
		dmas = <&dmac0 0x55>, <&dmac0 0x56>;
		dma-names = "tx", "rx";
		#address-cells = <1>;
		#size-cells = <0>;
		status = "disabled";
	};

	msiof2: spi@e6e00000 {
		compatible = "renesas,msiof-r8a7790";
		reg = <0 0xe6e00000 0 0x0064>, <0 0xe7e00000 0 0x0064>;
		interrupts = <0 158 IRQ_TYPE_LEVEL_HIGH>;
		clocks = <&mstp2_clks R8A7790_CLK_MSIOF2>;
		dmas = <&dmac0 0x41>, <&dmac0 0x42>;
		dma-names = "tx", "rx";
		#address-cells = <1>;
		#size-cells = <0>;
		status = "disabled";
	};

	msiof3: spi@e6c90000 {
		compatible = "renesas,msiof-r8a7790";
		reg = <0 0xe6c90000 0 0x0064>, <0 0xe7c90000 0 0x0064>;
		interrupts = <0 159 IRQ_TYPE_LEVEL_HIGH>;
		clocks = <&mstp2_clks R8A7790_CLK_MSIOF3>;
		dmas = <&dmac0 0x45>, <&dmac0 0x46>;
		dma-names = "tx", "rx";
		#address-cells = <1>;
		#size-cells = <0>;
		status = "disabled";
	};

	xhci: usb@ee000000 {
		compatible = "renesas,xhci-r8a7790";
		reg = <0 0xee000000 0 0xc00>;
		interrupts = <0 101 IRQ_TYPE_LEVEL_HIGH>;
		clocks = <&mstp3_clks R8A7790_CLK_SSUSB>;
		phys = <&usb2 1>;
		phy-names = "usb";
		status = "disabled";
	};

	pci0: pci@ee090000 {
		compatible = "renesas,pci-r8a7790";
		device_type = "pci";
		clocks = <&mstp7_clks R8A7790_CLK_EHCI>;
		reg = <0 0xee090000 0 0xc00>,
		      <0 0xee080000 0 0x1100>;
		interrupts = <0 108 IRQ_TYPE_LEVEL_HIGH>;
		status = "disabled";

		bus-range = <0 0>;
		#address-cells = <3>;
		#size-cells = <2>;
		#interrupt-cells = <1>;
		ranges = <0x02000000 0 0xee080000 0 0xee080000 0 0x00010000>;
		interrupt-map-mask = <0xff00 0 0 0x7>;
		interrupt-map = <0x0000 0 0 1 &gic 0 108 IRQ_TYPE_LEVEL_HIGH
				 0x0800 0 0 1 &gic 0 108 IRQ_TYPE_LEVEL_HIGH
				 0x1000 0 0 2 &gic 0 108 IRQ_TYPE_LEVEL_HIGH>;

		usb@0,1 {
			reg = <0x800 0 0 0 0>;
			device_type = "pci";
			phys = <&usb0 0>;
			phy-names = "usb";
		};

		usb@0,2 {
			reg = <0x1000 0 0 0 0>;
			device_type = "pci";
			phys = <&usb0 0>;
			phy-names = "usb";
		};
	};

	pci1: pci@ee0b0000 {
		compatible = "renesas,pci-r8a7790";
		device_type = "pci";
		clocks = <&mstp7_clks R8A7790_CLK_EHCI>;
		reg = <0 0xee0b0000 0 0xc00>,
		      <0 0xee0a0000 0 0x1100>;
		interrupts = <0 112 IRQ_TYPE_LEVEL_HIGH>;
		status = "disabled";

		bus-range = <1 1>;
		#address-cells = <3>;
		#size-cells = <2>;
		#interrupt-cells = <1>;
		ranges = <0x02000000 0 0xee0a0000 0 0xee0a0000 0 0x00010000>;
		interrupt-map-mask = <0xff00 0 0 0x7>;
		interrupt-map = <0x0000 0 0 1 &gic 0 112 IRQ_TYPE_LEVEL_HIGH
				 0x0800 0 0 1 &gic 0 112 IRQ_TYPE_LEVEL_HIGH
				 0x1000 0 0 2 &gic 0 112 IRQ_TYPE_LEVEL_HIGH>;
	};

	pci2: pci@ee0d0000 {
		compatible = "renesas,pci-r8a7790";
		device_type = "pci";
		clocks = <&mstp7_clks R8A7790_CLK_EHCI>;
		reg = <0 0xee0d0000 0 0xc00>,
		      <0 0xee0c0000 0 0x1100>;
		interrupts = <0 113 IRQ_TYPE_LEVEL_HIGH>;
		status = "disabled";

		bus-range = <2 2>;
		#address-cells = <3>;
		#size-cells = <2>;
		#interrupt-cells = <1>;
		ranges = <0x02000000 0 0xee0c0000 0 0xee0c0000 0 0x00010000>;
		interrupt-map-mask = <0xff00 0 0 0x7>;
		interrupt-map = <0x0000 0 0 1 &gic 0 113 IRQ_TYPE_LEVEL_HIGH
				 0x0800 0 0 1 &gic 0 113 IRQ_TYPE_LEVEL_HIGH
				 0x1000 0 0 2 &gic 0 113 IRQ_TYPE_LEVEL_HIGH>;

		usb@0,1 {
			reg = <0x800 0 0 0 0>;
			device_type = "pci";
			phys = <&usb2 0>;
			phy-names = "usb";
		};

		usb@0,2 {
			reg = <0x1000 0 0 0 0>;
			device_type = "pci";
			phys = <&usb2 0>;
			phy-names = "usb";
		};
	};

	pciec: pcie@fe000000 {
		compatible = "renesas,pcie-r8a7790";
		reg = <0 0xfe000000 0 0x80000>;
		#address-cells = <3>;
		#size-cells = <2>;
		bus-range = <0x00 0xff>;
		device_type = "pci";
		ranges = <0x01000000 0 0x00000000 0 0xfe100000 0 0x00100000
			  0x02000000 0 0xfe200000 0 0xfe200000 0 0x00200000
			  0x02000000 0 0x30000000 0 0x30000000 0 0x08000000
			  0x42000000 0 0x38000000 0 0x38000000 0 0x08000000>;
		/* Map all possible DDR as inbound ranges */
		dma-ranges = <0x42000000 0 0x40000000 0 0x40000000 0 0x80000000
			      0x43000000 1 0x80000000 1 0x80000000 0 0x80000000>;
		interrupts = <0 116 IRQ_TYPE_LEVEL_HIGH>,
			     <0 117 IRQ_TYPE_LEVEL_HIGH>,
			     <0 118 IRQ_TYPE_LEVEL_HIGH>;
		#interrupt-cells = <1>;
		interrupt-map-mask = <0 0 0 0>;
		interrupt-map = <0 0 0 0 &gic 0 116 IRQ_TYPE_LEVEL_HIGH>;
		clocks = <&mstp3_clks R8A7790_CLK_PCIEC>, <&pcie_bus_clk>;
		clock-names = "pcie", "pcie_bus";
		status = "disabled";
	};

	rcar_sound: rcar_sound@ec500000 {
		/*
		 * #sound-dai-cells is required
		 *
		 * Single DAI : #sound-dai-cells = <0>;         <&rcar_sound>;
		 * Multi  DAI : #sound-dai-cells = <1>;         <&rcar_sound N>;
		 */
		compatible =  "renesas,rcar_sound-r8a7790", "renesas,rcar_sound-gen2";
		reg =	<0 0xec500000 0 0x1000>, /* SCU */
			<0 0xec5a0000 0 0x100>,  /* ADG */
			<0 0xec540000 0 0x1000>, /* SSIU */
			<0 0xec541000 0 0x1280>; /* SSI */
		clocks = <&mstp10_clks R8A7790_CLK_SSI_ALL>,
			<&mstp10_clks R8A7790_CLK_SSI9>, <&mstp10_clks R8A7790_CLK_SSI8>,
			<&mstp10_clks R8A7790_CLK_SSI7>, <&mstp10_clks R8A7790_CLK_SSI6>,
			<&mstp10_clks R8A7790_CLK_SSI5>, <&mstp10_clks R8A7790_CLK_SSI4>,
			<&mstp10_clks R8A7790_CLK_SSI3>, <&mstp10_clks R8A7790_CLK_SSI2>,
			<&mstp10_clks R8A7790_CLK_SSI1>, <&mstp10_clks R8A7790_CLK_SSI0>,
			<&mstp10_clks R8A7790_CLK_SCU_SRC9>, <&mstp10_clks R8A7790_CLK_SCU_SRC8>,
			<&mstp10_clks R8A7790_CLK_SCU_SRC7>, <&mstp10_clks R8A7790_CLK_SCU_SRC6>,
			<&mstp10_clks R8A7790_CLK_SCU_SRC5>, <&mstp10_clks R8A7790_CLK_SCU_SRC4>,
			<&mstp10_clks R8A7790_CLK_SCU_SRC3>, <&mstp10_clks R8A7790_CLK_SCU_SRC2>,
			<&mstp10_clks R8A7790_CLK_SCU_SRC1>, <&mstp10_clks R8A7790_CLK_SCU_SRC0>,
			<&mstp10_clks R8A7790_CLK_SCU_DVC0>, <&mstp10_clks R8A7790_CLK_SCU_DVC1>,
			<&audio_clk_a>, <&audio_clk_b>, <&audio_clk_c>, <&m2_clk>;
		clock-names = "ssi-all",
				"ssi.9", "ssi.8", "ssi.7", "ssi.6", "ssi.5",
				"ssi.4", "ssi.3", "ssi.2", "ssi.1", "ssi.0",
				"src.9", "src.8", "src.7", "src.6", "src.5",
				"src.4", "src.3", "src.2", "src.1", "src.0",
				"dvc.0", "dvc.1",
				"clk_a", "clk_b", "clk_c", "clk_i";

		status = "disabled";

		rcar_sound,dvc {
			dvc0: dvc@0 { };
			dvc1: dvc@1 { };
		};

		rcar_sound,src {
			src0: src@0 { interrupts = <0 352 IRQ_TYPE_LEVEL_HIGH>; };
			src1: src@1 { interrupts = <0 353 IRQ_TYPE_LEVEL_HIGH>; };
			src2: src@2 { interrupts = <0 354 IRQ_TYPE_LEVEL_HIGH>; };
			src3: src@3 { interrupts = <0 355 IRQ_TYPE_LEVEL_HIGH>; };
			src4: src@4 { interrupts = <0 356 IRQ_TYPE_LEVEL_HIGH>; };
			src5: src@5 { interrupts = <0 357 IRQ_TYPE_LEVEL_HIGH>; };
			src6: src@6 { interrupts = <0 358 IRQ_TYPE_LEVEL_HIGH>; };
			src7: src@7 { interrupts = <0 359 IRQ_TYPE_LEVEL_HIGH>; };
			src8: src@8 { interrupts = <0 360 IRQ_TYPE_LEVEL_HIGH>; };
			src9: src@9 { interrupts = <0 361 IRQ_TYPE_LEVEL_HIGH>; };
		};

		rcar_sound,ssi {
			ssi0: ssi@0 { interrupts = <0 370 IRQ_TYPE_LEVEL_HIGH>; };
			ssi1: ssi@1 { interrupts = <0 371 IRQ_TYPE_LEVEL_HIGH>; };
			ssi2: ssi@2 { interrupts = <0 372 IRQ_TYPE_LEVEL_HIGH>; };
			ssi3: ssi@3 { interrupts = <0 373 IRQ_TYPE_LEVEL_HIGH>; };
			ssi4: ssi@4 { interrupts = <0 374 IRQ_TYPE_LEVEL_HIGH>; };
			ssi5: ssi@5 { interrupts = <0 375 IRQ_TYPE_LEVEL_HIGH>; };
			ssi6: ssi@6 { interrupts = <0 376 IRQ_TYPE_LEVEL_HIGH>; };
			ssi7: ssi@7 { interrupts = <0 377 IRQ_TYPE_LEVEL_HIGH>; };
			ssi8: ssi@8 { interrupts = <0 378 IRQ_TYPE_LEVEL_HIGH>; };
			ssi9: ssi@9 { interrupts = <0 379 IRQ_TYPE_LEVEL_HIGH>; };
		};
	};
};
