#include "dove-cubox.dts"

/ {
	model = "SolidRun CuBox (Engineering Sample)";
	compatible = "solidrun,cubox-es", "solidrun,cubox", "marvell,dove";
};

&sdio0 {
	/* sdio0 card detect is connected to wrong pin on CuBox ES */
	cd-gpios = <&gpio0 12 1>;
	pinctrl-0 = <&pmx_sdio0 &pmx_gpio_12>;
};
