/*
 * Device Tree file for LaCie 2Big Network v2
 *
 * Copyright (C) 2014
 *
 * Andrew Lunn <andrew@lunn.ch>
 *
 * Based on netxbig_v2-setup.c,
 * Copyright (C) 2010 Simon Guinot <sguinot@lacie.com>
 *
 * This file is licensed under the terms of the GNU General Public
 * License version 2.  This program is licensed "as is" without any
 * warranty of any kind, whether express or implied.
*/

/dts-v1/;

#include "kirkwood.dtsi"
#include "kirkwood-6281.dtsi"
#include "kirkwood-netxbig.dtsi"

/ {
	model = "LaCie 2Big Network v2";
	compatible = "lacie,net2big_v2", "lacie,netxbig", "marvell,kirkwood-88f6281", "marvell,kirkwood";

	memory {
		device_type = "memory";
		reg = <0x00000000 0x10000000>;
	};
};

&regulators {
	regulator@2 {
		compatible = "regulator-fixed";
		reg = <2>;
		regulator-name = "hdd1power";
		regulator-min-microvolt = <5000000>;
		regulator-max-microvolt = <5000000>;
		enable-active-high;
		regulator-always-on;
		regulator-boot-on;
		gpio = <&gpio0 17 GPIO_ACTIVE_HIGH>;
	};

	clocks {
	       g762_clk: g762-oscillator {
			 compatible = "fixed-clock";
			 #clock-cells = <0>;
			 clock-frequency = <32768>;
	       };
	};
};

&i2c0 {
	g762@3e {
		compatible = "gmt,g762";
		reg = <0x3e>;
		clocks = <&g762_clk>;
	};
};
