/*
 * Device Tree Source for OMAP2420 SoC
 *
 * Copyright (C) 2012 Texas Instruments Incorporated - http://www.ti.com/
 *
 * This file is licensed under the terms of the GNU General Public License
 * version 2.  This program is licensed "as is" without any warranty of any
 * kind, whether express or implied.
 */

#include "omap2.dtsi"

/ {
	compatible = "ti,omap2420", "ti,omap2";

	ocp {
		prcm: prcm@48008000 {
			compatible = "ti,omap2-prcm";
			reg = <0x48008000 0x1000>;

			prcm_clocks: clocks {
				#address-cells = <1>;
				#size-cells = <0>;
			};

			prcm_clockdomains: clockdomains {
			};
		};

		scrm: scrm@48000000 {
			compatible = "ti,omap2-scrm";
			reg = <0x48000000 0x1000>;

			scrm_clocks: clocks {
				#address-cells = <1>;
				#size-cells = <0>;
			};

			scrm_clockdomains: clockdomains {
			};
		};

		counter32k: counter@48004000 {
			compatible = "ti,omap-counter32k";
			reg = <0x48004000 0x20>;
			ti,hwmods = "counter_32k";
		};

		omap2420_pmx: pinmux@48000030 {
			compatible = "ti,omap2420-padconf", "pinctrl-single";
			reg = <0x48000030 0x0113>;
			#address-cells = <1>;
			#size-cells = <0>;
			pinctrl-single,register-width = <8>;
			pinctrl-single,function-mask = <0x3f>;
		};

		gpio1: gpio@48018000 {
			compatible = "ti,omap2-gpio";
			reg = <0x48018000 0x200>;
			interrupts = <29>;
			ti,hwmods = "gpio1";
			ti,gpio-always-on;
			#gpio-cells = <2>;
			gpio-controller;
			#interrupt-cells = <2>;
			interrupt-controller;
		};

		gpio2: gpio@4801a000 {
			compatible = "ti,omap2-gpio";
			reg = <0x4801a000 0x200>;
			interrupts = <30>;
			ti,hwmods = "gpio2";
			ti,gpio-always-on;
			#gpio-cells = <2>;
			gpio-controller;
			#interrupt-cells = <2>;
			interrupt-controller;
		};

		gpio3: gpio@4801c000 {
			compatible = "ti,omap2-gpio";
			reg = <0x4801c000 0x200>;
			interrupts = <31>;
			ti,hwmods = "gpio3";
			ti,gpio-always-on;
			#gpio-cells = <2>;
			gpio-controller;
			#interrupt-cells = <2>;
			interrupt-controller;
		};

		gpio4: gpio@4801e000 {
			compatible = "ti,omap2-gpio";
			reg = <0x4801e000 0x200>;
			interrupts = <32>;
			ti,hwmods = "gpio4";
			ti,gpio-always-on;
			#gpio-cells = <2>;
			gpio-controller;
			#interrupt-cells = <2>;
			interrupt-controller;
		};

		gpmc: gpmc@6800a000 {
			compatible = "ti,omap2420-gpmc";
			reg = <0x6800a000 0x1000>;
			#address-cells = <2>;
			#size-cells = <1>;
			interrupts = <20>;
			gpmc,num-cs = <8>;
			gpmc,num-waitpins = <4>;
			ti,hwmods = "gpmc";
		};

		mcbsp1: mcbsp@48074000 {
			compatible = "ti,omap2420-mcbsp";
			reg = <0x48074000 0xff>;
			reg-names = "mpu";
			interrupts = <59>, /* TX interrupt */
				     <60>; /* RX interrupt */
			interrupt-names = "tx", "rx";
			ti,hwmods = "mcbsp1";
			dmas = <&sdma 31>,
			       <&sdma 32>;
			dma-names = "tx", "rx";
			status = "disabled";
		};

		mcbsp2: mcbsp@48076000 {
			compatible = "ti,omap2420-mcbsp";
			reg = <0x48076000 0xff>;
			reg-names = "mpu";
			interrupts = <62>, /* TX interrupt */
				     <63>; /* RX interrupt */
			interrupt-names = "tx", "rx";
			ti,hwmods = "mcbsp2";
			dmas = <&sdma 33>,
			       <&sdma 34>;
			dma-names = "tx", "rx";
			status = "disabled";
		};

		msdi1: mmc@4809c000 {
			compatible = "ti,omap2420-mmc";
			ti,hwmods = "msdi1";
			reg = <0x4809c000 0x80>;
			interrupts = <83>;
			dmas = <&sdma 61 &sdma 62>;
			dma-names = "tx", "rx";
		};

		mailbox: mailbox@48094000 {
			compatible = "ti,omap2-mailbox";
			reg = <0x48094000 0x200>;
			interrupts = <26>, <34>;
			interrupt-names = "dsp", "iva";
			ti,hwmods = "mailbox";
			#mbox-cells = <1>;
			ti,mbox-num-users = <4>;
			ti,mbox-num-fifos = <6>;
			mbox_dsp: dsp {
				ti,mbox-tx = <0 0 0>;
				ti,mbox-rx = <1 0 0>;
			};
			mbox_iva: iva {
				ti,mbox-tx = <2 1 3>;
				ti,mbox-rx = <3 1 3>;
			};
		};

		timer1: timer@48028000 {
			compatible = "ti,omap2420-timer";
			reg = <0x48028000 0x400>;
			interrupts = <37>;
			ti,hwmods = "timer1";
			ti,timer-alwon;
		};

		wd_timer2: wdt@48022000 {
			compatible = "ti,omap2-wdt";
			ti,hwmods = "wd_timer2";
			reg = <0x48022000 0x80>;
		};
	};
};

&i2c1 {
	compatible = "ti,omap2420-i2c";
};

&i2c2 {
	compatible = "ti,omap2420-i2c";
};

/include/ "omap24xx-clocks.dtsi"
/include/ "omap2420-clocks.dtsi"
