/*
 * Copyright 2013 Eukréa Electromatique <denis@eukrea.com>
 *
 * This program is free software; you can redistribute it and/or
 * modify it under the terms of the GNU General Public License
 * as published by the Free Software Foundation; either version 2
 * of the License, or (at your option) any later version.
 * This program is distributed in the hope that it will be useful,
 * but WITHOUT ANY WARRANTY; without even the implied warranty of
 * MERCHANTABILITY or FITNESS FOR A PARTICULAR PURPOSE.  See the
 * GNU General Public License for more details.
 */

#include "imx25.dtsi"

/ {
	model = "Eukrea CPUIMX25";
	compatible = "eukrea,cpuimx25", "fsl,imx25";

	memory {
		reg = <0x80000000 0x4000000>; /* 64M */
	};
};

&fec {
	phy-mode = "rmii";
	pinctrl-names = "default";
	pinctrl-0 = <&pinctrl_fec>;
	status = "okay";
};

&i2c1 {
	pinctrl-names = "default";
	pinctrl-0 = <&pinctrl_i2c1>;
	status = "okay";

	pcf8563@51 {
		compatible = "nxp,pcf8563";
		reg = <0x51>;
	};
};

&iomuxc {
	imx25-eukrea-cpuimx25 {
		pinctrl_fec: fecgrp {
			fsl,pins = <
				MX25_PAD_FEC_MDC__FEC_MDC		0x80000000
				MX25_PAD_FEC_MDIO__FEC_MDIO		0x400001e0
				MX25_PAD_FEC_TDATA0__FEC_TDATA0		0x80000000
				MX25_PAD_FEC_TDATA1__FEC_TDATA1		0x80000000
				MX25_PAD_FEC_TX_EN__FEC_TX_EN		0x80000000
				MX25_PAD_FEC_RDATA0__FEC_RDATA0		0x80000000
				MX25_PAD_FEC_RDATA1__FEC_RDATA1		0x80000000
				MX25_PAD_FEC_RX_DV__FEC_RX_DV		0x80000000
				MX25_PAD_FEC_TX_CLK__FEC_TX_CLK		0x1c0
			>;
		};

		pinctrl_i2c1: i2c1grp {
			fsl,pins = <
				MX25_PAD_I2C1_CLK__I2C1_CLK		0x80000000
				MX25_PAD_I2C1_DAT__I2C1_DAT		0x80000000
			>;
		};
	};
};

&nfc {
	nand-bus-width = <8>;
	nand-ecc-mode = "hw";
	nand-on-flash-bbt;
	status = "okay";
};
