/*
 * MPC8572 DS Core1 Device Tree Source in CAMP mode.
 *
 * In CAMP mode, each core needs to have its own dts. Only mpic and L2 cache
 * can be shared, all the other devices must be assigned to one core only.
 * This dts allows core1 to have l2, dma2, eth2, eth3, pci2, msi.
 *
 * Please note to add "-b 1" for core1's dts compiling.
 *
 * Copyright 2007-2009 Freescale Semiconductor Inc.
 *
 * This program is free software; you can redistribute  it and/or modify it
 * under  the terms of  the GNU General  Public License as published by the
 * Free Software Foundation;  either version 2 of the  License, or (at your
 * option) any later version.
 */

/include/ "mpc8572ds.dts"

/ {
	model = "fsl,MPC8572DS";
	compatible = "fsl,MPC8572DS", "fsl,MPC8572DS-CAMP";

	cpus {
		PowerPC,8572@0 {
			status = "disabled";
		};
		PowerPC,8572@1 {
		};
	};

	localbus@ffe05000 {
		status = "disabled";
	};

	soc8572@ffe00000 {
		ecm-law@0 {
			status = "disabled";
		};
		ecm@1000 {
			status = "disabled";
		};
		memory-controller@2000 {
			status = "disabled";
		};
		memory-controller@6000 {
			status = "disabled";
		};
		i2c@3000 {
			status = "disabled";
		};
		i2c@3100 {
			status = "disabled";
		};
		serial@4500 {
			status = "disabled";
		};
		gpio-controller@f000 {
			status = "disabled";
		};
		l2-cache-controller@20000 {
			cache-size = <0x80000>;	// L2, 512K
		};
		dma@21300 {
			status = "disabled";
		};
		ethernet@24000 {
			status = "disabled";
		};
		ptp_clock@24e00 {
			status = "disabled";
		};
		ethernet@25000 {
			status = "disabled";
		};
		mdio@25520 {
			status = "disabled";
		};
		crypto@30000 {
			status = "disabled";
		};
		pic@40000 {
			protected-sources = <
			18 16 10 42 45 58	/* MEM L2 mdio serial crypto */
			29 30 34 35 36 40	/* enet0 enet1 */
			24 25 20 21 22 23	/* pci0 pci1 dma1 */
			43			/* i2c */
			0x1 0x2 0x3 0x4         /* pci slot */
			0x9 0xa 0xb 0xc         /* usb */
			0x6 0x7 0xe 0x5         /* Audio elgacy SATA */
			0xe0 0xe1 0xe2 0xe3	/* msi */
			>;
		};
		timer@41100 {
			status = "disabled";
		};
		msi@41600 {
			msi-available-ranges = <0x80 0x80>;
			interrupts = <
				0xe4 0 0 0
				0xe5 0 0 0
				0xe6 0 0 0
				0xe7 0 0 0>;
		};
		global-utilities@e0000 {
			status = "disabled";
		};
	};
	pcie@ffe08000 {
		status = "disabled";
	};
	pcie@ffe09000 {
		status = "disabled";
	};
};
