/*
 * Samsung's Exynos4415 SoC device tree source
 *
 * Copyright (c) 2014 Samsung Electronics Co., Ltd.
 *
 * Samsung's Exynos4415 SoC device nodes are listed in this file. Exynos4415
 * based board files can include this file and provide values for board
 * specific bindings.
 *
 * Note: This file does not include device nodes for all the controllers in
 * Exynos4415 SoC. As device tree coverage for Exynos4415 increases, additional
 * nodes can be added to this file.
 *
 * This program is free software; you can redistribute it and/or modify
 * it under the terms of the GNU General Public License version 2 as
 * published by the Free Software Foundation.
 */

#include "skeleton.dtsi"
#include <dt-bindings/clock/exynos4415.h>
#include <dt-bindings/clock/exynos-audss-clk.h>

/ {
	compatible = "samsung,exynos4415";
	interrupt-parent = <&gic>;

	aliases {
		pinctrl0 = &pinctrl_0;
		pinctrl1 = &pinctrl_1;
		pinctrl2 = &pinctrl_2;
		mshc0 = &mshc_0;
		mshc1 = &mshc_1;
		mshc2 = &mshc_2;
		spi0 = &spi_0;
		spi1 = &spi_1;
		spi2 = &spi_2;
		i2c0 = &i2c_0;
		i2c1 = &i2c_1;
		i2c2 = &i2c_2;
		i2c3 = &i2c_3;
		i2c4 = &i2c_4;
		i2c5 = &i2c_5;
		i2c6 = &i2c_6;
		i2c7 = &i2c_7;
	};

	cpus {
		#address-cells = <1>;
		#size-cells = <0>;

		cpu0: cpu@a00 {
			device_type = "cpu";
			compatible = "arm,cortex-a9";
			reg = <0xa00>;
			clock-frequency = <1600000000>;
		};

		cpu1: cpu@a01 {
			device_type = "cpu";
			compatible = "arm,cortex-a9";
			reg = <0xa01>;
			clock-frequency = <1600000000>;
		};

		cpu2: cpu@a02 {
			device_type = "cpu";
			compatible = "arm,cortex-a9";
			reg = <0xa02>;
			clock-frequency = <1600000000>;
		};

		cpu3: cpu@a03 {
			device_type = "cpu";
			compatible = "arm,cortex-a9";
			reg = <0xa03>;
			clock-frequency = <1600000000>;
		};
	};

	soc: soc {
		compatible = "simple-bus";
		#address-cells = <1>;
		#size-cells = <1>;
		ranges;

		sysram@02020000 {
			compatible = "mmio-sram";
			reg = <0x02020000 0x50000>;
			#address-cells = <1>;
			#size-cells = <1>;
			ranges = <0 0x02020000 0x50000>;

			smp-sysram@0 {
				compatible = "samsung,exynos4210-sysram";
				reg = <0x0 0x1000>;
			};

			smp-sysram@4f000 {
				compatible = "samsung,exynos4210-sysram-ns";
				reg = <0x4f000 0x1000>;
			};
		};

		pinctrl_2: pinctrl@03860000 {
			compatible = "samsung,exynos4415-pinctrl";
			reg = <0x03860000 0x1000>;
			interrupts = <0 242 0>;
		};

		chipid@10000000 {
			compatible = "samsung,exynos4210-chipid";
			reg = <0x10000000 0x100>;
		};

		sysreg_system_controller: syscon@10010000 {
			compatible = "samsung,exynos4-sysreg", "syscon";
			reg = <0x10010000 0x400>;
		};

		pmu_system_controller: system-controller@10020000 {
			compatible = "samsung,exynos4415-pmu", "syscon";
			reg = <0x10020000 0x4000>;
		};

		mipi_phy: video-phy@10020710 {
			compatible = "samsung,s5pv210-mipi-video-phy";
			reg = <0x10020710 8>;
			#phy-cells = <1>;
		};

		pd_cam: cam-power-domain@10024000 {
			compatible = "samsung,exynos4210-pd";
			reg = <0x10024000 0x20>;
			#power-domain-cells = <0>;
		};

		pd_tv: tv-power-domain@10024020 {
			compatible = "samsung,exynos4210-pd";
			reg = <0x10024020 0x20>;
			#power-domain-cells = <0>;
		};

		pd_mfc: mfc-power-domain@10024040 {
			compatible = "samsung,exynos4210-pd";
			reg = <0x10024040 0x20>;
			#power-domain-cells = <0>;
		};

		pd_g3d: g3d-power-domain@10024060 {
			compatible = "samsung,exynos4210-pd";
			reg = <0x10024060 0x20>;
			#power-domain-cells = <0>;
		};

		pd_lcd0: lcd0-power-domain@10024080 {
			compatible = "samsung,exynos4210-pd";
			reg = <0x10024080 0x20>;
			#power-domain-cells = <0>;
		};

		pd_isp0: isp0-power-domain@100240A0 {
			compatible = "samsung,exynos4210-pd";
			reg = <0x100240A0 0x20>;
			#power-domain-cells = <0>;
		};

		pd_isp1: isp1-power-domain@100240E0 {
			compatible = "samsung,exynos4210-pd";
			reg = <0x100240E0 0x20>;
			#power-domain-cells = <0>;
		};

		cmu: clock-controller@10030000 {
			compatible = "samsung,exynos4415-cmu";
			reg = <0x10030000 0x18000>;
			#clock-cells = <1>;
		};

		rtc: rtc@10070000 {
			compatible = "samsung,exynos3250-rtc";
			reg = <0x10070000 0x100>;
			interrupts = <0 73 0>, <0 74 0>;
			status = "disabled";
		};

		mct@10050000 {
			compatible = "samsung,exynos4210-mct";
			reg = <0x10050000 0x800>;
			interrupts = <0 218 0>, <0 219 0>, <0 220 0>, <0 221 0>,
				     <0 223 0>, <0 226 0>, <0 227 0>, <0 228 0>;
			clocks = <&cmu CLK_FIN_PLL>, <&cmu CLK_MCT>;
			clock-names = "fin_pll", "mct";
		};

		gic: interrupt-controller@10481000 {
			compatible = "arm,cortex-a9-gic";
			#interrupt-cells = <3>;
			interrupt-controller;
			reg = <0x10481000 0x1000>,
			      <0x10482000 0x1000>,
			      <0x10484000 0x2000>,
			      <0x10486000 0x2000>;
			interrupts = <1 9 0xf04>;
		};

		l2c: l2-cache-controller@10502000 {
			compatible = "arm,pl310-cache";
			reg = <0x10502000 0x1000>;
			cache-unified;
			cache-level = <2>;
			arm,tag-latency = <2 2 1>;
			arm,data-latency = <3 2 1>;
			arm,double-linefill = <1>;
			arm,double-linefill-incr = <0>;
			arm,double-linefill-wrap = <1>;
			arm,prefetch-drop = <1>;
			arm,prefetch-offset = <7>;
		};

		cmu_dmc: clock-controller@105C0000 {
			compatible = "samsung,exynos4415-cmu-dmc";
			reg = <0x105C0000 0x3000>;
			#clock-cells = <1>;
		};

		pinctrl_1: pinctrl@11000000 {
			compatible = "samsung,exynos4415-pinctrl";
			reg = <0x11000000 0x1000>;
			interrupts = <0 225 0>;

			wakeup-interrupt-controller {
				compatible = "samsung,exynos4210-wakeup-eint";
				interrupt-parent = <&gic>;
				interrupts = <0 48 0>;
			};
		};

		pinctrl_0: pinctrl@11400000 {
			compatible = "samsung,exynos4415-pinctrl";
			reg = <0x11400000 0x1000>;
			interrupts = <0 240 0>;
		};

		fimd: fimd@11C00000 {
			compatible = "samsung,exynos4415-fimd";
			reg = <0x11C00000 0x30000>;
			interrupt-names = "fifo", "vsync", "lcd_sys";
			interrupts = <0 84 0>, <0 85 0>, <0 86 0>;
			clocks = <&cmu CLK_SCLK_FIMD0>, <&cmu CLK_FIMD0>;
			clock-names = "sclk_fimd", "fimd";
			samsung,power-domain = <&pd_lcd0>;
			samsung,sysreg = <&sysreg_system_controller>;
			status = "disabled";
		};

		dsi_0: dsi@11C80000 {
			compatible = "samsung,exynos4415-mipi-dsi";
			reg = <0x11C80000 0x10000>;
			interrupts = <0 83 0>;
			samsung,phy-type = <0>;
			samsung,power-domain = <&pd_lcd0>;
			phys = <&mipi_phy 1>;
			phy-names = "dsim";
			clocks = <&cmu CLK_DSIM0>, <&cmu CLK_SCLK_MIPI0>;
			clock-names = "bus_clk", "pll_clk";
			#address-cells = <1>;
			#size-cells = <0>;
			status = "disabled";
		};

		hsotg: hsotg@12480000 {
			compatible = "samsung,s3c6400-hsotg";
			reg = <0x12480000 0x20000>;
			interrupts = <0 141 0>;
			clocks = <&cmu CLK_USBDEVICE>;
			clock-names = "otg";
			phys = <&exynos_usbphy 0>;
			phy-names = "usb2-phy";
			status = "disabled";
		};

		mshc_0: mshc@12510000 {
			compatible = "samsung,exynos5250-dw-mshc";
			reg = <0x12510000 0x1000>;
			interrupts = <0 142 0>;
			clocks = <&cmu CLK_SDMMC0>, <&cmu CLK_SCLK_MMC0>;
			clock-names = "biu", "ciu";
			fifo-depth = <0x80>;
			#address-cells = <1>;
			#size-cells = <0>;
			status = "disabled";
		};

		mshc_1: mshc@12520000 {
			compatible = "samsung,exynos5250-dw-mshc";
			reg = <0x12520000 0x1000>;
			interrupts = <0 143 0>;
			clocks = <&cmu CLK_SDMMC1>, <&cmu CLK_SCLK_MMC1>;
			clock-names = "biu", "ciu";
			fifo-depth = <0x80>;
			#address-cells = <1>;
			#size-cells = <0>;
			status = "disabled";
		};

		mshc_2: mshc@12530000 {
			compatible = "samsung,exynos5250-dw-mshc";
			reg = <0x12530000 0x1000>;
			interrupts = <0 144 0>;
			clocks = <&cmu CLK_SDMMC2>, <&cmu CLK_SCLK_MMC2>;
			clock-names = "biu", "ciu";
			fifo-depth = <0x80>;
			#address-cells = <1>;
			#size-cells = <0>;
			status = "disabled";
		};

		ehci: ehci@12580000 {
			compatible = "samsung,exynos4210-ehci";
			reg = <0x12580000 0x100>;
			interrupts = <0 140 0>;
			clocks = <&cmu CLK_USBHOST>;
			clock-names = "usbhost";
			status = "disabled";
			#address-cells = <1>;
			#size-cells = <0>;
			port@0 {
				reg = <0>;
				phys = <&exynos_usbphy 1>;
				status = "disabled";
			};
			port@1 {
				reg = <1>;
				phys = <&exynos_usbphy 2>;
				status = "disabled";
			};
			port@2 {
				reg = <2>;
				phys = <&exynos_usbphy 3>;
				status = "disabled";
			};
		};

		ohci: ohci@12590000 {
			compatible = "samsung,exynos4210-ohci";
			reg = <0x12590000 0x100>;
			interrupts = <0 140 0>;
			clocks = <&cmu CLK_USBHOST>;
			clock-names = "usbhost";
			status = "disabled";
			#address-cells = <1>;
			#size-cells = <0>;
			port@0 {
				reg = <0>;
				phys = <&exynos_usbphy 1>;
				status = "disabled";
			};
		};

		exynos_usbphy: exynos-usbphy@125B0000 {
			compatible = "samsung,exynos4x12-usb2-phy";
			reg = <0x125B0000 0x100>;
			samsung,pmureg-phandle = <&pmu_system_controller>;
			samsung,sysreg-phandle = <&sysreg_system_controller>;
			clocks = <&cmu CLK_USBDEVICE>, <&xusbxti>;
			clock-names = "phy", "ref";
			#phy-cells = <1>;
			status = "disabled";
		};

		amba {
			compatible = "arm,amba-bus";
			#address-cells = <1>;
			#size-cells = <1>;
			interrupt-parent = <&gic>;
			ranges;

			pdma0: pdma@12680000 {
				compatible = "arm,pl330", "arm,primecell";
				reg = <0x12680000 0x1000>;
				interrupts = <0 138 0>;
				clocks = <&cmu CLK_PDMA0>;
				clock-names = "apb_pclk";
				#dma-cells = <1>;
				#dma-channels = <8>;
				#dma-requests = <32>;
			};

			pdma1: pdma@12690000 {
				compatible = "arm,pl330", "arm,primecell";
				reg = <0x12690000 0x1000>;
				interrupts = <0 139 0>;
				clocks = <&cmu CLK_PDMA1>;
				clock-names = "apb_pclk";
				#dma-cells = <1>;
				#dma-channels = <8>;
				#dma-requests = <32>;
			};
		};

		adc: adc@126C0000 {
			compatible = "samsung,exynos3250-adc",
				     "samsung,exynos-adc-v2";
			reg = <0x126C0000 0x100>, <0x10020718 0x4>;
			interrupts = <0 137 0>;
			clock-names = "adc", "sclk";
			clocks = <&cmu CLK_TSADC>, <&cmu CLK_SCLK_TSADC>;
			#io-channel-cells = <1>;
			io-channel-ranges;
			status = "disabled";
		};

		serial_0: serial@13800000 {
			compatible = "samsung,exynos4210-uart";
			reg = <0x13800000 0x100>;
			interrupts = <0 109 0>;
			clocks = <&cmu CLK_UART0>, <&cmu CLK_SCLK_UART0>;
			clock-names = "uart", "clk_uart_baud0";
			status = "disabled";
		};

		serial_1: serial@13810000 {
			compatible = "samsung,exynos4210-uart";
			reg = <0x13810000 0x100>;
			interrupts = <0 110 0>;
			clocks = <&cmu CLK_UART1>, <&cmu CLK_SCLK_UART1>;
			clock-names = "uart", "clk_uart_baud0";
			status = "disabled";
		};

		serial_2: serial@13820000 {
			compatible = "samsung,exynos4210-uart";
			reg = <0x13820000 0x100>;
			interrupts = <0 111 0>;
			clocks = <&cmu CLK_UART2>, <&cmu CLK_SCLK_UART2>;
			clock-names = "uart", "clk_uart_baud0";
			status = "disabled";
		};

		serial_3: serial@13830000 {
			compatible = "samsung,exynos4210-uart";
			reg = <0x13830000 0x100>;
			interrupts = <0 112 0>;
			clocks = <&cmu CLK_UART3>, <&cmu CLK_SCLK_UART3>;
			clock-names = "uart", "clk_uart_baud0";
			status = "disabled";
		};

		i2c_0: i2c@13860000 {
			#address-cells = <1>;
			#size-cells = <0>;
			compatible = "samsung,s3c2440-i2c";
			reg = <0x13860000 0x100>;
			interrupts = <0 113 0>;
			clocks = <&cmu CLK_I2C0>;
			clock-names = "i2c";
			pinctrl-names = "default";
			pinctrl-0 = <&i2c0_bus>;
			status = "disabled";
		};

		i2c_1: i2c@13870000 {
			#address-cells = <1>;
			#size-cells = <0>;
			compatible = "samsung,s3c2440-i2c";
			reg = <0x13870000 0x100>;
			interrupts = <0 114 0>;
			clocks = <&cmu CLK_I2C1>;
			clock-names = "i2c";
			pinctrl-names = "default";
			pinctrl-0 = <&i2c1_bus>;
			status = "disabled";
		};

		i2c_2: i2c@13880000 {
			#address-cells = <1>;
			#size-cells = <0>;
			compatible = "samsung,s3c2440-i2c";
			reg = <0x13880000 0x100>;
			interrupts = <0 115 0>;
			clocks = <&cmu CLK_I2C2>;
			clock-names = "i2c";
			pinctrl-names = "default";
			pinctrl-0 = <&i2c2_bus>;
			status = "disabled";
		};

		i2c_3: i2c@13890000 {
			#address-cells = <1>;
			#size-cells = <0>;
			compatible = "samsung,s3c2440-i2c";
			reg = <0x13890000 0x100>;
			interrupts = <0 116 0>;
			clocks = <&cmu CLK_I2C3>;
			clock-names = "i2c";
			pinctrl-names = "default";
			pinctrl-0 = <&i2c3_bus>;
			status = "disabled";
		};

		i2c_4: i2c@138A0000 {
			#address-cells = <1>;
			#size-cells = <0>;
			compatible = "samsung,s3c2440-i2c";
			reg = <0x138A0000 0x100>;
			interrupts = <0 117 0>;
			clocks = <&cmu CLK_I2C4>;
			clock-names = "i2c";
			pinctrl-names = "default";
			pinctrl-0 = <&i2c4_bus>;
			status = "disabled";
		};

		i2c_5: i2c@138B0000 {
			#address-cells = <1>;
			#size-cells = <0>;
			compatible = "samsung,s3c2440-i2c";
			reg = <0x138B0000 0x100>;
			interrupts = <0 118 0>;
			clocks = <&cmu CLK_I2C5>;
			clock-names = "i2c";
			pinctrl-names = "default";
			pinctrl-0 = <&i2c5_bus>;
			status = "disabled";
		};

		i2c_6: i2c@138C0000 {
			#address-cells = <1>;
			#size-cells = <0>;
			compatible = "samsung,s3c2440-i2c";
			reg = <0x138C0000 0x100>;
			interrupts = <0 119 0>;
			clocks = <&cmu CLK_I2C6>;
			clock-names = "i2c";
			pinctrl-names = "default";
			pinctrl-0 = <&i2c6_bus>;
			status = "disabled";
		};

		i2c_7: i2c@138D0000 {
			#address-cells = <1>;
			#size-cells = <0>;
			compatible = "samsung,s3c2440-i2c";
			reg = <0x138D0000 0x100>;
			interrupts = <0 120 0>;
			clocks = <&cmu CLK_I2C7>;
			clock-names = "i2c";
			pinctrl-names = "default";
			pinctrl-0 = <&i2c7_bus>;
			status = "disabled";
		};

		spi_0: spi@13920000 {
			compatible = "samsung,exynos4210-spi";
			reg = <0x13920000 0x100>;
			interrupts = <0 121 0>;
			dmas = <&pdma0 7>, <&pdma0 6>;
			dma-names = "tx", "rx";
			#address-cells = <1>;
			#size-cells = <0>;
			clocks = <&cmu CLK_SPI0>, <&cmu CLK_SCLK_SPI0>;
			clock-names = "spi", "spi_busclk0";
			samsung,spi-src-clk = <0>;
			pinctrl-names = "default";
			pinctrl-0 = <&spi0_bus>;
			status = "disabled";
		};

		spi_1: spi@13930000 {
			compatible = "samsung,exynos4210-spi";
			reg = <0x13930000 0x100>;
			interrupts = <0 122 0>;
			dmas = <&pdma1 7>, <&pdma1 6>;
			dma-names = "tx", "rx";
			#address-cells = <1>;
			#size-cells = <0>;
			clocks = <&cmu CLK_SPI1>, <&cmu CLK_SCLK_SPI1>;
			clock-names = "spi", "spi_busclk0";
			samsung,spi-src-clk = <0>;
			pinctrl-names = "default";
			pinctrl-0 = <&spi1_bus>;
			status = "disabled";
		};

		spi_2: spi@13940000 {
			compatible = "samsung,exynos4210-spi";
			reg = <0x13940000 0x100>;
			interrupts = <0 123 0>;
			dmas = <&pdma0 9>, <&pdma0 8>;
			dma-names = "tx", "rx";
			#address-cells = <1>;
			#size-cells = <0>;
			clocks = <&cmu CLK_SPI2>, <&cmu CLK_SCLK_SPI2>;
			clock-names = "spi", "spi_busclk0";
			samsung,spi-src-clk = <0>;
			pinctrl-names = "default";
			pinctrl-0 = <&spi2_bus>;
			status = "disabled";
		};

		clock_audss: clock-controller@03810000 {
			compatible = "samsung,exynos4210-audss-clock";
			reg = <0x03810000 0x0C>;
			#clock-cells = <1>;
		};

		i2s0: i2s@3830000 {
			compatible = "samsung,s5pv210-i2s";
			reg = <0x03830000 0x100>;
			interrupts = <0 124 0>;
			clocks = <&clock_audss EXYNOS_I2S_BUS>,
				<&clock_audss EXYNOS_SCLK_I2S>;
			clock-names = "iis", "i2s_opclk0";
			dmas = <&pdma1 10>, <&pdma1 9>, <&pdma1 8>;
			dma-names = "tx", "rx", "tx-sec";
			pinctrl-names = "default";
			pinctrl-0 = <&i2s0_bus>;
			samsung,idma-addr = <0x03000000>;
			status = "disabled";
		};

		pwm: pwm@139D0000 {
			compatible = "samsung,exynos4210-pwm";
			reg = <0x139D0000 0x1000>;
			interrupts = <0 104 0>, <0 105 0>, <0 106 0>,
				     <0 107 0>, <0 108 0>;
			#pwm-cells = <3>;
			status = "disabled";
		};

		pmu {
			compatible = "arm,cortex-a9-pmu";
			interrupts = <0 18 0>, <0 19 0>, <0 20 0>, <0 21 0>;
		};
	};
};

#include "exynos4415-pinctrl.dtsi"
