/*
 * Copyright (c) 2015, The Linux Foundation. All rights reserved.
 *
 * This program is free software; you can redistribute it and/or modify
 * it under the terms of the GNU General Public License version 2 and
 * only version 2 as published by the Free Software Foundation.
 *
 * This program is distributed in the hope that it will be useful,
 * but WITHOUT ANY WARRANTY; without even the implied warranty of
 * MERCHANTABILITY or FITNESS FOR A PARTICULAR PURPOSE.  See the
 * GNU General Public License for more details.
 */

#include "msm8916.dtsi"

/ {
	aliases {
		serial0 = &blsp1_uart2;
	};

	chosen {
		stdout-path = "serial0";
	};

	soc {
		serial@78b0000 {
			status = "okay";
			pinctrl-names = "default", "sleep";
			pinctrl-0 = <&blsp1_uart2_default>;
			pinctrl-1 = <&blsp1_uart2_sleep>;
		};
	};
};
