/*
 * Copyright 2014 Freescale Semiconductor, Inc.
 *
 * This program is free software; you can redistribute it and/or modify
 * it under the terms of the GNU General Public License version 2 as
 * published by the Free Software Foundation.
 */

#include <dt-bindings/clock/imx6sx-clock.h>
#include <dt-bindings/gpio/gpio.h>
#include <dt-bindings/interrupt-controller/arm-gic.h>
#include "imx6sx-pinfunc.h"
#include "skeleton.dtsi"

/ {
	aliases {
		can0 = &flexcan1;
		can1 = &flexcan2;
		ethernet0 = &fec1;
		ethernet1 = &fec2;
		gpio0 = &gpio1;
		gpio1 = &gpio2;
		gpio2 = &gpio3;
		gpio3 = &gpio4;
		gpio4 = &gpio5;
		gpio5 = &gpio6;
		gpio6 = &gpio7;
		i2c0 = &i2c1;
		i2c1 = &i2c2;
		i2c2 = &i2c3;
		i2c3 = &i2c4;
		mmc0 = &usdhc1;
		mmc1 = &usdhc2;
		mmc2 = &usdhc3;
		mmc3 = &usdhc4;
		serial0 = &uart1;
		serial1 = &uart2;
		serial2 = &uart3;
		serial3 = &uart4;
		serial4 = &uart5;
		serial5 = &uart6;
		spi0 = &ecspi1;
		spi1 = &ecspi2;
		spi2 = &ecspi3;
		spi3 = &ecspi4;
		spi4 = &ecspi5;
		usbphy0 = &usbphy1;
		usbphy1 = &usbphy2;
	};

	cpus {
		#address-cells = <1>;
		#size-cells = <0>;

		cpu0: cpu@0 {
			compatible = "arm,cortex-a9";
			device_type = "cpu";
			reg = <0>;
			next-level-cache = <&L2>;
			operating-points = <
				/* kHz    uV */
				996000  1250000
				792000  1175000
				396000  1075000
			>;
			fsl,soc-operating-points = <
				/* ARM kHz  SOC uV */
				996000      1175000
				792000      1175000
				396000      1175000
			>;
			clock-latency = <61036>; /* two CLK32 periods */
			clocks = <&clks IMX6SX_CLK_ARM>,
				 <&clks IMX6SX_CLK_PLL2_PFD2>,
				 <&clks IMX6SX_CLK_STEP>,
				 <&clks IMX6SX_CLK_PLL1_SW>,
				 <&clks IMX6SX_CLK_PLL1_SYS>;
			clock-names = "arm", "pll2_pfd2_396m", "step",
				      "pll1_sw", "pll1_sys";
			arm-supply = <&reg_arm>;
			soc-supply = <&reg_soc>;
		};
	};

	intc: interrupt-controller@00a01000 {
		compatible = "arm,cortex-a9-gic";
		#interrupt-cells = <3>;
		interrupt-controller;
		reg = <0x00a01000 0x1000>,
		      <0x00a00100 0x100>;
		interrupt-parent = <&intc>;
	};

	clocks {
		#address-cells = <1>;
		#size-cells = <0>;

		ckil: clock@0 {
			compatible = "fixed-clock";
			reg = <0>;
			#clock-cells = <0>;
			clock-frequency = <32768>;
			clock-output-names = "ckil";
		};

		osc: clock@1 {
			compatible = "fixed-clock";
			reg = <1>;
			#clock-cells = <0>;
			clock-frequency = <24000000>;
			clock-output-names = "osc";
		};

		ipp_di0: clock@2 {
			compatible = "fixed-clock";
			reg = <2>;
			#clock-cells = <0>;
			clock-frequency = <0>;
			clock-output-names = "ipp_di0";
		};

		ipp_di1: clock@3 {
			compatible = "fixed-clock";
			reg = <3>;
			#clock-cells = <0>;
			clock-frequency = <0>;
			clock-output-names = "ipp_di1";
		};
	};

	soc {
		#address-cells = <1>;
		#size-cells = <1>;
		compatible = "simple-bus";
		interrupt-parent = <&gpc>;
		ranges;

		pmu {
			compatible = "arm,cortex-a9-pmu";
			interrupts = <GIC_SPI 94 IRQ_TYPE_LEVEL_HIGH>;
		};

		ocram: sram@00900000 {
			compatible = "mmio-sram";
			reg = <0x00900000 0x20000>;
			clocks = <&clks IMX6SX_CLK_OCRAM>;
		};

		L2: l2-cache@00a02000 {
			compatible = "arm,pl310-cache";
			reg = <0x00a02000 0x1000>;
			interrupts = <GIC_SPI 92 IRQ_TYPE_LEVEL_HIGH>;
			cache-unified;
			cache-level = <2>;
			arm,tag-latency = <4 2 3>;
			arm,data-latency = <4 2 3>;
		};

		dma_apbh: dma-apbh@01804000 {
			compatible = "fsl,imx6sx-dma-apbh", "fsl,imx28-dma-apbh";
			reg = <0x01804000 0x2000>;
			interrupts = <GIC_SPI 13 IRQ_TYPE_LEVEL_HIGH>,
				     <GIC_SPI 13 IRQ_TYPE_LEVEL_HIGH>,
				     <GIC_SPI 13 IRQ_TYPE_LEVEL_HIGH>,
				     <GIC_SPI 13 IRQ_TYPE_LEVEL_HIGH>;
			interrupt-names = "gpmi0", "gpmi1", "gpmi2", "gpmi3";
			#dma-cells = <1>;
			dma-channels = <4>;
			clocks = <&clks IMX6SX_CLK_APBH_DMA>;
		};

		gpmi: gpmi-nand@01806000{
			compatible = "fsl,imx6sx-gpmi-nand";
			#address-cells = <1>;
			#size-cells = <1>;
			reg = <0x01806000 0x2000>, <0x01808000 0x4000>;
			reg-names = "gpmi-nand", "bch";
			interrupts = <GIC_SPI 15 IRQ_TYPE_LEVEL_HIGH>;
			interrupt-names = "bch";
			clocks = <&clks IMX6SX_CLK_GPMI_IO>,
				 <&clks IMX6SX_CLK_GPMI_APB>,
				 <&clks IMX6SX_CLK_GPMI_BCH>,
				 <&clks IMX6SX_CLK_GPMI_BCH_APB>,
				 <&clks IMX6SX_CLK_PER1_BCH>;
			clock-names = "gpmi_io", "gpmi_apb", "gpmi_bch",
				      "gpmi_bch_apb", "per1_bch";
			dmas = <&dma_apbh 0>;
			dma-names = "rx-tx";
			status = "disabled";
		};

		aips1: aips-bus@02000000 {
			compatible = "fsl,aips-bus", "simple-bus";
			#address-cells = <1>;
			#size-cells = <1>;
			reg = <0x02000000 0x100000>;
			ranges;

			spba-bus@02000000 {
				compatible = "fsl,spba-bus", "simple-bus";
				#address-cells = <1>;
				#size-cells = <1>;
				reg = <0x02000000 0x40000>;
				ranges;

				spdif: spdif@02004000 {
					compatible = "fsl,imx6sx-spdif", "fsl,imx35-spdif";
					reg = <0x02004000 0x4000>;
					interrupts = <GIC_SPI 52 IRQ_TYPE_LEVEL_HIGH>;
					dmas = <&sdma 14 18 0>,
					       <&sdma 15 18 0>;
					dma-names = "rx", "tx";
					clocks = <&clks IMX6SX_CLK_SPDIF>,
						 <&clks IMX6SX_CLK_OSC>,
						 <&clks IMX6SX_CLK_SPDIF>,
						 <&clks 0>, <&clks 0>, <&clks 0>,
						 <&clks IMX6SX_CLK_IPG>,
						 <&clks 0>, <&clks 0>,
						 <&clks IMX6SX_CLK_SPBA>;
					clock-names = "core", "rxtx0",
						      "rxtx1", "rxtx2",
						      "rxtx3", "rxtx4",
						      "rxtx5", "rxtx6",
						      "rxtx7", "dma";
					status = "disabled";
				};

				ecspi1: ecspi@02008000 {
					#address-cells = <1>;
					#size-cells = <0>;
					compatible = "fsl,imx6sx-ecspi", "fsl,imx51-ecspi";
					reg = <0x02008000 0x4000>;
					interrupts = <GIC_SPI 31 IRQ_TYPE_LEVEL_HIGH>;
					clocks = <&clks IMX6SX_CLK_ECSPI1>,
						 <&clks IMX6SX_CLK_ECSPI1>;
					clock-names = "ipg", "per";
					status = "disabled";
				};

				ecspi2: ecspi@0200c000 {
					#address-cells = <1>;
					#size-cells = <0>;
					compatible = "fsl,imx6sx-ecspi", "fsl,imx51-ecspi";
					reg = <0x0200c000 0x4000>;
					interrupts = <GIC_SPI 32 IRQ_TYPE_LEVEL_HIGH>;
					clocks = <&clks IMX6SX_CLK_ECSPI2>,
						 <&clks IMX6SX_CLK_ECSPI2>;
					clock-names = "ipg", "per";
					status = "disabled";
				};

				ecspi3: ecspi@02010000 {
					#address-cells = <1>;
					#size-cells = <0>;
					compatible = "fsl,imx6sx-ecspi", "fsl,imx51-ecspi";
					reg = <0x02010000 0x4000>;
					interrupts = <GIC_SPI 33 IRQ_TYPE_LEVEL_HIGH>;
					clocks = <&clks IMX6SX_CLK_ECSPI3>,
						 <&clks IMX6SX_CLK_ECSPI3>;
					clock-names = "ipg", "per";
					status = "disabled";
				};

				ecspi4: ecspi@02014000 {
					#address-cells = <1>;
					#size-cells = <0>;
					compatible = "fsl,imx6sx-ecspi", "fsl,imx51-ecspi";
					reg = <0x02014000 0x4000>;
					interrupts = <GIC_SPI 34 IRQ_TYPE_LEVEL_HIGH>;
					clocks = <&clks IMX6SX_CLK_ECSPI4>,
						 <&clks IMX6SX_CLK_ECSPI4>;
					clock-names = "ipg", "per";
					status = "disabled";
				};

				uart1: serial@02020000 {
					compatible = "fsl,imx6sx-uart", "fsl,imx21-uart";
					reg = <0x02020000 0x4000>;
					interrupts = <GIC_SPI 26 IRQ_TYPE_LEVEL_HIGH>;
					clocks = <&clks IMX6SX_CLK_UART_IPG>,
						 <&clks IMX6SX_CLK_UART_SERIAL>;
					clock-names = "ipg", "per";
					dmas = <&sdma 25 4 0>, <&sdma 26 4 0>;
					dma-names = "rx", "tx";
					status = "disabled";
				};

				esai: esai@02024000 {
					reg = <0x02024000 0x4000>;
					interrupts = <GIC_SPI 51 IRQ_TYPE_LEVEL_HIGH>;
					clocks = <&clks IMX6SX_CLK_ESAI_IPG>,
						 <&clks IMX6SX_CLK_ESAI_MEM>,
						 <&clks IMX6SX_CLK_ESAI_EXTAL>,
						 <&clks IMX6SX_CLK_ESAI_IPG>,
						 <&clks IMX6SX_CLK_SPBA>;
					clock-names = "core", "mem", "extal",
						      "fsys", "dma";
					status = "disabled";
				};

				ssi1: ssi@02028000 {
					#sound-dai-cells = <0>;
					compatible = "fsl,imx6sx-ssi", "fsl,imx51-ssi";
					reg = <0x02028000 0x4000>;
					interrupts = <GIC_SPI 46 IRQ_TYPE_LEVEL_HIGH>;
					clocks = <&clks IMX6SX_CLK_SSI1_IPG>,
						 <&clks IMX6SX_CLK_SSI1>;
					clock-names = "ipg", "baud";
					dmas = <&sdma 37 1 0>, <&sdma 38 1 0>;
					dma-names = "rx", "tx";
					fsl,fifo-depth = <15>;
					status = "disabled";
				};

				ssi2: ssi@0202c000 {
					#sound-dai-cells = <0>;
					compatible = "fsl,imx6sx-ssi", "fsl,imx51-ssi";
					reg = <0x0202c000 0x4000>;
					interrupts = <GIC_SPI 47 IRQ_TYPE_LEVEL_HIGH>;
					clocks = <&clks IMX6SX_CLK_SSI2_IPG>,
						 <&clks IMX6SX_CLK_SSI2>;
					clock-names = "ipg", "baud";
					dmas = <&sdma 41 1 0>, <&sdma 42 1 0>;
					dma-names = "rx", "tx";
					fsl,fifo-depth = <15>;
					status = "disabled";
				};

				ssi3: ssi@02030000 {
					#sound-dai-cells = <0>;
					compatible = "fsl,imx6sx-ssi", "fsl,imx51-ssi";
					reg = <0x02030000 0x4000>;
					interrupts = <GIC_SPI 48 IRQ_TYPE_LEVEL_HIGH>;
					clocks = <&clks IMX6SX_CLK_SSI3_IPG>,
						 <&clks IMX6SX_CLK_SSI3>;
					clock-names = "ipg", "baud";
					dmas = <&sdma 45 1 0>, <&sdma 46 1 0>;
					dma-names = "rx", "tx";
					fsl,fifo-depth = <15>;
					status = "disabled";
				};

				asrc: asrc@02034000 {
					reg = <0x02034000 0x4000>;
					interrupts = <GIC_SPI 50 IRQ_TYPE_LEVEL_HIGH>;
					clocks = <&clks IMX6SX_CLK_ASRC_MEM>,
						 <&clks IMX6SX_CLK_ASRC_IPG>,
						 <&clks IMX6SX_CLK_SPDIF>,
						 <&clks IMX6SX_CLK_SPBA>;
					clock-names = "mem", "ipg", "asrck", "dma";
					dmas = <&sdma 17 20 1>, <&sdma 18 20 1>,
					       <&sdma 19 20 1>, <&sdma 20 20 1>,
					       <&sdma 21 20 1>, <&sdma 22 20 1>;
					dma-names = "rxa", "rxb", "rxc",
						    "txa", "txb", "txc";
					status = "okay";
				};
			};

			pwm1: pwm@02080000 {
				compatible = "fsl,imx6sx-pwm", "fsl,imx27-pwm";
				reg = <0x02080000 0x4000>;
				interrupts = <GIC_SPI 83 IRQ_TYPE_LEVEL_HIGH>;
				clocks = <&clks IMX6SX_CLK_PWM1>,
					 <&clks IMX6SX_CLK_PWM1>;
				clock-names = "ipg", "per";
				#pwm-cells = <2>;
			};

			pwm2: pwm@02084000 {
				compatible = "fsl,imx6sx-pwm", "fsl,imx27-pwm";
				reg = <0x02084000 0x4000>;
				interrupts = <GIC_SPI 84 IRQ_TYPE_LEVEL_HIGH>;
				clocks = <&clks IMX6SX_CLK_PWM2>,
					 <&clks IMX6SX_CLK_PWM2>;
				clock-names = "ipg", "per";
				#pwm-cells = <2>;
			};

			pwm3: pwm@02088000 {
				compatible = "fsl,imx6sx-pwm", "fsl,imx27-pwm";
				reg = <0x02088000 0x4000>;
				interrupts = <GIC_SPI 85 IRQ_TYPE_LEVEL_HIGH>;
				clocks = <&clks IMX6SX_CLK_PWM3>,
					 <&clks IMX6SX_CLK_PWM3>;
				clock-names = "ipg", "per";
				#pwm-cells = <2>;
			};

			pwm4: pwm@0208c000 {
				compatible = "fsl,imx6sx-pwm", "fsl,imx27-pwm";
				reg = <0x0208c000 0x4000>;
				interrupts = <GIC_SPI 86 IRQ_TYPE_LEVEL_HIGH>;
				clocks = <&clks IMX6SX_CLK_PWM4>,
					 <&clks IMX6SX_CLK_PWM4>;
				clock-names = "ipg", "per";
				#pwm-cells = <2>;
			};

			flexcan1: can@02090000 {
				compatible = "fsl,imx6sx-flexcan", "fsl,imx6q-flexcan";
				reg = <0x02090000 0x4000>;
				interrupts = <GIC_SPI 110 IRQ_TYPE_LEVEL_HIGH>;
				clocks = <&clks IMX6SX_CLK_CAN1_IPG>,
					 <&clks IMX6SX_CLK_CAN1_SERIAL>;
				clock-names = "ipg", "per";
				status = "disabled";
			};

			flexcan2: can@02094000 {
				compatible = "fsl,imx6sx-flexcan", "fsl,imx6q-flexcan";
				reg = <0x02094000 0x4000>;
				interrupts = <GIC_SPI 111 IRQ_TYPE_LEVEL_HIGH>;
				clocks = <&clks IMX6SX_CLK_CAN2_IPG>,
					 <&clks IMX6SX_CLK_CAN2_SERIAL>;
				clock-names = "ipg", "per";
				status = "disabled";
			};

			gpt: gpt@02098000 {
				compatible = "fsl,imx6sx-gpt", "fsl,imx31-gpt";
				reg = <0x02098000 0x4000>;
				interrupts = <GIC_SPI 55 IRQ_TYPE_LEVEL_HIGH>;
				clocks = <&clks IMX6SX_CLK_GPT_BUS>,
					 <&clks IMX6SX_CLK_GPT_3M>;
				clock-names = "ipg", "per";
			};

			gpio1: gpio@0209c000 {
				compatible = "fsl,imx6sx-gpio", "fsl,imx35-gpio";
				reg = <0x0209c000 0x4000>;
				interrupts = <GIC_SPI 66 IRQ_TYPE_LEVEL_HIGH>,
					     <GIC_SPI 67 IRQ_TYPE_LEVEL_HIGH>;
				gpio-controller;
				#gpio-cells = <2>;
				interrupt-controller;
				#interrupt-cells = <2>;
			};

			gpio2: gpio@020a0000 {
				compatible = "fsl,imx6sx-gpio", "fsl,imx35-gpio";
				reg = <0x020a0000 0x4000>;
				interrupts = <GIC_SPI 68 IRQ_TYPE_LEVEL_HIGH>,
					     <GIC_SPI 69 IRQ_TYPE_LEVEL_HIGH>;
				gpio-controller;
				#gpio-cells = <2>;
				interrupt-controller;
				#interrupt-cells = <2>;
			};

			gpio3: gpio@020a4000 {
				compatible = "fsl,imx6sx-gpio", "fsl,imx35-gpio";
				reg = <0x020a4000 0x4000>;
				interrupts = <GIC_SPI 70 IRQ_TYPE_LEVEL_HIGH>,
					     <GIC_SPI 71 IRQ_TYPE_LEVEL_HIGH>;
				gpio-controller;
				#gpio-cells = <2>;
				interrupt-controller;
				#interrupt-cells = <2>;
			};

			gpio4: gpio@020a8000 {
				compatible = "fsl,imx6sx-gpio", "fsl,imx35-gpio";
				reg = <0x020a8000 0x4000>;
				interrupts = <GIC_SPI 72 IRQ_TYPE_LEVEL_HIGH>,
					     <GIC_SPI 73 IRQ_TYPE_LEVEL_HIGH>;
				gpio-controller;
				#gpio-cells = <2>;
				interrupt-controller;
				#interrupt-cells = <2>;
			};

			gpio5: gpio@020ac000 {
				compatible = "fsl,imx6sx-gpio", "fsl,imx35-gpio";
				reg = <0x020ac000 0x4000>;
				interrupts = <GIC_SPI 74 IRQ_TYPE_LEVEL_HIGH>,
					     <GIC_SPI 75 IRQ_TYPE_LEVEL_HIGH>;
				gpio-controller;
				#gpio-cells = <2>;
				interrupt-controller;
				#interrupt-cells = <2>;
			};

			gpio6: gpio@020b0000 {
				compatible = "fsl,imx6sx-gpio", "fsl,imx35-gpio";
				reg = <0x020b0000 0x4000>;
				interrupts = <GIC_SPI 76 IRQ_TYPE_LEVEL_HIGH>,
					     <GIC_SPI 77 IRQ_TYPE_LEVEL_HIGH>;
				gpio-controller;
				#gpio-cells = <2>;
				interrupt-controller;
				#interrupt-cells = <2>;
			};

			gpio7: gpio@020b4000 {
				compatible = "fsl,imx6sx-gpio", "fsl,imx35-gpio";
				reg = <0x020b4000 0x4000>;
				interrupts = <GIC_SPI 78 IRQ_TYPE_LEVEL_HIGH>,
					     <GIC_SPI 79 IRQ_TYPE_LEVEL_HIGH>;
				gpio-controller;
				#gpio-cells = <2>;
				interrupt-controller;
				#interrupt-cells = <2>;
			};

			kpp: kpp@020b8000 {
				compatible = "fsl,imx6sx-kpp", "fsl,imx21-kpp";
				reg = <0x020b8000 0x4000>;
				interrupts = <GIC_SPI 82 IRQ_TYPE_LEVEL_HIGH>;
				clocks = <&clks IMX6SX_CLK_DUMMY>;
				status = "disabled";
			};

			wdog1: wdog@020bc000 {
				compatible = "fsl,imx6sx-wdt", "fsl,imx21-wdt";
				reg = <0x020bc000 0x4000>;
				interrupts = <GIC_SPI 80 IRQ_TYPE_LEVEL_HIGH>;
				clocks = <&clks IMX6SX_CLK_DUMMY>;
			};

			wdog2: wdog@020c0000 {
				compatible = "fsl,imx6sx-wdt", "fsl,imx21-wdt";
				reg = <0x020c0000 0x4000>;
				interrupts = <GIC_SPI 81 IRQ_TYPE_LEVEL_HIGH>;
				clocks = <&clks IMX6SX_CLK_DUMMY>;
				status = "disabled";
			};

			clks: ccm@020c4000 {
				compatible = "fsl,imx6sx-ccm";
				reg = <0x020c4000 0x4000>;
				interrupts = <GIC_SPI 87 IRQ_TYPE_LEVEL_HIGH>,
					     <GIC_SPI 88 IRQ_TYPE_LEVEL_HIGH>;
				#clock-cells = <1>;
				clocks = <&ckil>, <&osc>, <&ipp_di0>, <&ipp_di1>;
				clock-names = "ckil", "osc", "ipp_di0", "ipp_di1";
			};

			anatop: anatop@020c8000 {
				compatible = "fsl,imx6sx-anatop", "fsl,imx6q-anatop",
					     "syscon", "simple-bus";
				reg = <0x020c8000 0x1000>;
				interrupts = <GIC_SPI 49 IRQ_TYPE_LEVEL_HIGH>,
					     <GIC_SPI 54 IRQ_TYPE_LEVEL_HIGH>,
					     <GIC_SPI 127 IRQ_TYPE_LEVEL_HIGH>;

				regulator-1p1@110 {
					compatible = "fsl,anatop-regulator";
					regulator-name = "vdd1p1";
					regulator-min-microvolt = <800000>;
					regulator-max-microvolt = <1375000>;
					regulator-always-on;
					anatop-reg-offset = <0x110>;
					anatop-vol-bit-shift = <8>;
					anatop-vol-bit-width = <5>;
					anatop-min-bit-val = <4>;
					anatop-min-voltage = <800000>;
					anatop-max-voltage = <1375000>;
				};

				regulator-3p0@120 {
					compatible = "fsl,anatop-regulator";
					regulator-name = "vdd3p0";
					regulator-min-microvolt = <2800000>;
					regulator-max-microvolt = <3150000>;
					regulator-always-on;
					anatop-reg-offset = <0x120>;
					anatop-vol-bit-shift = <8>;
					anatop-vol-bit-width = <5>;
					anatop-min-bit-val = <0>;
					anatop-min-voltage = <2625000>;
					anatop-max-voltage = <3400000>;
				};

				regulator-2p5@130 {
					compatible = "fsl,anatop-regulator";
					regulator-name = "vdd2p5";
					regulator-min-microvolt = <2100000>;
					regulator-max-microvolt = <2875000>;
					regulator-always-on;
					anatop-reg-offset = <0x130>;
					anatop-vol-bit-shift = <8>;
					anatop-vol-bit-width = <5>;
					anatop-min-bit-val = <0>;
					anatop-min-voltage = <2100000>;
					anatop-max-voltage = <2875000>;
				};

				reg_arm: regulator-vddcore@140 {
					compatible = "fsl,anatop-regulator";
					regulator-name = "vddarm";
					regulator-min-microvolt = <725000>;
					regulator-max-microvolt = <1450000>;
					regulator-always-on;
					anatop-reg-offset = <0x140>;
					anatop-vol-bit-shift = <0>;
					anatop-vol-bit-width = <5>;
					anatop-delay-reg-offset = <0x170>;
					anatop-delay-bit-shift = <24>;
					anatop-delay-bit-width = <2>;
					anatop-min-bit-val = <1>;
					anatop-min-voltage = <725000>;
					anatop-max-voltage = <1450000>;
				};

				reg_pcie: regulator-vddpcie@140 {
					compatible = "fsl,anatop-regulator";
					regulator-name = "vddpcie";
					regulator-min-microvolt = <725000>;
					regulator-max-microvolt = <1450000>;
					anatop-reg-offset = <0x140>;
					anatop-vol-bit-shift = <9>;
					anatop-vol-bit-width = <5>;
					anatop-delay-reg-offset = <0x170>;
					anatop-delay-bit-shift = <26>;
					anatop-delay-bit-width = <2>;
					anatop-min-bit-val = <1>;
					anatop-min-voltage = <725000>;
					anatop-max-voltage = <1450000>;
				};

				reg_soc: regulator-vddsoc@140 {
					compatible = "fsl,anatop-regulator";
					regulator-name = "vddsoc";
					regulator-min-microvolt = <725000>;
					regulator-max-microvolt = <1450000>;
					regulator-always-on;
					anatop-reg-offset = <0x140>;
					anatop-vol-bit-shift = <18>;
					anatop-vol-bit-width = <5>;
					anatop-delay-reg-offset = <0x170>;
					anatop-delay-bit-shift = <28>;
					anatop-delay-bit-width = <2>;
					anatop-min-bit-val = <1>;
					anatop-min-voltage = <725000>;
					anatop-max-voltage = <1450000>;
				};
			};

			tempmon: tempmon {
				compatible = "fsl,imx6sx-tempmon", "fsl,imx6q-tempmon";
				interrupts = <GIC_SPI 49 IRQ_TYPE_LEVEL_HIGH>;
				fsl,tempmon = <&anatop>;
				fsl,tempmon-data = <&ocotp>;
				clocks = <&clks IMX6SX_CLK_PLL3_USB_OTG>;
			};

			usbphy1: usbphy@020c9000 {
				compatible = "fsl,imx6sx-usbphy", "fsl,imx23-usbphy";
				reg = <0x020c9000 0x1000>;
				interrupts = <GIC_SPI 44 IRQ_TYPE_LEVEL_HIGH>;
				clocks = <&clks IMX6SX_CLK_USBPHY1>;
				fsl,anatop = <&anatop>;
			};

			usbphy2: usbphy@020ca000 {
				compatible = "fsl,imx6sx-usbphy", "fsl,imx23-usbphy";
				reg = <0x020ca000 0x1000>;
				interrupts = <GIC_SPI 45 IRQ_TYPE_LEVEL_HIGH>;
				clocks = <&clks IMX6SX_CLK_USBPHY2>;
				fsl,anatop = <&anatop>;
			};

			snvs: snvs@020cc000 {
				compatible = "fsl,sec-v4.0-mon", "simple-bus";
				#address-cells = <1>;
				#size-cells = <1>;
				ranges = <0 0x020cc000 0x4000>;

				snvs_rtc: snvs-rtc-lp@34 {
					compatible = "fsl,sec-v4.0-mon-rtc-lp";
					reg = <0x34 0x58>;
					interrupts = <GIC_SPI 19 IRQ_TYPE_LEVEL_HIGH>, <GIC_SPI 20 IRQ_TYPE_LEVEL_HIGH>;
				};

				snvs_poweroff: snvs-poweroff@38 {
					compatible = "fsl,sec-v4.0-poweroff";
					reg = <0x38 0x4>;
					status = "disabled";
				};
			};

			epit1: epit@020d0000 {
				reg = <0x020d0000 0x4000>;
				interrupts = <GIC_SPI 56 IRQ_TYPE_LEVEL_HIGH>;
			};

			epit2: epit@020d4000 {
				reg = <0x020d4000 0x4000>;
				interrupts = <GIC_SPI 57 IRQ_TYPE_LEVEL_HIGH>;
			};

			src: src@020d8000 {
				compatible = "fsl,imx6sx-src", "fsl,imx51-src";
				reg = <0x020d8000 0x4000>;
				interrupts = <GIC_SPI 91 IRQ_TYPE_LEVEL_HIGH>,
					     <GIC_SPI 96 IRQ_TYPE_LEVEL_HIGH>;
				#reset-cells = <1>;
			};

			gpc: gpc@020dc000 {
				compatible = "fsl,imx6sx-gpc", "fsl,imx6q-gpc";
				reg = <0x020dc000 0x4000>;
				interrupt-controller;
				#interrupt-cells = <3>;
				interrupts = <GIC_SPI 89 IRQ_TYPE_LEVEL_HIGH>;
				interrupt-parent = <&intc>;
			};

			iomuxc: iomuxc@020e0000 {
				compatible = "fsl,imx6sx-iomuxc";
				reg = <0x020e0000 0x4000>;
			};

			gpr: iomuxc-gpr@020e4000 {
				compatible = "fsl,imx6sx-iomuxc-gpr",
					     "fsl,imx6q-iomuxc-gpr", "syscon";
				reg = <0x020e4000 0x4000>;
			};

			sdma: sdma@020ec000 {
				compatible = "fsl,imx6sx-sdma", "fsl,imx6q-sdma";
				reg = <0x020ec000 0x4000>;
				interrupts = <GIC_SPI 2 IRQ_TYPE_LEVEL_HIGH>;
				clocks = <&clks IMX6SX_CLK_SDMA>,
					 <&clks IMX6SX_CLK_SDMA>;
				clock-names = "ipg", "ahb";
				#dma-cells = <3>;
				/* imx6sx reuses imx6q sdma firmware */
				fsl,sdma-ram-script-name = "imx/sdma/sdma-imx6q.bin";
			};
		};

		aips2: aips-bus@02100000 {
			compatible = "fsl,aips-bus", "simple-bus";
			#address-cells = <1>;
			#size-cells = <1>;
			reg = <0x02100000 0x100000>;
			ranges;

			usbotg1: usb@02184000 {
				compatible = "fsl,imx6sx-usb", "fsl,imx27-usb";
				reg = <0x02184000 0x200>;
				interrupts = <GIC_SPI 43 IRQ_TYPE_LEVEL_HIGH>;
				clocks = <&clks IMX6SX_CLK_USBOH3>;
				fsl,usbphy = <&usbphy1>;
				fsl,usbmisc = <&usbmisc 0>;
				fsl,anatop = <&anatop>;
				status = "disabled";
			};

			usbotg2: usb@02184200 {
				compatible = "fsl,imx6sx-usb", "fsl,imx27-usb";
				reg = <0x02184200 0x200>;
				interrupts = <GIC_SPI 42 IRQ_TYPE_LEVEL_HIGH>;
				clocks = <&clks IMX6SX_CLK_USBOH3>;
				fsl,usbphy = <&usbphy2>;
				fsl,usbmisc = <&usbmisc 1>;
				status = "disabled";
			};

			usbh: usb@02184400 {
				compatible = "fsl,imx6sx-usb", "fsl,imx27-usb";
				reg = <0x02184400 0x200>;
				interrupts = <GIC_SPI 40 IRQ_TYPE_LEVEL_HIGH>;
				clocks = <&clks IMX6SX_CLK_USBOH3>;
				fsl,usbmisc = <&usbmisc 2>;
				phy_type = "hsic";
				fsl,anatop = <&anatop>;
				dr_mode = "host";
				status = "disabled";
			};

			usbmisc: usbmisc@02184800 {
				#index-cells = <1>;
				compatible = "fsl,imx6sx-usbmisc", "fsl,imx6q-usbmisc";
				reg = <0x02184800 0x200>;
				clocks = <&clks IMX6SX_CLK_USBOH3>;
			};

			fec1: ethernet@02188000 {
				compatible = "fsl,imx6sx-fec", "fsl,imx6q-fec";
				reg = <0x02188000 0x4000>;
				interrupts = <GIC_SPI 118 IRQ_TYPE_LEVEL_HIGH>,
					     <GIC_SPI 119 IRQ_TYPE_LEVEL_HIGH>;
				clocks = <&clks IMX6SX_CLK_ENET>,
					 <&clks IMX6SX_CLK_ENET_AHB>,
					 <&clks IMX6SX_CLK_ENET_PTP>,
					 <&clks IMX6SX_CLK_ENET_REF>,
					 <&clks IMX6SX_CLK_ENET_PTP>;
				clock-names = "ipg", "ahb", "ptp",
					      "enet_clk_ref", "enet_out";
				fsl,num-tx-queues=<3>;
				fsl,num-rx-queues=<3>;
				status = "disabled";
                        };

			mlb: mlb@0218c000 {
				reg = <0x0218c000 0x4000>;
				interrupts = <GIC_SPI 53 IRQ_TYPE_LEVEL_HIGH>,
					     <GIC_SPI 117 IRQ_TYPE_LEVEL_HIGH>,
					     <GIC_SPI 126 IRQ_TYPE_LEVEL_HIGH>;
				clocks = <&clks IMX6SX_CLK_MLB>;
				status = "disabled";
			};

			usdhc1: usdhc@02190000 {
				compatible = "fsl,imx6sx-usdhc", "fsl,imx6sl-usdhc";
				reg = <0x02190000 0x4000>;
				interrupts = <GIC_SPI 22 IRQ_TYPE_LEVEL_HIGH>;
				clocks = <&clks IMX6SX_CLK_USDHC1>,
					 <&clks IMX6SX_CLK_USDHC1>,
					 <&clks IMX6SX_CLK_USDHC1>;
				clock-names = "ipg", "ahb", "per";
				bus-width = <4>;
				status = "disabled";
			};

			usdhc2: usdhc@02194000 {
				compatible = "fsl,imx6sx-usdhc", "fsl,imx6sl-usdhc";
				reg = <0x02194000 0x4000>;
				interrupts = <GIC_SPI 23 IRQ_TYPE_LEVEL_HIGH>;
				clocks = <&clks IMX6SX_CLK_USDHC2>,
					 <&clks IMX6SX_CLK_USDHC2>,
					 <&clks IMX6SX_CLK_USDHC2>;
				clock-names = "ipg", "ahb", "per";
				bus-width = <4>;
				status = "disabled";
			};

			usdhc3: usdhc@02198000 {
				compatible = "fsl,imx6sx-usdhc", "fsl,imx6sl-usdhc";
				reg = <0x02198000 0x4000>;
				interrupts = <GIC_SPI 24 IRQ_TYPE_LEVEL_HIGH>;
				clocks = <&clks IMX6SX_CLK_USDHC3>,
					 <&clks IMX6SX_CLK_USDHC3>,
					 <&clks IMX6SX_CLK_USDHC3>;
				clock-names = "ipg", "ahb", "per";
				bus-width = <4>;
				status = "disabled";
			};

			usdhc4: usdhc@0219c000 {
				compatible = "fsl,imx6sx-usdhc", "fsl,imx6sl-usdhc";
				reg = <0x0219c000 0x4000>;
				interrupts = <GIC_SPI 25 IRQ_TYPE_LEVEL_HIGH>;
				clocks = <&clks IMX6SX_CLK_USDHC4>,
					 <&clks IMX6SX_CLK_USDHC4>,
					 <&clks IMX6SX_CLK_USDHC4>;
				clock-names = "ipg", "ahb", "per";
				bus-width = <4>;
				status = "disabled";
			};

			i2c1: i2c@021a0000 {
				#address-cells = <1>;
				#size-cells = <0>;
				compatible = "fsl,imx6sx-i2c", "fsl,imx21-i2c";
				reg = <0x021a0000 0x4000>;
				interrupts = <GIC_SPI 36 IRQ_TYPE_LEVEL_HIGH>;
				clocks = <&clks IMX6SX_CLK_I2C1>;
				status = "disabled";
			};

			i2c2: i2c@021a4000 {
				#address-cells = <1>;
				#size-cells = <0>;
				compatible = "fsl,imx6sx-i2c", "fsl,imx21-i2c";
				reg = <0x021a4000 0x4000>;
				interrupts = <GIC_SPI 37 IRQ_TYPE_LEVEL_HIGH>;
				clocks = <&clks IMX6SX_CLK_I2C2>;
				status = "disabled";
			};

			i2c3: i2c@021a8000 {
				#address-cells = <1>;
				#size-cells = <0>;
				compatible = "fsl,imx6sx-i2c", "fsl,imx21-i2c";
				reg = <0x021a8000 0x4000>;
				interrupts = <GIC_SPI 38 IRQ_TYPE_LEVEL_HIGH>;
				clocks = <&clks IMX6SX_CLK_I2C3>;
				status = "disabled";
			};

			mmdc: mmdc@021b0000 {
				compatible = "fsl,imx6sx-mmdc", "fsl,imx6q-mmdc";
				reg = <0x021b0000 0x4000>;
			};

			fec2: ethernet@021b4000 {
				compatible = "fsl,imx6sx-fec", "fsl,imx6q-fec";
				reg = <0x021b4000 0x4000>;
				interrupts = <GIC_SPI 102 IRQ_TYPE_LEVEL_HIGH>,
					     <GIC_SPI 103 IRQ_TYPE_LEVEL_HIGH>;
				clocks = <&clks IMX6SX_CLK_ENET>,
					 <&clks IMX6SX_CLK_ENET_AHB>,
					 <&clks IMX6SX_CLK_ENET_PTP>,
					 <&clks IMX6SX_CLK_ENET2_REF_125M>,
					 <&clks IMX6SX_CLK_ENET_PTP>;
				clock-names = "ipg", "ahb", "ptp",
					      "enet_clk_ref", "enet_out";
				status = "disabled";
			};

			weim: weim@021b8000 {
				compatible = "fsl,imx6sx-weim", "fsl,imx6q-weim";
				reg = <0x021b8000 0x4000>;
				interrupts = <GIC_SPI 14 IRQ_TYPE_LEVEL_HIGH>;
				clocks = <&clks IMX6SX_CLK_EIM_SLOW>;
			};

			ocotp: ocotp@021bc000 {
				compatible = "fsl,imx6sx-ocotp", "syscon";
				reg = <0x021bc000 0x4000>;
				clocks = <&clks IMX6SX_CLK_OCOTP>;
			};

			sai1: sai@021d4000 {
				compatible = "fsl,imx6sx-sai";
				reg = <0x021d4000 0x4000>;
				interrupts = <GIC_SPI 97 IRQ_TYPE_LEVEL_HIGH>;
				clocks = <&clks IMX6SX_CLK_SAI1_IPG>,
					 <&clks IMX6SX_CLK_SAI1>,
					 <&clks 0>, <&clks 0>;
				clock-names = "bus", "mclk1", "mclk2", "mclk3";
				dma-names = "rx", "tx";
				dmas = <&sdma 31 23 0>, <&sdma 32 23 0>;
				dma-source = <&gpr 0 15 0 16>;
				status = "disabled";
			};

			audmux: audmux@021d8000 {
				compatible = "fsl,imx6sx-audmux", "fsl,imx31-audmux";
				reg = <0x021d8000 0x4000>;
				status = "disabled";
			};

			sai2: sai@021dc000 {
				compatible = "fsl,imx6sx-sai";
				reg = <0x021dc000 0x4000>;
				interrupts = <GIC_SPI 98 IRQ_TYPE_LEVEL_HIGH>;
				clocks = <&clks IMX6SX_CLK_SAI2_IPG>,
					 <&clks IMX6SX_CLK_SAI2>,
					 <&clks 0>, <&clks 0>;
				clock-names = "bus", "mclk1", "mclk2", "mclk3";
				dma-names = "rx", "tx";
				dmas = <&sdma 33 23 0>, <&sdma 34 23 0>;
				dma-source = <&gpr 0 17 0 18>;
				status = "disabled";
			};

			qspi1: qspi@021e0000 {
				#address-cells = <1>;
				#size-cells = <0>;
				compatible = "fsl,imx6sx-qspi";
				reg = <0x021e0000 0x4000>, <0x60000000 0x10000000>;
				reg-names = "QuadSPI", "QuadSPI-memory";
				interrupts = <GIC_SPI 107 IRQ_TYPE_LEVEL_HIGH>;
				clocks = <&clks IMX6SX_CLK_QSPI1>,
					 <&clks IMX6SX_CLK_QSPI1>;
				clock-names = "qspi_en", "qspi";
				status = "disabled";
			};

			qspi2: qspi@021e4000 {
				#address-cells = <1>;
				#size-cells = <0>;
				compatible = "fsl,imx6sx-qspi";
				reg = <0x021e4000 0x4000>, <0x70000000 0x10000000>;
				reg-names = "QuadSPI", "QuadSPI-memory";
				interrupts = <GIC_SPI 109 IRQ_TYPE_LEVEL_HIGH>;
				clocks = <&clks IMX6SX_CLK_QSPI2>,
					 <&clks IMX6SX_CLK_QSPI2>;
				clock-names = "qspi_en", "qspi";
				status = "disabled";
			};

			uart2: serial@021e8000 {
				compatible = "fsl,imx6sx-uart", "fsl,imx21-uart";
				reg = <0x021e8000 0x4000>;
				interrupts = <GIC_SPI 27 IRQ_TYPE_LEVEL_HIGH>;
				clocks = <&clks IMX6SX_CLK_UART_IPG>,
					 <&clks IMX6SX_CLK_UART_SERIAL>;
				clock-names = "ipg", "per";
				dmas = <&sdma 27 4 0>, <&sdma 28 4 0>;
				dma-names = "rx", "tx";
				status = "disabled";
			};

			uart3: serial@021ec000 {
				compatible = "fsl,imx6sx-uart", "fsl,imx21-uart";
				reg = <0x021ec000 0x4000>;
				interrupts = <GIC_SPI 28 IRQ_TYPE_LEVEL_HIGH>;
				clocks = <&clks IMX6SX_CLK_UART_IPG>,
					 <&clks IMX6SX_CLK_UART_SERIAL>;
				clock-names = "ipg", "per";
				dmas = <&sdma 29 4 0>, <&sdma 30 4 0>;
				dma-names = "rx", "tx";
				status = "disabled";
			};

			uart4: serial@021f0000 {
				compatible = "fsl,imx6sx-uart", "fsl,imx21-uart";
				reg = <0x021f0000 0x4000>;
				interrupts = <GIC_SPI 29 IRQ_TYPE_LEVEL_HIGH>;
				clocks = <&clks IMX6SX_CLK_UART_IPG>,
					 <&clks IMX6SX_CLK_UART_SERIAL>;
				clock-names = "ipg", "per";
				dmas = <&sdma 31 4 0>, <&sdma 32 4 0>;
				dma-names = "rx", "tx";
				status = "disabled";
			};

			uart5: serial@021f4000 {
				compatible = "fsl,imx6sx-uart", "fsl,imx21-uart";
				reg = <0x021f4000 0x4000>;
				interrupts = <GIC_SPI 30 IRQ_TYPE_LEVEL_HIGH>;
				clocks = <&clks IMX6SX_CLK_UART_IPG>,
					 <&clks IMX6SX_CLK_UART_SERIAL>;
				clock-names = "ipg", "per";
				dmas = <&sdma 33 4 0>, <&sdma 34 4 0>;
				dma-names = "rx", "tx";
				status = "disabled";
			};

			i2c4: i2c@021f8000 {
				#address-cells = <1>;
				#size-cells = <0>;
				compatible = "fsl,imx6sx-i2c", "fsl,imx21-i2c";
				reg = <0x021f8000 0x4000>;
				interrupts = <GIC_SPI 35 IRQ_TYPE_LEVEL_HIGH>;
				clocks = <&clks IMX6SX_CLK_I2C4>;
				status = "disabled";
			};
		};

		aips3: aips-bus@02200000 {
			compatible = "fsl,aips-bus", "simple-bus";
			#address-cells = <1>;
			#size-cells = <1>;
			reg = <0x02200000 0x100000>;
			ranges;

			spba-bus@02200000 {
				compatible = "fsl,spba-bus", "simple-bus";
				#address-cells = <1>;
				#size-cells = <1>;
				reg = <0x02240000 0x40000>;
				ranges;

				csi1: csi@02214000 {
					reg = <0x02214000 0x4000>;
					interrupts = <GIC_SPI 7 IRQ_TYPE_LEVEL_HIGH>;
					clocks = <&clks IMX6SX_CLK_DISPLAY_AXI>,
						 <&clks IMX6SX_CLK_CSI>,
						 <&clks IMX6SX_CLK_DCIC1>;
					clock-names = "disp-axi", "csi_mclk", "dcic";
					status = "disabled";
				};

				pxp: pxp@02218000 {
					reg = <0x02218000 0x4000>;
					interrupts = <GIC_SPI 8 IRQ_TYPE_LEVEL_HIGH>;
					clocks = <&clks IMX6SX_CLK_PXP_AXI>,
						 <&clks IMX6SX_CLK_DISPLAY_AXI>;
					clock-names = "pxp-axi", "disp-axi";
					status = "disabled";
				};

				csi2: csi@0221c000 {
					reg = <0x0221c000 0x4000>;
					interrupts = <GIC_SPI 41 IRQ_TYPE_LEVEL_HIGH>;
					clocks = <&clks IMX6SX_CLK_DISPLAY_AXI>,
						 <&clks IMX6SX_CLK_CSI>,
						 <&clks IMX6SX_CLK_DCIC2>;
					clock-names = "disp-axi", "csi_mclk", "dcic";
					status = "disabled";
				};

				lcdif1: lcdif@02220000 {
					compatible = "fsl,imx6sx-lcdif", "fsl,imx28-lcdif";
					reg = <0x02220000 0x4000>;
					interrupts = <GIC_SPI 5 IRQ_TYPE_LEVEL_HIGH>;
					clocks = <&clks IMX6SX_CLK_LCDIF1_PIX>,
						 <&clks IMX6SX_CLK_LCDIF_APB>,
						 <&clks IMX6SX_CLK_DISPLAY_AXI>;
					clock-names = "pix", "axi", "disp_axi";
					status = "disabled";
				};

				lcdif2: lcdif@02224000 {
					compatible = "fsl,imx6sx-lcdif", "fsl,imx28-lcdif";
					reg = <0x02224000 0x4000>;
					interrupts = <GIC_SPI 6 IRQ_TYPE_LEVEL_HIGH>;
					clocks = <&clks IMX6SX_CLK_LCDIF2_PIX>,
						 <&clks IMX6SX_CLK_LCDIF_APB>,
						 <&clks IMX6SX_CLK_DISPLAY_AXI>;
					clock-names = "pix", "axi", "disp_axi";
					status = "disabled";
				};

				vadc: vadc@02228000 {
					reg = <0x02228000 0x4000>, <0x0222c000 0x4000>;
					reg-names = "vadc-vafe", "vadc-vdec";
					clocks = <&clks IMX6SX_CLK_VADC>,
						 <&clks IMX6SX_CLK_CSI>;
					clock-names = "vadc", "csi";
					status = "disabled";
				};
			};

			adc1: adc@02280000 {
				compatible = "fsl,imx6sx-adc", "fsl,vf610-adc";
				reg = <0x02280000 0x4000>;
				interrupts = <GIC_SPI 100 IRQ_TYPE_LEVEL_HIGH>;
				clocks = <&clks IMX6SX_CLK_IPG>;
				clock-names = "adc";
				status = "disabled";
                        };

			adc2: adc@02284000 {
				compatible = "fsl,imx6sx-adc", "fsl,vf610-adc";
				reg = <0x02284000 0x4000>;
				interrupts = <GIC_SPI 101 IRQ_TYPE_LEVEL_HIGH>;
				clocks = <&clks IMX6SX_CLK_IPG>;
				clock-names = "adc";
				status = "disabled";
                        };

			wdog3: wdog@02288000 {
				compatible = "fsl,imx6sx-wdt", "fsl,imx21-wdt";
				reg = <0x02288000 0x4000>;
				interrupts = <GIC_SPI 11 IRQ_TYPE_LEVEL_HIGH>;
				clocks = <&clks IMX6SX_CLK_DUMMY>;
				status = "disabled";
			};

			ecspi5: ecspi@0228c000 {
				#address-cells = <1>;
				#size-cells = <0>;
				compatible = "fsl,imx6sx-ecspi", "fsl,imx51-ecspi";
				reg = <0x0228c000 0x4000>;
				interrupts = <GIC_SPI 18 IRQ_TYPE_LEVEL_HIGH>;
				clocks = <&clks IMX6SX_CLK_ECSPI5>,
					 <&clks IMX6SX_CLK_ECSPI5>;
				clock-names = "ipg", "per";
				status = "disabled";
			};

			uart6: serial@022a0000 {
				compatible = "fsl,imx6sx-uart", "fsl,imx21-uart";
				reg = <0x022a0000 0x4000>;
				interrupts = <GIC_SPI 17 IRQ_TYPE_LEVEL_HIGH>;
				clocks = <&clks IMX6SX_CLK_UART_IPG>,
					 <&clks IMX6SX_CLK_UART_SERIAL>;
				clock-names = "ipg", "per";
				dmas = <&sdma 0 4 0>, <&sdma 47 4 0>;
				dma-names = "rx", "tx";
				status = "disabled";
			};

			pwm5: pwm@022a4000 {
				compatible = "fsl,imx6sx-pwm", "fsl,imx27-pwm";
				reg = <0x022a4000 0x4000>;
				interrupts = <GIC_SPI 83 IRQ_TYPE_LEVEL_HIGH>;
				clocks = <&clks IMX6SX_CLK_PWM5>,
					 <&clks IMX6SX_CLK_PWM5>;
				clock-names = "ipg", "per";
				#pwm-cells = <2>;
			};

			pwm6: pwm@022a8000 {
				compatible = "fsl,imx6sx-pwm", "fsl,imx27-pwm";
				reg = <0x022a8000 0x4000>;
				interrupts = <GIC_SPI 84 IRQ_TYPE_LEVEL_HIGH>;
				clocks = <&clks IMX6SX_CLK_PWM6>,
					 <&clks IMX6SX_CLK_PWM6>;
				clock-names = "ipg", "per";
				#pwm-cells = <2>;
			};

			pwm7: pwm@022ac000 {
				compatible = "fsl,imx6sx-pwm", "fsl,imx27-pwm";
				reg = <0x022ac000 0x4000>;
				interrupts = <GIC_SPI 85 IRQ_TYPE_LEVEL_HIGH>;
				clocks = <&clks IMX6SX_CLK_PWM7>,
					 <&clks IMX6SX_CLK_PWM7>;
				clock-names = "ipg", "per";
				#pwm-cells = <2>;
			};

			pwm8: pwm@0022b0000 {
				compatible = "fsl,imx6sx-pwm", "fsl,imx27-pwm";
				reg = <0x0022b0000 0x4000>;
				interrupts = <GIC_SPI 86 IRQ_TYPE_LEVEL_HIGH>;
				clocks = <&clks IMX6SX_CLK_PWM8>,
					 <&clks IMX6SX_CLK_PWM8>;
				clock-names = "ipg", "per";
				#pwm-cells = <2>;
			};
		};

		pcie: pcie@0x08000000 {
			compatible = "fsl,imx6sx-pcie", "snps,dw-pcie";
			reg = <0x08ffc000 0x4000>; /* DBI */
			#address-cells = <3>;
			#size-cells = <2>;
			device_type = "pci";
				  /* configuration space */
			ranges = <0x00000800 0 0x08f00000 0x08f00000 0 0x00080000
				  /* downstream I/O */
				  0x81000000 0 0          0x08f80000 0 0x00010000
				  /* non-prefetchable memory */
				  0x82000000 0 0x08000000 0x08000000 0 0x00f00000>;
			num-lanes = <1>;
			interrupts = <GIC_SPI 123 IRQ_TYPE_LEVEL_HIGH>;
			clocks = <&clks IMX6SX_CLK_PCIE_REF_125M>,
				 <&clks IMX6SX_CLK_PCIE_AXI>,
				 <&clks IMX6SX_CLK_LVDS1_OUT>,
				 <&clks IMX6SX_CLK_DISPLAY_AXI>;
			clock-names = "pcie_ref_125m", "pcie_axi",
				      "lvds_gate", "display_axi";
			status = "disabled";
		};
	};
};
