Broadcom BCM2835
================

Raspberry Pi
------------

  1. Prepare a card with a FAT filesystem. Download a tiny NOOBS LITE
     zip archive and unpack it into FAT partition.
     See http://www.raspberrypi.org/help/noobs-setup/ for details.

  2. Compile ``barebox.bin`` image (use ``rpi_defconfig``).
     Copy it to the SD/microSD card and name it ``recovery.img``.

  3. Connect to board's UART (115200 8N1);
     Use PIN6 (GND), PIN8 (UART_TX), PIN10 (UART_RX) pins.

  4. Turn board's power on.
