/*
 * Device Tree Include file for Marvell Armada 385 SoC.
 *
 * Copyright (C) 2014 Marvell
 *
 * Lior Amsalem <alior@marvell.com>
 * Gregory CLEMENT <gregory.clement@free-electrons.com>
 * Thomas Petazzoni <thomas.petazzoni@free-electrons.com>
 *
 * This file is dual-licensed: you can use it either under the terms
 * of the GPL or the X11 license, at your option. Note that this dual
 * licensing only applies to this file, and not this project as a
 * whole.
 *
 *  a) This file is free software; you can redistribute it and/or
 *     modify it under the terms of the GNU General Public License as
 *     published by the Free Software Foundation; either version 2 of the
 *     License, or (at your option) any later version.
 *
 *     This file is distributed in the hope that it will be useful
 *     but WITHOUT ANY WARRANTY; without even the implied warranty of
 *     MERCHANTABILITY or FITNESS FOR A PARTICULAR PURPOSE.  See the
 *     GNU General Public License for more details.
 *
 * Or, alternatively
 *
 *  b) Permission is hereby granted, free of charge, to any person
 *     obtaining a copy of this software and associated documentation
 *     files (the "Software"), to deal in the Software without
 *     restriction, including without limitation the rights to use
 *     copy, modify, merge, publish, distribute, sublicense, and/or
 *     sell copies of the Software, and to permit persons to whom the
 *     Software is furnished to do so, subject to the following
 *     conditions:
 *
 *     The above copyright notice and this permission notice shall be
 *     included in all copies or substantial portions of the Software.
 *
 *     THE SOFTWARE IS PROVIDED , WITHOUT WARRANTY OF ANY KIND
 *     EXPRESS OR IMPLIED, INCLUDING BUT NOT LIMITED TO THE WARRANTIES
 *     OF MERCHANTABILITY, FITNESS FOR A PARTICULAR PURPOSE AND
 *     NONINFRINGEMENT. IN NO EVENT SHALL THE AUTHORS OR COPYRIGHT
 *     HOLDERS BE LIABLE FOR ANY CLAIM, DAMAGES OR OTHER LIABILITY
 *     WHETHER IN AN ACTION OF CONTRACT, TORT OR OTHERWISE, ARISING
 *     FROM, OUT OF OR IN CONNECTION WITH THE SOFTWARE OR THE USE OR
 *     OTHER DEALINGS IN THE SOFTWARE.
 */

#include "armada-38x.dtsi"

/ {
	model = "Marvell Armada 385 family SoC";
	compatible = "marvell,armada385", "marvell,armada380";

	cpus {
		#address-cells = <1>;
		#size-cells = <0>;
		enable-method = "marvell,armada-380-smp";

		cpu@0 {
			device_type = "cpu";
			compatible = "arm,cortex-a9";
			reg = <0>;
		};
		cpu@1 {
			device_type = "cpu";
			compatible = "arm,cortex-a9";
			reg = <1>;
		};
	};

	soc {
		internal-regs {
			pinctrl@18000 {
				compatible = "marvell,mv88f6820-pinctrl";
			};
		};

		pcie-controller {
			compatible = "marvell,armada-370-pcie";
			status = "disabled";
			device_type = "pci";

			#address-cells = <3>;
			#size-cells = <2>;

			msi-parent = <&mpic>;
			bus-range = <0x00 0xff>;

			ranges =
			       <0x82000000 0 0x80000 MBUS_ID(0xf0, 0x01) 0x80000 0 0x00002000
				0x82000000 0 0x40000 MBUS_ID(0xf0, 0x01) 0x40000 0 0x00002000
				0x82000000 0 0x44000 MBUS_ID(0xf0, 0x01) 0x44000 0 0x00002000
				0x82000000 0 0x48000 MBUS_ID(0xf0, 0x01) 0x48000 0 0x00002000
				0x82000000 0x1 0     MBUS_ID(0x08, 0xe8) 0 1 0 /* Port 0 MEM */
				0x81000000 0x1 0     MBUS_ID(0x08, 0xe0) 0 1 0 /* Port 0 IO  */
				0x82000000 0x2 0     MBUS_ID(0x04, 0xe8) 0 1 0 /* Port 1 MEM */
				0x81000000 0x2 0     MBUS_ID(0x04, 0xe0) 0 1 0 /* Port 1 IO  */
				0x82000000 0x3 0     MBUS_ID(0x04, 0xd8) 0 1 0 /* Port 2 MEM */
				0x81000000 0x3 0     MBUS_ID(0x04, 0xd0) 0 1 0 /* Port 2 IO  */
				0x82000000 0x4 0     MBUS_ID(0x04, 0xb8) 0 1 0 /* Port 3 MEM */
				0x81000000 0x4 0     MBUS_ID(0x04, 0xb0) 0 1 0 /* Port 3 IO  */>;

			/*
			 * This port can be either x4 or x1. When
			 * configured in x4 by the bootloader, then
			 * pcie@4,0 is not available.
			 */
			pcie@1,0 {
				device_type = "pci";
				assigned-addresses = <0x82000800 0 0x80000 0 0x2000>;
				reg = <0x0800 0 0 0 0>;
				#address-cells = <3>;
				#size-cells = <2>;
				#interrupt-cells = <1>;
				ranges = <0x82000000 0 0 0x82000000 0x1 0 1 0
					  0x81000000 0 0 0x81000000 0x1 0 1 0>;
				interrupt-map-mask = <0 0 0 0>;
				interrupt-map = <0 0 0 0 &gic GIC_SPI 29 IRQ_TYPE_LEVEL_HIGH>;
				marvell,pcie-port = <0>;
				marvell,pcie-lane = <0>;
				clocks = <&gateclk 8>;
				status = "disabled";
			};

			/* x1 port */
			pcie@2,0 {
				device_type = "pci";
				assigned-addresses = <0x82000800 0 0x40000 0 0x2000>;
				reg = <0x1000 0 0 0 0>;
				#address-cells = <3>;
				#size-cells = <2>;
				#interrupt-cells = <1>;
				ranges = <0x82000000 0 0 0x82000000 0x2 0 1 0
					  0x81000000 0 0 0x81000000 0x2 0 1 0>;
				interrupt-map-mask = <0 0 0 0>;
				interrupt-map = <0 0 0 0 &gic GIC_SPI 33 IRQ_TYPE_LEVEL_HIGH>;
				marvell,pcie-port = <1>;
				marvell,pcie-lane = <0>;
				clocks = <&gateclk 5>;
				status = "disabled";
			};

			/* x1 port */
			pcie@3,0 {
				device_type = "pci";
				assigned-addresses = <0x82000800 0 0x44000 0 0x2000>;
				reg = <0x1800 0 0 0 0>;
				#address-cells = <3>;
				#size-cells = <2>;
				#interrupt-cells = <1>;
				ranges = <0x82000000 0 0 0x82000000 0x3 0 1 0
					  0x81000000 0 0 0x81000000 0x3 0 1 0>;
				interrupt-map-mask = <0 0 0 0>;
				interrupt-map = <0 0 0 0 &gic GIC_SPI 70 IRQ_TYPE_LEVEL_HIGH>;
				marvell,pcie-port = <2>;
				marvell,pcie-lane = <0>;
				clocks = <&gateclk 6>;
				status = "disabled";
			};

			/*
			 * x1 port only available when pcie@1,0 is
			 * configured as a x1 port
			 */
			pcie@4,0 {
				device_type = "pci";
				assigned-addresses = <0x82000800 0 0x48000 0 0x2000>;
				reg = <0x2000 0 0 0 0>;
				#address-cells = <3>;
				#size-cells = <2>;
				#interrupt-cells = <1>;
				ranges = <0x82000000 0 0 0x82000000 0x4 0 1 0
					  0x81000000 0 0 0x81000000 0x4 0 1 0>;
				interrupt-map-mask = <0 0 0 0>;
				interrupt-map = <0 0 0 0 &gic GIC_SPI 71 IRQ_TYPE_LEVEL_HIGH>;
				marvell,pcie-port = <3>;
				marvell,pcie-lane = <0>;
				clocks = <&gateclk 7>;
				status = "disabled";
			};
		};
	};
};
