/*
 * Copyright 2013 Maxime Ripard
 *
 * Maxime Ripard <maxime.ripard@free-electrons.com>
 *
 * This file is dual-licensed: you can use it either under the terms
 * of the GPL or the X11 license, at your option. Note that this dual
 * licensing only applies to this file, and not this project as a
 * whole.
 *
 *  a) This file is free software; you can redistribute it and/or
 *     modify it under the terms of the GNU General Public License as
 *     published by the Free Software Foundation; either version 2 of the
 *     License, or (at your option) any later version.
 *
 *     This file is distributed in the hope that it will be useful,
 *     but WITHOUT ANY WARRANTY; without even the implied warranty of
 *     MERCHANTABILITY or FITNESS FOR A PARTICULAR PURPOSE.  See the
 *     GNU General Public License for more details.
 *
 *     You should have received a copy of the GNU General Public
 *     License along with this file; if not, write to the Free
 *     Software Foundation, Inc., 51 Franklin St, Fifth Floor, Boston,
 *     MA 02110-1301 USA
 *
 * Or, alternatively,
 *
 *  b) Permission is hereby granted, free of charge, to any person
 *     obtaining a copy of this software and associated documentation
 *     files (the "Software"), to deal in the Software without
 *     restriction, including without limitation the rights to use,
 *     copy, modify, merge, publish, distribute, sublicense, and/or
 *     sell copies of the Software, and to permit persons to whom the
 *     Software is furnished to do so, subject to the following
 *     conditions:
 *
 *     The above copyright notice and this permission notice shall be
 *     included in all copies or substantial portions of the Software.
 *
 *     THE SOFTWARE IS PROVIDED "AS IS", WITHOUT WARRANTY OF ANY KIND,
 *     EXPRESS OR IMPLIED, INCLUDING BUT NOT LIMITED TO THE WARRANTIES
 *     OF MERCHANTABILITY, FITNESS FOR A PARTICULAR PURPOSE AND
 *     NONINFRINGEMENT. IN NO EVENT SHALL THE AUTHORS OR COPYRIGHT
 *     HOLDERS BE LIABLE FOR ANY CLAIM, DAMAGES OR OTHER LIABILITY,
 *     WHETHER IN AN ACTION OF CONTRACT, TORT OR OTHERWISE, ARISING
 *     FROM, OUT OF OR IN CONNECTION WITH THE SOFTWARE OR THE USE OR
 *     OTHER DEALINGS IN THE SOFTWARE.
 */

#include "skeleton.dtsi"

#include <dt-bindings/interrupt-controller/arm-gic.h>
#include <dt-bindings/thermal/thermal.h>

#include <dt-bindings/dma/sun4i-a10.h>
#include <dt-bindings/pinctrl/sun4i-a10.h>

/ {
	interrupt-parent = <&gic>;

	aliases {
		ethernet0 = &gmac;
	};

	chosen {
		#address-cells = <1>;
		#size-cells = <1>;
		ranges;

		framebuffer@0 {
			compatible = "allwinner,simple-framebuffer", "simple-framebuffer";
			allwinner,pipeline = "de_be0-lcd0-hdmi";
			clocks = <&pll5 1>, <&ahb_gates 36>, <&ahb_gates 43>,
				 <&ahb_gates 44>;
			status = "disabled";
		};

		framebuffer@1 {
			compatible = "allwinner,simple-framebuffer",
				     "simple-framebuffer";
			allwinner,pipeline = "de_be0-lcd0";
			clocks = <&pll5 1>, <&ahb_gates 36>, <&ahb_gates 44>;
			status = "disabled";
		};

		framebuffer@2 {
			compatible = "allwinner,simple-framebuffer",
				     "simple-framebuffer";
			allwinner,pipeline = "de_be0-lcd0-tve0";
			clocks = <&pll5 1>, <&ahb_gates 34>, <&ahb_gates 36>,
				 <&ahb_gates 44>;
			status = "disabled";
		};
	};

	cpus {
		#address-cells = <1>;
		#size-cells = <0>;

		cpu0: cpu@0 {
			compatible = "arm,cortex-a7";
			device_type = "cpu";
			reg = <0>;
			clocks = <&cpu>;
			clock-latency = <244144>; /* 8 32k periods */
			operating-points = <
				/* kHz    uV */
				960000  1400000
				912000  1400000
				864000  1300000
				720000  1200000
				528000  1100000
				312000  1000000
				144000  900000
				>;
			#cooling-cells = <2>;
			cooling-min-level = <0>;
			cooling-max-level = <6>;
		};

		cpu@1 {
			compatible = "arm,cortex-a7";
			device_type = "cpu";
			reg = <1>;
		};
	};

	thermal-zones {
		cpu_thermal {
			/* milliseconds */
			polling-delay-passive = <250>;
			polling-delay = <1000>;
			thermal-sensors = <&rtp>;

			cooling-maps {
				map0 {
					trip = <&cpu_alert0>;
					cooling-device = <&cpu0 THERMAL_NO_LIMIT THERMAL_NO_LIMIT>;
				};
			};

			trips {
				cpu_alert0: cpu_alert0 {
					/* milliCelsius */
					temperature = <75000>;
					hysteresis = <2000>;
					type = "passive";
				};

				cpu_crit: cpu_crit {
					/* milliCelsius */
					temperature = <100000>;
					hysteresis = <2000>;
					type = "critical";
				};
			};
		};
	};

	memory {
		reg = <0x40000000 0x80000000>;
	};

	timer {
		compatible = "arm,armv7-timer";
		interrupts = <GIC_PPI 13 (GIC_CPU_MASK_SIMPLE(4) | IRQ_TYPE_LEVEL_LOW)>,
			     <GIC_PPI 14 (GIC_CPU_MASK_SIMPLE(4) | IRQ_TYPE_LEVEL_LOW)>,
			     <GIC_PPI 11 (GIC_CPU_MASK_SIMPLE(4) | IRQ_TYPE_LEVEL_LOW)>,
			     <GIC_PPI 10 (GIC_CPU_MASK_SIMPLE(4) | IRQ_TYPE_LEVEL_LOW)>;
	};

	pmu {
		compatible = "arm,cortex-a7-pmu", "arm,cortex-a15-pmu";
		interrupts = <GIC_SPI 120 IRQ_TYPE_LEVEL_HIGH>,
			     <GIC_SPI 121 IRQ_TYPE_LEVEL_HIGH>;
	};

	clocks {
		#address-cells = <1>;
		#size-cells = <1>;
		ranges;

		osc24M: clk@01c20050 {
			#clock-cells = <0>;
			compatible = "allwinner,sun4i-a10-osc-clk";
			reg = <0x01c20050 0x4>;
			clock-frequency = <24000000>;
			clock-output-names = "osc24M";
		};

		osc32k: clk@0 {
			#clock-cells = <0>;
			compatible = "fixed-clock";
			clock-frequency = <32768>;
			clock-output-names = "osc32k";
		};

		pll1: clk@01c20000 {
			#clock-cells = <0>;
			compatible = "allwinner,sun4i-a10-pll1-clk";
			reg = <0x01c20000 0x4>;
			clocks = <&osc24M>;
			clock-output-names = "pll1";
		};

		pll4: clk@01c20018 {
			#clock-cells = <0>;
			compatible = "allwinner,sun7i-a20-pll4-clk";
			reg = <0x01c20018 0x4>;
			clocks = <&osc24M>;
			clock-output-names = "pll4";
		};

		pll5: clk@01c20020 {
			#clock-cells = <1>;
			compatible = "allwinner,sun4i-a10-pll5-clk";
			reg = <0x01c20020 0x4>;
			clocks = <&osc24M>;
			clock-output-names = "pll5_ddr", "pll5_other";
		};

		pll6: clk@01c20028 {
			#clock-cells = <1>;
			compatible = "allwinner,sun4i-a10-pll6-clk";
			reg = <0x01c20028 0x4>;
			clocks = <&osc24M>;
			clock-output-names = "pll6_sata", "pll6_other", "pll6";
		};

		pll8: clk@01c20040 {
			#clock-cells = <0>;
			compatible = "allwinner,sun7i-a20-pll4-clk";
			reg = <0x01c20040 0x4>;
			clocks = <&osc24M>;
			clock-output-names = "pll8";
		};

		cpu: cpu@01c20054 {
			#clock-cells = <0>;
			compatible = "allwinner,sun4i-a10-cpu-clk";
			reg = <0x01c20054 0x4>;
			clocks = <&osc32k>, <&osc24M>, <&pll1>, <&pll6 1>;
			clock-output-names = "cpu";
		};

		axi: axi@01c20054 {
			#clock-cells = <0>;
			compatible = "allwinner,sun4i-a10-axi-clk";
			reg = <0x01c20054 0x4>;
			clocks = <&cpu>;
			clock-output-names = "axi";
		};

		ahb: ahb@01c20054 {
			#clock-cells = <0>;
			compatible = "allwinner,sun4i-a10-ahb-clk";
			reg = <0x01c20054 0x4>;
			clocks = <&axi>;
			clock-output-names = "ahb";
		};

		ahb_gates: clk@01c20060 {
			#clock-cells = <1>;
			compatible = "allwinner,sun7i-a20-ahb-gates-clk";
			reg = <0x01c20060 0x8>;
			clocks = <&ahb>;
			clock-output-names = "ahb_usb0", "ahb_ehci0",
				"ahb_ohci0", "ahb_ehci1", "ahb_ohci1",
				"ahb_ss", "ahb_dma", "ahb_bist", "ahb_mmc0",
				"ahb_mmc1", "ahb_mmc2", "ahb_mmc3", "ahb_ms",
				"ahb_nand", "ahb_sdram", "ahb_ace",
				"ahb_emac", "ahb_ts", "ahb_spi0", "ahb_spi1",
				"ahb_spi2", "ahb_spi3", "ahb_sata",
				"ahb_hstimer", "ahb_ve", "ahb_tvd", "ahb_tve0",
				"ahb_tve1", "ahb_lcd0", "ahb_lcd1", "ahb_csi0",
				"ahb_csi1", "ahb_hdmi1", "ahb_hdmi0",
				"ahb_de_be0", "ahb_de_be1", "ahb_de_fe0",
				"ahb_de_fe1", "ahb_gmac", "ahb_mp",
				"ahb_mali";
		};

		apb0: apb0@01c20054 {
			#clock-cells = <0>;
			compatible = "allwinner,sun4i-a10-apb0-clk";
			reg = <0x01c20054 0x4>;
			clocks = <&ahb>;
			clock-output-names = "apb0";
		};

		apb0_gates: clk@01c20068 {
			#clock-cells = <1>;
			compatible = "allwinner,sun7i-a20-apb0-gates-clk";
			reg = <0x01c20068 0x4>;
			clocks = <&apb0>;
			clock-output-names = "apb0_codec", "apb0_spdif",
				"apb0_ac97", "apb0_iis0", "apb0_iis1",
				"apb0_pio", "apb0_ir0", "apb0_ir1",
				"apb0_iis2", "apb0_keypad";
		};

		apb1: clk@01c20058 {
			#clock-cells = <0>;
			compatible = "allwinner,sun4i-a10-apb1-clk";
			reg = <0x01c20058 0x4>;
			clocks = <&osc24M>, <&pll6 1>, <&osc32k>;
			clock-output-names = "apb1";
		};

		apb1_gates: clk@01c2006c {
			#clock-cells = <1>;
			compatible = "allwinner,sun7i-a20-apb1-gates-clk";
			reg = <0x01c2006c 0x4>;
			clocks = <&apb1>;
			clock-output-names = "apb1_i2c0", "apb1_i2c1",
				"apb1_i2c2", "apb1_i2c3", "apb1_can",
				"apb1_scr", "apb1_ps20", "apb1_ps21",
				"apb1_i2c4", "apb1_uart0", "apb1_uart1",
				"apb1_uart2", "apb1_uart3", "apb1_uart4",
				"apb1_uart5", "apb1_uart6", "apb1_uart7";
		};

		nand_clk: clk@01c20080 {
			#clock-cells = <0>;
			compatible = "allwinner,sun4i-a10-mod0-clk";
			reg = <0x01c20080 0x4>;
			clocks = <&osc24M>, <&pll6 1>, <&pll5 1>;
			clock-output-names = "nand";
		};

		ms_clk: clk@01c20084 {
			#clock-cells = <0>;
			compatible = "allwinner,sun4i-a10-mod0-clk";
			reg = <0x01c20084 0x4>;
			clocks = <&osc24M>, <&pll6 1>, <&pll5 1>;
			clock-output-names = "ms";
		};

		mmc0_clk: clk@01c20088 {
			#clock-cells = <1>;
			compatible = "allwinner,sun4i-a10-mmc-clk";
			reg = <0x01c20088 0x4>;
			clocks = <&osc24M>, <&pll6 1>, <&pll5 1>;
			clock-output-names = "mmc0",
					     "mmc0_output",
					     "mmc0_sample";
		};

		mmc1_clk: clk@01c2008c {
			#clock-cells = <1>;
			compatible = "allwinner,sun4i-a10-mmc-clk";
			reg = <0x01c2008c 0x4>;
			clocks = <&osc24M>, <&pll6 1>, <&pll5 1>;
			clock-output-names = "mmc1",
					     "mmc1_output",
					     "mmc1_sample";
		};

		mmc2_clk: clk@01c20090 {
			#clock-cells = <1>;
			compatible = "allwinner,sun4i-a10-mmc-clk";
			reg = <0x01c20090 0x4>;
			clocks = <&osc24M>, <&pll6 1>, <&pll5 1>;
			clock-output-names = "mmc2",
					     "mmc2_output",
					     "mmc2_sample";
		};

		mmc3_clk: clk@01c20094 {
			#clock-cells = <1>;
			compatible = "allwinner,sun4i-a10-mmc-clk";
			reg = <0x01c20094 0x4>;
			clocks = <&osc24M>, <&pll6 1>, <&pll5 1>;
			clock-output-names = "mmc3",
					     "mmc3_output",
					     "mmc3_sample";
		};

		ts_clk: clk@01c20098 {
			#clock-cells = <0>;
			compatible = "allwinner,sun4i-a10-mod0-clk";
			reg = <0x01c20098 0x4>;
			clocks = <&osc24M>, <&pll6 1>, <&pll5 1>;
			clock-output-names = "ts";
		};

		ss_clk: clk@01c2009c {
			#clock-cells = <0>;
			compatible = "allwinner,sun4i-a10-mod0-clk";
			reg = <0x01c2009c 0x4>;
			clocks = <&osc24M>, <&pll6 1>, <&pll5 1>;
			clock-output-names = "ss";
		};

		spi0_clk: clk@01c200a0 {
			#clock-cells = <0>;
			compatible = "allwinner,sun4i-a10-mod0-clk";
			reg = <0x01c200a0 0x4>;
			clocks = <&osc24M>, <&pll6 1>, <&pll5 1>;
			clock-output-names = "spi0";
		};

		spi1_clk: clk@01c200a4 {
			#clock-cells = <0>;
			compatible = "allwinner,sun4i-a10-mod0-clk";
			reg = <0x01c200a4 0x4>;
			clocks = <&osc24M>, <&pll6 1>, <&pll5 1>;
			clock-output-names = "spi1";
		};

		spi2_clk: clk@01c200a8 {
			#clock-cells = <0>;
			compatible = "allwinner,sun4i-a10-mod0-clk";
			reg = <0x01c200a8 0x4>;
			clocks = <&osc24M>, <&pll6 1>, <&pll5 1>;
			clock-output-names = "spi2";
		};

		pata_clk: clk@01c200ac {
			#clock-cells = <0>;
			compatible = "allwinner,sun4i-a10-mod0-clk";
			reg = <0x01c200ac 0x4>;
			clocks = <&osc24M>, <&pll6 1>, <&pll5 1>;
			clock-output-names = "pata";
		};

		ir0_clk: clk@01c200b0 {
			#clock-cells = <0>;
			compatible = "allwinner,sun4i-a10-mod0-clk";
			reg = <0x01c200b0 0x4>;
			clocks = <&osc24M>, <&pll6 1>, <&pll5 1>;
			clock-output-names = "ir0";
		};

		ir1_clk: clk@01c200b4 {
			#clock-cells = <0>;
			compatible = "allwinner,sun4i-a10-mod0-clk";
			reg = <0x01c200b4 0x4>;
			clocks = <&osc24M>, <&pll6 1>, <&pll5 1>;
			clock-output-names = "ir1";
		};

		usb_clk: clk@01c200cc {
			#clock-cells = <1>;
		        #reset-cells = <1>;
			compatible = "allwinner,sun4i-a10-usb-clk";
			reg = <0x01c200cc 0x4>;
			clocks = <&pll6 1>;
			clock-output-names = "usb_ohci0", "usb_ohci1", "usb_phy";
		};

		spi3_clk: clk@01c200d4 {
			#clock-cells = <0>;
			compatible = "allwinner,sun4i-a10-mod0-clk";
			reg = <0x01c200d4 0x4>;
			clocks = <&osc24M>, <&pll6 1>, <&pll5 1>;
			clock-output-names = "spi3";
		};

		mbus_clk: clk@01c2015c {
			#clock-cells = <0>;
			compatible = "allwinner,sun5i-a13-mbus-clk";
			reg = <0x01c2015c 0x4>;
			clocks = <&osc24M>, <&pll6 2>, <&pll5 1>;
			clock-output-names = "mbus";
		};

		/*
		 * The following two are dummy clocks, placeholders used in the gmac_tx
		 * clock. The gmac driver will choose one parent depending on the PHY
		 * interface mode, using clk_set_rate auto-reparenting.
		 * The actual TX clock rate is not controlled by the gmac_tx clock.
		 */
		mii_phy_tx_clk: clk@2 {
			#clock-cells = <0>;
			compatible = "fixed-clock";
			clock-frequency = <25000000>;
			clock-output-names = "mii_phy_tx";
		};

		gmac_int_tx_clk: clk@3 {
			#clock-cells = <0>;
			compatible = "fixed-clock";
			clock-frequency = <125000000>;
			clock-output-names = "gmac_int_tx";
		};

		gmac_tx_clk: clk@01c20164 {
			#clock-cells = <0>;
			compatible = "allwinner,sun7i-a20-gmac-clk";
			reg = <0x01c20164 0x4>;
			clocks = <&mii_phy_tx_clk>, <&gmac_int_tx_clk>;
			clock-output-names = "gmac_tx";
		};

		/*
		 * Dummy clock used by output clocks
		 */
		osc24M_32k: clk@1 {
			#clock-cells = <0>;
			compatible = "fixed-factor-clock";
			clock-div = <750>;
			clock-mult = <1>;
			clocks = <&osc24M>;
			clock-output-names = "osc24M_32k";
		};

		clk_out_a: clk@01c201f0 {
			#clock-cells = <0>;
			compatible = "allwinner,sun7i-a20-out-clk";
			reg = <0x01c201f0 0x4>;
			clocks = <&osc24M_32k>, <&osc32k>, <&osc24M>;
			clock-output-names = "clk_out_a";
		};

		clk_out_b: clk@01c201f4 {
			#clock-cells = <0>;
			compatible = "allwinner,sun7i-a20-out-clk";
			reg = <0x01c201f4 0x4>;
			clocks = <&osc24M_32k>, <&osc32k>, <&osc24M>;
			clock-output-names = "clk_out_b";
		};
	};

	soc@01c00000 {
		compatible = "simple-bus";
		#address-cells = <1>;
		#size-cells = <1>;
		ranges;

		nmi_intc: interrupt-controller@01c00030 {
			compatible = "allwinner,sun7i-a20-sc-nmi";
			interrupt-controller;
			#interrupt-cells = <2>;
			reg = <0x01c00030 0x0c>;
			interrupts = <GIC_SPI 0 IRQ_TYPE_LEVEL_HIGH>;
		};

		dma: dma-controller@01c02000 {
			compatible = "allwinner,sun4i-a10-dma";
			reg = <0x01c02000 0x1000>;
			interrupts = <GIC_SPI 27 IRQ_TYPE_LEVEL_HIGH>;
			clocks = <&ahb_gates 6>;
			#dma-cells = <2>;
		};

		spi0: spi@01c05000 {
			compatible = "allwinner,sun4i-a10-spi";
			reg = <0x01c05000 0x1000>;
			interrupts = <GIC_SPI 10 IRQ_TYPE_LEVEL_HIGH>;
			clocks = <&ahb_gates 20>, <&spi0_clk>;
			clock-names = "ahb", "mod";
			dmas = <&dma SUN4I_DMA_DEDICATED 27>,
			       <&dma SUN4I_DMA_DEDICATED 26>;
			dma-names = "rx", "tx";
			status = "disabled";
			#address-cells = <1>;
			#size-cells = <0>;
		};

		spi1: spi@01c06000 {
			compatible = "allwinner,sun4i-a10-spi";
			reg = <0x01c06000 0x1000>;
			interrupts = <GIC_SPI 11 IRQ_TYPE_LEVEL_HIGH>;
			clocks = <&ahb_gates 21>, <&spi1_clk>;
			clock-names = "ahb", "mod";
			dmas = <&dma SUN4I_DMA_DEDICATED 9>,
			       <&dma SUN4I_DMA_DEDICATED 8>;
			dma-names = "rx", "tx";
			status = "disabled";
			#address-cells = <1>;
			#size-cells = <0>;
		};

		emac: ethernet@01c0b000 {
			compatible = "allwinner,sun4i-a10-emac";
			reg = <0x01c0b000 0x1000>;
			interrupts = <GIC_SPI 55 IRQ_TYPE_LEVEL_HIGH>;
			clocks = <&ahb_gates 17>;
			status = "disabled";
		};

		mdio: mdio@01c0b080 {
			compatible = "allwinner,sun4i-a10-mdio";
			reg = <0x01c0b080 0x14>;
			status = "disabled";
			#address-cells = <1>;
			#size-cells = <0>;
		};

		mmc0: mmc@01c0f000 {
			compatible = "allwinner,sun5i-a13-mmc";
			reg = <0x01c0f000 0x1000>;
			clocks = <&ahb_gates 8>,
				 <&mmc0_clk 0>,
				 <&mmc0_clk 1>,
				 <&mmc0_clk 2>;
			clock-names = "ahb",
				      "mmc",
				      "output",
				      "sample";
			interrupts = <GIC_SPI 32 IRQ_TYPE_LEVEL_HIGH>;
			status = "disabled";
		};

		mmc1: mmc@01c10000 {
			compatible = "allwinner,sun5i-a13-mmc";
			reg = <0x01c10000 0x1000>;
			clocks = <&ahb_gates 9>,
				 <&mmc1_clk 0>,
				 <&mmc1_clk 1>,
				 <&mmc1_clk 2>;
			clock-names = "ahb",
				      "mmc",
				      "output",
				      "sample";
			interrupts = <GIC_SPI 33 IRQ_TYPE_LEVEL_HIGH>;
			status = "disabled";
		};

		mmc2: mmc@01c11000 {
			compatible = "allwinner,sun5i-a13-mmc";
			reg = <0x01c11000 0x1000>;
			clocks = <&ahb_gates 10>,
				 <&mmc2_clk 0>,
				 <&mmc2_clk 1>,
				 <&mmc2_clk 2>;
			clock-names = "ahb",
				      "mmc",
				      "output",
				      "sample";
			interrupts = <GIC_SPI 34 IRQ_TYPE_LEVEL_HIGH>;
			status = "disabled";
		};

		mmc3: mmc@01c12000 {
			compatible = "allwinner,sun5i-a13-mmc";
			reg = <0x01c12000 0x1000>;
			clocks = <&ahb_gates 11>,
				 <&mmc3_clk 0>,
				 <&mmc3_clk 1>,
				 <&mmc3_clk 2>;
			clock-names = "ahb",
				      "mmc",
				      "output",
				      "sample";
			interrupts = <GIC_SPI 35 IRQ_TYPE_LEVEL_HIGH>;
			status = "disabled";
		};

		usbphy: phy@01c13400 {
			#phy-cells = <1>;
			compatible = "allwinner,sun7i-a20-usb-phy";
			reg = <0x01c13400 0x10 0x01c14800 0x4 0x01c1c800 0x4>;
			reg-names = "phy_ctrl", "pmu1", "pmu2";
			clocks = <&usb_clk 8>;
			clock-names = "usb_phy";
			resets = <&usb_clk 0>, <&usb_clk 1>, <&usb_clk 2>;
			reset-names = "usb0_reset", "usb1_reset", "usb2_reset";
			status = "disabled";
		};

		ehci0: usb@01c14000 {
			compatible = "allwinner,sun7i-a20-ehci", "generic-ehci";
			reg = <0x01c14000 0x100>;
			interrupts = <GIC_SPI 39 IRQ_TYPE_LEVEL_HIGH>;
			clocks = <&ahb_gates 1>;
			phys = <&usbphy 1>;
			phy-names = "usb";
			status = "disabled";
		};

		ohci0: usb@01c14400 {
			compatible = "allwinner,sun7i-a20-ohci", "generic-ohci";
			reg = <0x01c14400 0x100>;
			interrupts = <GIC_SPI 64 IRQ_TYPE_LEVEL_HIGH>;
			clocks = <&usb_clk 6>, <&ahb_gates 2>;
			phys = <&usbphy 1>;
			phy-names = "usb";
			status = "disabled";
		};

		spi2: spi@01c17000 {
			compatible = "allwinner,sun4i-a10-spi";
			reg = <0x01c17000 0x1000>;
			interrupts = <GIC_SPI 12 IRQ_TYPE_LEVEL_HIGH>;
			clocks = <&ahb_gates 22>, <&spi2_clk>;
			clock-names = "ahb", "mod";
			dmas = <&dma SUN4I_DMA_DEDICATED 29>,
			       <&dma SUN4I_DMA_DEDICATED 28>;
			dma-names = "rx", "tx";
			status = "disabled";
			#address-cells = <1>;
			#size-cells = <0>;
		};

		ahci: sata@01c18000 {
			compatible = "allwinner,sun4i-a10-ahci";
			reg = <0x01c18000 0x1000>;
			interrupts = <GIC_SPI 56 IRQ_TYPE_LEVEL_HIGH>;
			clocks = <&pll6 0>, <&ahb_gates 25>;
			status = "disabled";
		};

		ehci1: usb@01c1c000 {
			compatible = "allwinner,sun7i-a20-ehci", "generic-ehci";
			reg = <0x01c1c000 0x100>;
			interrupts = <GIC_SPI 40 IRQ_TYPE_LEVEL_HIGH>;
			clocks = <&ahb_gates 3>;
			phys = <&usbphy 2>;
			phy-names = "usb";
			status = "disabled";
		};

		ohci1: usb@01c1c400 {
			compatible = "allwinner,sun7i-a20-ohci", "generic-ohci";
			reg = <0x01c1c400 0x100>;
			interrupts = <GIC_SPI 65 IRQ_TYPE_LEVEL_HIGH>;
			clocks = <&usb_clk 7>, <&ahb_gates 4>;
			phys = <&usbphy 2>;
			phy-names = "usb";
			status = "disabled";
		};

		spi3: spi@01c1f000 {
			compatible = "allwinner,sun4i-a10-spi";
			reg = <0x01c1f000 0x1000>;
			interrupts = <GIC_SPI 50 IRQ_TYPE_LEVEL_HIGH>;
			clocks = <&ahb_gates 23>, <&spi3_clk>;
			clock-names = "ahb", "mod";
			dmas = <&dma SUN4I_DMA_DEDICATED 31>,
			       <&dma SUN4I_DMA_DEDICATED 30>;
			dma-names = "rx", "tx";
			status = "disabled";
			#address-cells = <1>;
			#size-cells = <0>;
		};

		pio: pinctrl@01c20800 {
			compatible = "allwinner,sun7i-a20-pinctrl";
			reg = <0x01c20800 0x400>;
			interrupts = <GIC_SPI 28 IRQ_TYPE_LEVEL_HIGH>;
			clocks = <&apb0_gates 5>;
			gpio-controller;
			interrupt-controller;
			#interrupt-cells = <2>;
			#size-cells = <0>;
			#gpio-cells = <3>;

			pwm0_pins_a: pwm0@0 {
				allwinner,pins = "PB2";
				allwinner,function = "pwm";
				allwinner,drive = <SUN4I_PINCTRL_10_MA>;
				allwinner,pull = <SUN4I_PINCTRL_NO_PULL>;
			};

			pwm1_pins_a: pwm1@0 {
				allwinner,pins = "PI3";
				allwinner,function = "pwm";
				allwinner,drive = <SUN4I_PINCTRL_10_MA>;
				allwinner,pull = <SUN4I_PINCTRL_NO_PULL>;
			};

			uart0_pins_a: uart0@0 {
				allwinner,pins = "PB22", "PB23";
				allwinner,function = "uart0";
				allwinner,drive = <SUN4I_PINCTRL_10_MA>;
				allwinner,pull = <SUN4I_PINCTRL_NO_PULL>;
			};

			uart2_pins_a: uart2@0 {
				allwinner,pins = "PI16", "PI17", "PI18", "PI19";
				allwinner,function = "uart2";
				allwinner,drive = <SUN4I_PINCTRL_10_MA>;
				allwinner,pull = <SUN4I_PINCTRL_NO_PULL>;
			};

			uart3_pins_a: uart3@0 {
				allwinner,pins = "PG6", "PG7", "PG8", "PG9";
				allwinner,function = "uart3";
				allwinner,drive = <SUN4I_PINCTRL_10_MA>;
				allwinner,pull = <SUN4I_PINCTRL_NO_PULL>;
			};

			uart3_pins_b: uart3@1 {
				allwinner,pins = "PH0", "PH1";
				allwinner,function = "uart3";
				allwinner,drive = <SUN4I_PINCTRL_10_MA>;
				allwinner,pull = <SUN4I_PINCTRL_NO_PULL>;
			};

			uart4_pins_a: uart4@0 {
				allwinner,pins = "PG10", "PG11";
				allwinner,function = "uart4";
				allwinner,drive = <SUN4I_PINCTRL_10_MA>;
				allwinner,pull = <SUN4I_PINCTRL_NO_PULL>;
			};

			uart5_pins_a: uart5@0 {
				allwinner,pins = "PI10", "PI11";
				allwinner,function = "uart5";
				allwinner,drive = <SUN4I_PINCTRL_10_MA>;
				allwinner,pull = <SUN4I_PINCTRL_NO_PULL>;
			};

			uart6_pins_a: uart6@0 {
				allwinner,pins = "PI12", "PI13";
				allwinner,function = "uart6";
				allwinner,drive = <SUN4I_PINCTRL_10_MA>;
				allwinner,pull = <SUN4I_PINCTRL_NO_PULL>;
			};

			uart7_pins_a: uart7@0 {
				allwinner,pins = "PI20", "PI21";
				allwinner,function = "uart7";
				allwinner,drive = <SUN4I_PINCTRL_10_MA>;
				allwinner,pull = <SUN4I_PINCTRL_NO_PULL>;
			};

			i2c0_pins_a: i2c0@0 {
				allwinner,pins = "PB0", "PB1";
				allwinner,function = "i2c0";
				allwinner,drive = <SUN4I_PINCTRL_10_MA>;
				allwinner,pull = <SUN4I_PINCTRL_NO_PULL>;
			};

			i2c1_pins_a: i2c1@0 {
				allwinner,pins = "PB18", "PB19";
				allwinner,function = "i2c1";
				allwinner,drive = <SUN4I_PINCTRL_10_MA>;
				allwinner,pull = <SUN4I_PINCTRL_NO_PULL>;
			};

			i2c2_pins_a: i2c2@0 {
				allwinner,pins = "PB20", "PB21";
				allwinner,function = "i2c2";
				allwinner,drive = <SUN4I_PINCTRL_10_MA>;
				allwinner,pull = <SUN4I_PINCTRL_NO_PULL>;
			};

			i2c3_pins_a: i2c3@0 {
				allwinner,pins = "PI0", "PI1";
				allwinner,function = "i2c3";
				allwinner,drive = <SUN4I_PINCTRL_10_MA>;
				allwinner,pull = <SUN4I_PINCTRL_NO_PULL>;
			};

			emac_pins_a: emac0@0 {
				allwinner,pins = "PA0", "PA1", "PA2",
						"PA3", "PA4", "PA5", "PA6",
						"PA7", "PA8", "PA9", "PA10",
						"PA11", "PA12", "PA13", "PA14",
						"PA15", "PA16";
				allwinner,function = "emac";
				allwinner,drive = <SUN4I_PINCTRL_10_MA>;
				allwinner,pull = <SUN4I_PINCTRL_NO_PULL>;
			};

			clk_out_a_pins_a: clk_out_a@0 {
				allwinner,pins = "PI12";
				allwinner,function = "clk_out_a";
				allwinner,drive = <SUN4I_PINCTRL_10_MA>;
				allwinner,pull = <SUN4I_PINCTRL_NO_PULL>;
			};

			clk_out_b_pins_a: clk_out_b@0 {
				allwinner,pins = "PI13";
				allwinner,function = "clk_out_b";
				allwinner,drive = <SUN4I_PINCTRL_10_MA>;
				allwinner,pull = <SUN4I_PINCTRL_NO_PULL>;
			};

			gmac_pins_mii_a: gmac_mii@0 {
				allwinner,pins = "PA0", "PA1", "PA2",
						"PA3", "PA4", "PA5", "PA6",
						"PA7", "PA8", "PA9", "PA10",
						"PA11", "PA12", "PA13", "PA14",
						"PA15", "PA16";
				allwinner,function = "gmac";
				allwinner,drive = <SUN4I_PINCTRL_10_MA>;
				allwinner,pull = <SUN4I_PINCTRL_NO_PULL>;
			};

			gmac_pins_rgmii_a: gmac_rgmii@0 {
				allwinner,pins = "PA0", "PA1", "PA2",
						"PA3", "PA4", "PA5", "PA6",
						"PA7", "PA8", "PA10",
						"PA11", "PA12", "PA13",
						"PA15", "PA16";
				allwinner,function = "gmac";
				/*
				 * data lines in RGMII mode use DDR mode
				 * and need a higher signal drive strength
				 */
				allwinner,drive = <SUN4I_PINCTRL_40_MA>;
				allwinner,pull = <SUN4I_PINCTRL_NO_PULL>;
			};

			spi0_pins_a: spi0@0 {
				allwinner,pins = "PI10", "PI11", "PI12", "PI13", "PI14";
				allwinner,function = "spi0";
				allwinner,drive = <SUN4I_PINCTRL_10_MA>;
				allwinner,pull = <SUN4I_PINCTRL_NO_PULL>;
			};

			spi1_pins_a: spi1@0 {
				allwinner,pins = "PI16", "PI17", "PI18", "PI19";
				allwinner,function = "spi1";
				allwinner,drive = <SUN4I_PINCTRL_10_MA>;
				allwinner,pull = <SUN4I_PINCTRL_NO_PULL>;
			};

			spi2_pins_a: spi2@0 {
				allwinner,pins = "PC19", "PC20", "PC21", "PC22";
				allwinner,function = "spi2";
				allwinner,drive = <SUN4I_PINCTRL_10_MA>;
				allwinner,pull = <SUN4I_PINCTRL_NO_PULL>;
			};

			spi2_pins_b: spi2@1 {
				allwinner,pins = "PB14", "PB15", "PB16", "PB17";
				allwinner,function = "spi2";
				allwinner,drive = <SUN4I_PINCTRL_10_MA>;
				allwinner,pull = <SUN4I_PINCTRL_NO_PULL>;
			};

			mmc0_pins_a: mmc0@0 {
				allwinner,pins = "PF0","PF1","PF2","PF3","PF4","PF5";
				allwinner,function = "mmc0";
				allwinner,drive = <SUN4I_PINCTRL_30_MA>;
				allwinner,pull = <SUN4I_PINCTRL_NO_PULL>;
			};

			mmc0_cd_pin_reference_design: mmc0_cd_pin@0 {
				allwinner,pins = "PH1";
				allwinner,function = "gpio_in";
				allwinner,drive = <SUN4I_PINCTRL_10_MA>;
				allwinner,pull = <SUN4I_PINCTRL_PULL_UP>;
			};

			mmc2_pins_a: mmc2@0 {
				allwinner,pins = "PC6","PC7","PC8","PC9","PC10","PC11";
				allwinner,function = "mmc2";
				allwinner,drive = <SUN4I_PINCTRL_30_MA>;
				allwinner,pull = <SUN4I_PINCTRL_PULL_UP>;
			};

			mmc3_pins_a: mmc3@0 {
				allwinner,pins = "PI4","PI5","PI6","PI7","PI8","PI9";
				allwinner,function = "mmc3";
				allwinner,drive = <SUN4I_PINCTRL_30_MA>;
				allwinner,pull = <SUN4I_PINCTRL_NO_PULL>;
			};

			ir0_pins_a: ir0@0 {
				    allwinner,pins = "PB3","PB4";
				    allwinner,function = "ir0";
				    allwinner,drive = <SUN4I_PINCTRL_10_MA>;
				    allwinner,pull = <SUN4I_PINCTRL_NO_PULL>;
			};

			ir1_pins_a: ir1@0 {
				    allwinner,pins = "PB22","PB23";
				    allwinner,function = "ir1";
				    allwinner,drive = <SUN4I_PINCTRL_10_MA>;
				    allwinner,pull = <SUN4I_PINCTRL_NO_PULL>;
			};

			ps20_pins_a: ps20@0 {
				allwinner,pins = "PI20", "PI21";
				allwinner,function = "ps2";
				allwinner,drive = <SUN4I_PINCTRL_10_MA>;
				allwinner,pull = <SUN4I_PINCTRL_NO_PULL>;
			};

			ps21_pins_a: ps21@0 {
				allwinner,pins = "PH12", "PH13";
				allwinner,function = "ps2";
				allwinner,drive = <SUN4I_PINCTRL_10_MA>;
				allwinner,pull = <SUN4I_PINCTRL_NO_PULL>;
			};
		};

		timer@01c20c00 {
			compatible = "allwinner,sun4i-a10-timer";
			reg = <0x01c20c00 0x90>;
			interrupts = <GIC_SPI 22 IRQ_TYPE_LEVEL_HIGH>,
				     <GIC_SPI 23 IRQ_TYPE_LEVEL_HIGH>,
				     <GIC_SPI 24 IRQ_TYPE_LEVEL_HIGH>,
				     <GIC_SPI 25 IRQ_TYPE_LEVEL_HIGH>,
				     <GIC_SPI 67 IRQ_TYPE_LEVEL_HIGH>,
				     <GIC_SPI 68 IRQ_TYPE_LEVEL_HIGH>;
			clocks = <&osc24M>;
		};

		wdt: watchdog@01c20c90 {
			compatible = "allwinner,sun4i-a10-wdt";
			reg = <0x01c20c90 0x10>;
		};

		rtc: rtc@01c20d00 {
			compatible = "allwinner,sun7i-a20-rtc";
			reg = <0x01c20d00 0x20>;
			interrupts = <GIC_SPI 24 IRQ_TYPE_LEVEL_HIGH>;
		};

		pwm: pwm@01c20e00 {
			compatible = "allwinner,sun7i-a20-pwm";
			reg = <0x01c20e00 0xc>;
			clocks = <&osc24M>;
			#pwm-cells = <3>;
			status = "disabled";
		};

		ir0: ir@01c21800 {
			compatible = "allwinner,sun4i-a10-ir";
			clocks = <&apb0_gates 6>, <&ir0_clk>;
			clock-names = "apb", "ir";
			interrupts = <GIC_SPI 5 IRQ_TYPE_LEVEL_HIGH>;
			reg = <0x01c21800 0x40>;
			status = "disabled";
		};

		ir1: ir@01c21c00 {
			compatible = "allwinner,sun4i-a10-ir";
			clocks = <&apb0_gates 7>, <&ir1_clk>;
			clock-names = "apb", "ir";
			interrupts = <GIC_SPI 6 IRQ_TYPE_LEVEL_HIGH>;
			reg = <0x01c21c00 0x40>;
			status = "disabled";
		};

		lradc: lradc@01c22800 {
			compatible = "allwinner,sun4i-a10-lradc-keys";
			reg = <0x01c22800 0x100>;
			interrupts = <GIC_SPI 31 IRQ_TYPE_LEVEL_HIGH>;
			status = "disabled";
		};

		sid: eeprom@01c23800 {
			compatible = "allwinner,sun7i-a20-sid";
			reg = <0x01c23800 0x200>;
		};

		rtp: rtp@01c25000 {
			compatible = "allwinner,sun4i-a10-ts";
			reg = <0x01c25000 0x100>;
			interrupts = <GIC_SPI 29 IRQ_TYPE_LEVEL_HIGH>;
			#thermal-sensor-cells = <0>;
		};

		uart0: serial@01c28000 {
			compatible = "snps,dw-apb-uart";
			reg = <0x01c28000 0x400>;
			interrupts = <GIC_SPI 1 IRQ_TYPE_LEVEL_HIGH>;
			reg-shift = <2>;
			reg-io-width = <4>;
			clocks = <&apb1_gates 16>;
			status = "disabled";
		};

		uart1: serial@01c28400 {
			compatible = "snps,dw-apb-uart";
			reg = <0x01c28400 0x400>;
			interrupts = <GIC_SPI 2 IRQ_TYPE_LEVEL_HIGH>;
			reg-shift = <2>;
			reg-io-width = <4>;
			clocks = <&apb1_gates 17>;
			status = "disabled";
		};

		uart2: serial@01c28800 {
			compatible = "snps,dw-apb-uart";
			reg = <0x01c28800 0x400>;
			interrupts = <GIC_SPI 3 IRQ_TYPE_LEVEL_HIGH>;
			reg-shift = <2>;
			reg-io-width = <4>;
			clocks = <&apb1_gates 18>;
			status = "disabled";
		};

		uart3: serial@01c28c00 {
			compatible = "snps,dw-apb-uart";
			reg = <0x01c28c00 0x400>;
			interrupts = <GIC_SPI 4 IRQ_TYPE_LEVEL_HIGH>;
			reg-shift = <2>;
			reg-io-width = <4>;
			clocks = <&apb1_gates 19>;
			status = "disabled";
		};

		uart4: serial@01c29000 {
			compatible = "snps,dw-apb-uart";
			reg = <0x01c29000 0x400>;
			interrupts = <GIC_SPI 17 IRQ_TYPE_LEVEL_HIGH>;
			reg-shift = <2>;
			reg-io-width = <4>;
			clocks = <&apb1_gates 20>;
			status = "disabled";
		};

		uart5: serial@01c29400 {
			compatible = "snps,dw-apb-uart";
			reg = <0x01c29400 0x400>;
			interrupts = <GIC_SPI 18 IRQ_TYPE_LEVEL_HIGH>;
			reg-shift = <2>;
			reg-io-width = <4>;
			clocks = <&apb1_gates 21>;
			status = "disabled";
		};

		uart6: serial@01c29800 {
			compatible = "snps,dw-apb-uart";
			reg = <0x01c29800 0x400>;
			interrupts = <GIC_SPI 19 IRQ_TYPE_LEVEL_HIGH>;
			reg-shift = <2>;
			reg-io-width = <4>;
			clocks = <&apb1_gates 22>;
			status = "disabled";
		};

		uart7: serial@01c29c00 {
			compatible = "snps,dw-apb-uart";
			reg = <0x01c29c00 0x400>;
			interrupts = <GIC_SPI 20 IRQ_TYPE_LEVEL_HIGH>;
			reg-shift = <2>;
			reg-io-width = <4>;
			clocks = <&apb1_gates 23>;
			status = "disabled";
		};

		i2c0: i2c@01c2ac00 {
			compatible = "allwinner,sun7i-a20-i2c", "allwinner,sun4i-a10-i2c";
			reg = <0x01c2ac00 0x400>;
			interrupts = <GIC_SPI 7 IRQ_TYPE_LEVEL_HIGH>;
			clocks = <&apb1_gates 0>;
			status = "disabled";
			#address-cells = <1>;
			#size-cells = <0>;
		};

		i2c1: i2c@01c2b000 {
			compatible = "allwinner,sun7i-a20-i2c", "allwinner,sun4i-a10-i2c";
			reg = <0x01c2b000 0x400>;
			interrupts = <GIC_SPI 8 IRQ_TYPE_LEVEL_HIGH>;
			clocks = <&apb1_gates 1>;
			status = "disabled";
			#address-cells = <1>;
			#size-cells = <0>;
		};

		i2c2: i2c@01c2b400 {
			compatible = "allwinner,sun7i-a20-i2c", "allwinner,sun4i-a10-i2c";
			reg = <0x01c2b400 0x400>;
			interrupts = <GIC_SPI 9 IRQ_TYPE_LEVEL_HIGH>;
			clocks = <&apb1_gates 2>;
			status = "disabled";
			#address-cells = <1>;
			#size-cells = <0>;
		};

		i2c3: i2c@01c2b800 {
			compatible = "allwinner,sun7i-a20-i2c", "allwinner,sun4i-a10-i2c";
			reg = <0x01c2b800 0x400>;
			interrupts = <GIC_SPI 88 IRQ_TYPE_LEVEL_HIGH>;
			clocks = <&apb1_gates 3>;
			status = "disabled";
			#address-cells = <1>;
			#size-cells = <0>;
		};

		i2c4: i2c@01c2c000 {
			compatible = "allwinner,sun7i-a20-i2c", "allwinner,sun4i-a10-i2c";
			reg = <0x01c2c000 0x400>;
			interrupts = <GIC_SPI 89 IRQ_TYPE_LEVEL_HIGH>;
			clocks = <&apb1_gates 15>;
			status = "disabled";
			#address-cells = <1>;
			#size-cells = <0>;
		};

		gmac: ethernet@01c50000 {
			compatible = "allwinner,sun7i-a20-gmac";
			reg = <0x01c50000 0x10000>;
			interrupts = <GIC_SPI 85 IRQ_TYPE_LEVEL_HIGH>;
			interrupt-names = "macirq";
			clocks = <&ahb_gates 49>, <&gmac_tx_clk>;
			clock-names = "stmmaceth", "allwinner_gmac_tx";
			snps,pbl = <2>;
			snps,fixed-burst;
			snps,force_sf_dma_mode;
			status = "disabled";
			#address-cells = <1>;
			#size-cells = <0>;
		};

		hstimer@01c60000 {
			compatible = "allwinner,sun7i-a20-hstimer";
			reg = <0x01c60000 0x1000>;
			interrupts = <GIC_SPI 81 IRQ_TYPE_LEVEL_HIGH>,
				     <GIC_SPI 82 IRQ_TYPE_LEVEL_HIGH>,
				     <GIC_SPI 83 IRQ_TYPE_LEVEL_HIGH>,
				     <GIC_SPI 84 IRQ_TYPE_LEVEL_HIGH>;
			clocks = <&ahb_gates 28>;
		};

		gic: interrupt-controller@01c81000 {
			compatible = "arm,cortex-a7-gic", "arm,cortex-a15-gic";
			reg = <0x01c81000 0x1000>,
			      <0x01c82000 0x1000>,
			      <0x01c84000 0x2000>,
			      <0x01c86000 0x2000>;
			interrupt-controller;
			#interrupt-cells = <3>;
			interrupts = <GIC_PPI 9 (GIC_CPU_MASK_SIMPLE(4) | IRQ_TYPE_LEVEL_HIGH)>;
		};

		ps20: ps2@01c2a000 {
			compatible = "allwinner,sun4i-a10-ps2";
			reg = <0x01c2a000 0x400>;
			interrupts = <GIC_SPI 62 IRQ_TYPE_LEVEL_HIGH>;
			clocks = <&apb1_gates 6>;
			status = "disabled";
		};

		ps21: ps2@01c2a400 {
			compatible = "allwinner,sun4i-a10-ps2";
			reg = <0x01c2a400 0x400>;
			interrupts = <GIC_SPI 63 IRQ_TYPE_LEVEL_HIGH>;
			clocks = <&apb1_gates 7>;
			status = "disabled";
		};
	};
};
