/*
 * Device Tree Include file for Marvell Armada XP family SoC
 *
 * Copyright (C) 2012 Marvell
 *
 * Lior Amsalem <alior@marvell.com>
 * Gregory CLEMENT <gregory.clement@free-electrons.com>
 * Thomas Petazzoni <thomas.petazzoni@free-electrons.com>
 * Ben Dooks <ben.dooks@codethink.co.uk>
 *
 * This file is dual-licensed: you can use it either under the terms
 * of the GPL or the X11 license, at your option. Note that this dual
 * licensing only applies to this file, and not this project as a
 * whole.
 *
 *  a) This file is free software; you can redistribute it and/or
 *     modify it under the terms of the GNU General Public License as
 *     published by the Free Software Foundation; either version 2 of the
 *     License, or (at your option) any later version.
 *
 *     This file is distributed in the hope that it will be useful
 *     but WITHOUT ANY WARRANTY; without even the implied warranty of
 *     MERCHANTABILITY or FITNESS FOR A PARTICULAR PURPOSE.  See the
 *     GNU General Public License for more details.
 *
 * Or, alternatively
 *
 *  b) Permission is hereby granted, free of charge, to any person
 *     obtaining a copy of this software and associated documentation
 *     files (the "Software"), to deal in the Software without
 *     restriction, including without limitation the rights to use
 *     copy, modify, merge, publish, distribute, sublicense, and/or
 *     sell copies of the Software, and to permit persons to whom the
 *     Software is furnished to do so, subject to the following
 *     conditions:
 *
 *     The above copyright notice and this permission notice shall be
 *     included in all copies or substantial portions of the Software.
 *
 *     THE SOFTWARE IS PROVIDED , WITHOUT WARRANTY OF ANY KIND
 *     EXPRESS OR IMPLIED, INCLUDING BUT NOT LIMITED TO THE WARRANTIES
 *     OF MERCHANTABILITY, FITNESS FOR A PARTICULAR PURPOSE AND
 *     NONINFRINGEMENT. IN NO EVENT SHALL THE AUTHORS OR COPYRIGHT
 *     HOLDERS BE LIABLE FOR ANY CLAIM, DAMAGES OR OTHER LIABILITY
 *     WHETHER IN AN ACTION OF CONTRACT, TORT OR OTHERWISE, ARISING
 *     FROM, OUT OF OR IN CONNECTION WITH THE SOFTWARE OR THE USE OR
 *     OTHER DEALINGS IN THE SOFTWARE.
 *
 * Contains definitions specific to the Armada XP SoC that are not
 * common to all Armada SoCs.
 */

#include "armada-370-xp.dtsi"

/ {
	model = "Marvell Armada XP family SoC";
	compatible = "marvell,armadaxp", "marvell,armada-370-xp";

	aliases {
		serial2 = &uart2;
		serial3 = &uart3;
	};

	soc {
		compatible = "marvell,armadaxp-mbus", "simple-bus";

		bootrom {
			compatible = "marvell,bootrom";
			reg = <MBUS_ID(0x01, 0x1d) 0 0x100000>;
		};

		internal-regs {
			sdramc@1400 {
				compatible = "marvell,armada-xp-sdram-controller";
				reg = <0x1400 0x500>;
			};

			L2: l2-cache {
				compatible = "marvell,aurora-system-cache";
				reg = <0x08000 0x1000>;
				cache-id-part = <0x100>;
				cache-level = <2>;
				cache-unified;
				wt-override;
			};

			spi0: spi@10600 {
				pinctrl-0 = <&spi0_pins>;
				pinctrl-names = "default";
			};

			i2c0: i2c@11000 {
				compatible = "marvell,mv78230-i2c", "marvell,mv64xxx-i2c";
				reg = <0x11000 0x100>;
			};

			i2c1: i2c@11100 {
				compatible = "marvell,mv78230-i2c", "marvell,mv64xxx-i2c";
				reg = <0x11100 0x100>;
			};

			uart2: serial@12200 {
				compatible = "snps,dw-apb-uart";
				pinctrl-0 = <&uart2_pins>;
				pinctrl-names = "default";
				reg = <0x12200 0x100>;
				reg-shift = <2>;
				interrupts = <43>;
				reg-io-width = <1>;
				clocks = <&coreclk 0>;
				status = "disabled";
			};

			uart3: serial@12300 {
				compatible = "snps,dw-apb-uart";
				pinctrl-0 = <&uart3_pins>;
				pinctrl-names = "default";
				reg = <0x12300 0x100>;
				reg-shift = <2>;
				interrupts = <44>;
				reg-io-width = <1>;
				clocks = <&coreclk 0>;
				status = "disabled";
			};

			system-controller@18200 {
				compatible = "marvell,armada-370-xp-system-controller";
				reg = <0x18200 0x500>;
			};

			gateclk: clock-gating-control@18220 {
				compatible = "marvell,armada-xp-gating-clock";
				reg = <0x18220 0x4>;
				clocks = <&coreclk 0>;
				#clock-cells = <1>;
			};

			coreclk: mvebu-sar@18230 {
				compatible = "marvell,armada-xp-core-clock";
				reg = <0x18230 0x08>;
				#clock-cells = <1>;
			};

			thermal@182b0 {
				compatible = "marvell,armadaxp-thermal";
				reg = <0x182b0 0x4
					0x184d0 0x4>;
				status = "okay";
			};

			cpuclk: clock-complex@18700 {
				#clock-cells = <1>;
				compatible = "marvell,armada-xp-cpu-clock";
				reg = <0x18700 0x24>, <0x1c054 0x10>;
				clocks = <&coreclk 1>;
			};

			interrupt-controller@20a00 {
			      reg = <0x20a00 0x2d0>, <0x21070 0x58>;
			};

			timer@20300 {
				compatible = "marvell,armada-xp-timer";
				clocks = <&coreclk 2>, <&refclk>;
				clock-names = "nbclk", "fixed";
			};

			watchdog@20300 {
				compatible = "marvell,armada-xp-wdt";
				clocks = <&coreclk 2>, <&refclk>;
				clock-names = "nbclk", "fixed";
			};

			cpurst@20800 {
				compatible = "marvell,armada-370-cpu-reset";
				reg = <0x20800 0x20>;
			};

			eth2: ethernet@30000 {
				compatible = "marvell,armada-370-neta";
				reg = <0x30000 0x4000>;
				interrupts = <12>;
				clocks = <&gateclk 2>;
				status = "disabled";
			};

			usb@50000 {
				clocks = <&gateclk 18>;
			};

			usb@51000 {
				clocks = <&gateclk 19>;
			};

			usb@52000 {
				compatible = "marvell,orion-ehci";
				reg = <0x52000 0x500>;
				interrupts = <47>;
				clocks = <&gateclk 20>;
				status = "disabled";
			};

			xor@60900 {
				compatible = "marvell,orion-xor";
				reg = <0x60900 0x100
				       0x60b00 0x100>;
				clocks = <&gateclk 22>;
				status = "okay";

				xor10 {
					interrupts = <51>;
					dmacap,memcpy;
					dmacap,xor;
				};
				xor11 {
					interrupts = <52>;
					dmacap,memcpy;
					dmacap,xor;
					dmacap,memset;
				};
			};

			xor@f0900 {
				compatible = "marvell,orion-xor";
				reg = <0xF0900 0x100
				       0xF0B00 0x100>;
				clocks = <&gateclk 28>;
				status = "okay";

				xor00 {
					interrupts = <94>;
					dmacap,memcpy;
					dmacap,xor;
				};
				xor01 {
					interrupts = <95>;
					dmacap,memcpy;
					dmacap,xor;
					dmacap,memset;
				};
			};
		};
	};

	clocks {
		/* 25 MHz reference crystal */
		refclk: oscillator {
			compatible = "fixed-clock";
			#clock-cells = <0>;
			clock-frequency = <25000000>;
		};
	};
};

&pinctrl {
	ge0_gmii_pins: ge0-gmii-pins {
		marvell,pins =
		     "mpp0",  "mpp1",  "mpp2",  "mpp3",
		     "mpp4",  "mpp5",  "mpp6",  "mpp7",
		     "mpp8",  "mpp9",  "mpp10", "mpp11",
		     "mpp12", "mpp13", "mpp14", "mpp15",
		     "mpp16", "mpp17", "mpp18", "mpp19",
		     "mpp20", "mpp21", "mpp22", "mpp23";
		marvell,function = "ge0";
	};

	ge0_rgmii_pins: ge0-rgmii-pins {
		marvell,pins =
		     "mpp0", "mpp1", "mpp2", "mpp3",
		     "mpp4", "mpp5", "mpp6", "mpp7",
		     "mpp8", "mpp9", "mpp10", "mpp11";
		marvell,function = "ge0";
	};

	ge1_rgmii_pins: ge1-rgmii-pins {
		marvell,pins =
		     "mpp12", "mpp13", "mpp14", "mpp15",
		     "mpp16", "mpp17", "mpp18", "mpp19",
		     "mpp20", "mpp21", "mpp22", "mpp23";
		marvell,function = "ge1";
	};

	sdio_pins: sdio-pins {
		marvell,pins = "mpp30", "mpp31", "mpp32",
			       "mpp33", "mpp34", "mpp35";
		marvell,function = "sd0";
	};

	spi0_pins: spi0-pins {
		marvell,pins = "mpp36", "mpp37",
			       "mpp38", "mpp39";
		marvell,function = "spi";
	};

	uart2_pins: uart2-pins {
		marvell,pins = "mpp42", "mpp43";
		marvell,function = "uart2";
	};

	uart3_pins: uart3-pins {
		marvell,pins = "mpp44", "mpp45";
		marvell,function = "uart3";
	};
};
