/*
 * Copyright (C) 2015 Jablotron s.r.o. -- http://www.jablotron.com/
 * Author: Rostislav Lisovy <lisovy@jablotron.cz>
 *
 * This program is free software; you can redistribute it and/or modify
 * it under the terms of the GNU General Public License version 2 as
 * published by the Free Software Foundation.
 */
/dts-v1/;
#include "am335x-chilisom.dtsi"

/ {
	model = "AM335x Chiliboard";
	compatible = "grinn,am335x-chiliboard", "grinn,am335x-chilisom",
		     "ti,am33xx";

	leds {
		compatible = "gpio-leds";
		pinctrl-names = "default";
		pinctrl-0 = <&led_gpio_pins>;

		led0 {
			label = "led0";
			gpios = <&gpio3 7 GPIO_ACTIVE_LOW>;
			default-state = "keep";
			linux,default-trigger = "heartbeat";
		};

		led1 {
			label = "led1";
			gpios = <&gpio3 8 GPIO_ACTIVE_LOW>;
			default-state = "keep";
		};
	};
};

&am33xx_pinmux {
	usb1_drvvbus: usb1_drvvbus {
		pinctrl-single,pins = <
			0x234 (PIN_OUTPUT_PULLDOWN | MUX_MODE0) /* usb1_drvvbus.usb1_drvvbus */
		>;
	};

	sd_pins: pinmux_sd_card {
		pinctrl-single,pins = <
			0xf0 (PIN_INPUT | MUX_MODE0) /* mmc0_dat0.mmc0_dat0 */
			0xf4 (PIN_INPUT | MUX_MODE0) /* mmc0_dat1.mmc0_dat1 */
			0xf8 (PIN_INPUT | MUX_MODE0) /* mmc0_dat2.mmc0_dat2 */
			0xfc (PIN_INPUT | MUX_MODE0) /* mmc0_dat3.mmc0_dat3 */
			0x100 (PIN_INPUT | MUX_MODE0) /* mmc0_clk.mmc0_clk */
			0x104 (PIN_INPUT | MUX_MODE0) /* mmc0_cmd.mmc0_cmd */
			0x160 (PIN_INPUT | MUX_MODE7) /* spi0_cs1.gpio0_6 */
		>;
	};

	led_gpio_pins: led_gpio_pins {
		pinctrl-single,pins = <
			0x1e4 (PIN_OUTPUT | MUX_MODE7) /* emu0.gpio3_7 */
			0x1e8 (PIN_OUTPUT | MUX_MODE7) /* emu1.gpio3_8 */
		>;
	};
};

&ldo4_reg {
	regulator-min-microvolt = <3300000>;
	regulator-max-microvolt = <3300000>;
};

/* Ethernet */
&cpsw_emac0 {
	phy_id = <&davinci_mdio>, <0>;
	phy-mode = "rmii";
};

&phy_sel {
	rmii-clock-ext;
};

/* USB */
&usb {
	status = "okay";
};

&usb_ctrl_mod {
	status = "okay";
};

&usb1_phy {
	status = "okay";
};

&usb1 {
	pinctrl-names = "default";
	pinctrl-0 = <&usb1_drvvbus>;

	status = "okay";
	dr_mode = "host";
};

&cppi41dma  {
	status = "okay";
};

/* microSD */
&mmc1 {
	pinctrl-names = "default";
	pinctrl-0 = <&sd_pins>;
	vmmc-supply = <&ldo4_reg>;
	bus-width = <0x4>;
	cd-gpios = <&gpio0 6 GPIO_ACTIVE_HIGH>;
	status = "okay";
};
