/*
 * SBC8349E Device Tree Source
 *
 * Copyright 2007 Wind River Inc.
 *
 * Paul Gortmaker (see MAINTAINERS for contact information)
 *
 *	-based largely on the Freescale MPC834x_MDS dts.
 *
 * This program is free software; you can redistribute  it and/or modify it
 * under  the terms of  the GNU General  Public License as published by the
 * Free Software Foundation;  either version 2 of the  License, or (at your
 * option) any later version.
 */

/dts-v1/;

/ {
	model = "SBC8349E";
	compatible = "SBC834xE";
	#address-cells = <1>;
	#size-cells = <1>;

	aliases {
		ethernet0 = &enet0;
		ethernet1 = &enet1;
		serial0 = &serial0;
		serial1 = &serial1;
		pci0 = &pci0;
	};

	cpus {
		#address-cells = <1>;
		#size-cells = <0>;

		PowerPC,8349@0 {
			device_type = "cpu";
			reg = <0x0>;
			d-cache-line-size = <32>;
			i-cache-line-size = <32>;
			d-cache-size = <32768>;
			i-cache-size = <32768>;
			timebase-frequency = <0>;	// from bootloader
			bus-frequency = <0>;		// from bootloader
			clock-frequency = <0>;		// from bootloader
		};
	};

	memory {
		device_type = "memory";
		reg = <0x00000000 0x10000000>;	// 256MB at 0
	};

	soc8349@e0000000 {
		#address-cells = <1>;
		#size-cells = <1>;
		device_type = "soc";
		ranges = <0x0 0xe0000000 0x00100000>;
		reg = <0xe0000000 0x00000200>;
		bus-frequency = <0>;

		wdt@200 {
			compatible = "mpc83xx_wdt";
			reg = <0x200 0x100>;
		};

		i2c@3000 {
			#address-cells = <1>;
			#size-cells = <0>;
			cell-index = <0>;
			compatible = "fsl-i2c";
			reg = <0x3000 0x100>;
			interrupts = <14 0x8>;
			interrupt-parent = <&ipic>;
			dfsrr;
		};

		i2c@3100 {
			#address-cells = <1>;
			#size-cells = <0>;
			cell-index = <1>;
			compatible = "fsl-i2c";
			reg = <0x3100 0x100>;
			interrupts = <15 0x8>;
			interrupt-parent = <&ipic>;
			dfsrr;
		};

		spi@7000 {
			cell-index = <0>;
			compatible = "fsl,spi";
			reg = <0x7000 0x1000>;
			interrupts = <16 0x8>;
			interrupt-parent = <&ipic>;
			mode = "cpu";
		};

		dma@82a8 {
			#address-cells = <1>;
			#size-cells = <1>;
			compatible = "fsl,mpc8349-dma", "fsl,elo-dma";
			reg = <0x82a8 4>;
			ranges = <0 0x8100 0x1a8>;
			interrupt-parent = <&ipic>;
			interrupts = <71 8>;
			cell-index = <0>;
			dma-channel@0 {
				compatible = "fsl,mpc8349-dma-channel", "fsl,elo-dma-channel";
				reg = <0 0x80>;
				cell-index = <0>;
				interrupt-parent = <&ipic>;
				interrupts = <71 8>;
			};
			dma-channel@80 {
				compatible = "fsl,mpc8349-dma-channel", "fsl,elo-dma-channel";
				reg = <0x80 0x80>;
				cell-index = <1>;
				interrupt-parent = <&ipic>;
				interrupts = <71 8>;
			};
			dma-channel@100 {
				compatible = "fsl,mpc8349-dma-channel", "fsl,elo-dma-channel";
				reg = <0x100 0x80>;
				cell-index = <2>;
				interrupt-parent = <&ipic>;
				interrupts = <71 8>;
			};
			dma-channel@180 {
				compatible = "fsl,mpc8349-dma-channel", "fsl,elo-dma-channel";
				reg = <0x180 0x28>;
				cell-index = <3>;
				interrupt-parent = <&ipic>;
				interrupts = <71 8>;
			};
		};

		/* phy type (ULPI or SERIAL) are only types supported for MPH */
		/* port = 0 or 1 */
		usb@22000 {
			compatible = "fsl-usb2-mph";
			reg = <0x22000 0x1000>;
			#address-cells = <1>;
			#size-cells = <0>;
			interrupt-parent = <&ipic>;
			interrupts = <39 0x8>;
			phy_type = "ulpi";
			port0;
		};

		enet0: ethernet@24000 {
			#address-cells = <1>;
			#size-cells = <1>;
			cell-index = <0>;
			device_type = "network";
			model = "TSEC";
			compatible = "gianfar";
			reg = <0x24000 0x1000>;
			ranges = <0x0 0x24000 0x1000>;
			local-mac-address = [ 00 00 00 00 00 00 ];
			interrupts = <32 0x8 33 0x8 34 0x8>;
			interrupt-parent = <&ipic>;
			tbi-handle = <&tbi0>;
			phy-handle = <&phy0>;
			linux,network-index = <0>;

			mdio@520 {
				#address-cells = <1>;
				#size-cells = <0>;
				compatible = "fsl,gianfar-mdio";
				reg = <0x520 0x20>;

				phy0: ethernet-phy@19 {
					interrupt-parent = <&ipic>;
					interrupts = <20 0x8>;
					reg = <0x19>;
				};

				phy1: ethernet-phy@1a {
					interrupt-parent = <&ipic>;
					interrupts = <21 0x8>;
					reg = <0x1a>;
				};

				tbi0: tbi-phy@11 {
					reg = <0x11>;
					device_type = "tbi-phy";
				};
			};
		};

		enet1: ethernet@25000 {
			#address-cells = <1>;
			#size-cells = <1>;
			cell-index = <1>;
			device_type = "network";
			model = "TSEC";
			compatible = "gianfar";
			reg = <0x25000 0x1000>;
			ranges = <0x0 0x25000 0x1000>;
			local-mac-address = [ 00 00 00 00 00 00 ];
			interrupts = <35 0x8 36 0x8 37 0x8>;
			interrupt-parent = <&ipic>;
			tbi-handle = <&tbi1>;
			phy-handle = <&phy1>;
			linux,network-index = <1>;

			mdio@520 {
				#address-cells = <1>;
				#size-cells = <0>;
				compatible = "fsl,gianfar-tbi";
				reg = <0x520 0x20>;

				tbi1: tbi-phy@11 {
					reg = <0x11>;
					device_type = "tbi-phy";
				};
			};
		};

		serial0: serial@4500 {
			cell-index = <0>;
			device_type = "serial";
			compatible = "fsl,ns16550", "ns16550";
			reg = <0x4500 0x100>;
			clock-frequency = <0>;
			interrupts = <9 0x8>;
			interrupt-parent = <&ipic>;
		};

		serial1: serial@4600 {
			cell-index = <1>;
			device_type = "serial";
			compatible = "fsl,ns16550", "ns16550";
			reg = <0x4600 0x100>;
			clock-frequency = <0>;
			interrupts = <10 0x8>;
			interrupt-parent = <&ipic>;
		};

		crypto@30000 {
			compatible = "fsl,sec2.0";
			reg = <0x30000 0x10000>;
			interrupts = <11 0x8>;
			interrupt-parent = <&ipic>;
			fsl,num-channels = <4>;
			fsl,channel-fifo-len = <24>;
			fsl,exec-units-mask = <0x7e>;
			fsl,descriptor-types-mask = <0x01010ebf>;
		};

		/* IPIC
		 * interrupts cell = <intr #, sense>
		 * sense values match linux IORESOURCE_IRQ_* defines:
		 * sense == 8: Level, low assertion
		 * sense == 2: Edge, high-to-low change
		 */
		ipic: pic@700 {
			interrupt-controller;
			#address-cells = <0>;
			#interrupt-cells = <2>;
			reg = <0x700 0x100>;
			device_type = "ipic";
		};
	};

	localbus@e0005000 {
		#address-cells = <2>;
		#size-cells = <1>;
		compatible = "fsl,mpc8349-localbus", "simple-bus";
		reg = <0xe0005000 0x1000>;
		interrupts = <77 0x8>;
		interrupt-parent = <&ipic>;
		ranges = <0x0 0x0 0xff800000 0x00800000		/* 8MB Flash */
			  0x1 0x0 0xf8000000 0x00002000		/* 8KB EEPROM */
			  0x2 0x0 0x10000000 0x04000000		/* 64MB SDRAM */
			  0x3 0x0 0x10000000 0x04000000>;	/* 64MB SDRAM */

		flash@0,0 {
			#address-cells = <1>;
			#size-cells = <1>;
			compatible = "intel,28F640J3A", "cfi-flash";
			reg = <0x0 0x0 0x800000>;
			bank-width = <2>;
			device-width = <1>;

			partition@0 {
				label = "u-boot";
				reg = <0x00000000 0x00040000>;
				read-only;
			};

			partition@40000 {
				label = "user";
				reg = <0x00040000 0x006c0000>;
			};

			partition@700000 {
				label = "legacy u-boot";
				reg = <0x00700000 0x00100000>;
				read-only;
			};

		};
	};

	pci0: pci@e0008500 {
		interrupt-map-mask = <0xf800 0x0 0x0 0x7>;
		interrupt-map = <

				/* IDSEL 0x11 */
				 0x8800 0x0 0x0 0x1 &ipic 48 0x8
				 0x8800 0x0 0x0 0x2 &ipic 17 0x8
				 0x8800 0x0 0x0 0x3 &ipic 18 0x8
				 0x8800 0x0 0x0 0x4 &ipic 19 0x8>;

		interrupt-parent = <&ipic>;
		interrupts = <0x42 0x8>;
		bus-range = <0 0>;
		ranges = <0x02000000 0x0 0x90000000 0x90000000 0x0 0x10000000
			  0x42000000 0x0 0x80000000 0x80000000 0x0 0x10000000
			  0x01000000 0x0 0x00000000 0xe2000000 0x0 0x00100000>;
		clock-frequency = <66666666>;
		#interrupt-cells = <1>;
		#size-cells = <2>;
		#address-cells = <3>;
		reg = <0xe0008500 0x100		/* internal registers */
		       0xe0008300 0x8>;		/* config space access registers */
		compatible = "fsl,mpc8349-pci";
		device_type = "pci";
	};
};
