Upstream-Status: Pending
diff --git a/include/linux/if_pppol2tp.h b/include/linux/if_pppol2tp.h
index 4113d6a..7ee86b2 100644
--- a/include/linux/if_pppol2tp.h
+++ b/include/linux/if_pppol2tp.h
@@ -2,7 +2,7 @@
  * Linux PPP over L2TP (PPPoL2TP) Socket Implementation (RFC 2661)
  *
  * This file supplies definitions required by the PPP over L2TP driver
- * (pppol2tp.c).  All version information wrt this file is located in pppol2tp.c
+ * (l2tp_ppp.c).  All version information wrt this file is located in l2tp_ppp.c
  *
  * License:
  *		This program is free software; you can redistribute it and/or
@@ -15,14 +15,14 @@
 #ifndef __LINUX_IF_PPPOL2TP_H
 #define __LINUX_IF_PPPOL2TP_H
 
-#include <asm/types.h>
+#include <linux/types.h>
+
 
 /* Structure used to connect() the socket to a particular tunnel UDP
  * socket.
  */
-struct pppol2tp_addr
-{
-	pid_t	pid;			/* pid that owns the fd.
+struct pppol2tp_addr {
+	__kernel_pid_t	pid;		/* pid that owns the fd.
 					 * 0 => current */
 	int	fd;			/* FD of UDP socket to use */
 
@@ -32,6 +32,20 @@ struct pppol2tp_addr
 	__u16 d_tunnel, d_session;	/* For sending outgoing packets */
 };
 
+/* The L2TPv3 protocol changes tunnel and session ids from 16 to 32
+ * bits. So we need a different sockaddr structure.
+ */
+struct pppol2tpv3_addr {
+	pid_t	pid;			/* pid that owns the fd.
+					 * 0 => current */
+	int	fd;			/* FD of UDP or IP socket to use */
+
+	struct sockaddr_in addr;	/* IP address and port to send to */
+
+	__u32 s_tunnel, s_session;	/* For matching incoming packets */
+	__u32 d_tunnel, d_session;	/* For sending outgoing packets */
+};
+
 /* Socket options:
  * DEBUG	- bitmask of debug message categories
  * SENDSEQ	- 0 => don't send packets with sequence numbers
