From 08181bee8ee375225129d086656c567022becf41 Mon Sep 17 00:00:00 2001
From: Jonas Gorski <jogo@openwrt.org>
Date: Fri, 28 Jun 2013 00:08:16 +0200
Subject: [PATCH V2 09/13] MIPS: BCM63XX: always register bmips smp ops

Use the return value for guarding further SMP setup.

Signed-off-by: Jonas Gorski <jogo@openwrt.org>
---
 arch/mips/bcm63xx/prom.c | 6 ++----
 1 file changed, 2 insertions(+), 4 deletions(-)

--- a/arch/mips/bcm63xx/prom.c
+++ b/arch/mips/bcm63xx/prom.c
@@ -59,10 +59,8 @@ void __init prom_init(void)
 	/* do low level board init */
 	board_prom_init();
 
-	if (IS_ENABLED(CONFIG_CPU_BMIPS4350) && IS_ENABLED(CONFIG_SMP)) {
-		/* set up SMP */
-		register_bmips_smp_ops();
-
+	/* set up SMP */
+	if (!register_bmips_smp_ops()) {
 		/*
 		 * BCM6328 might not have its second CPU enabled, while BCM3368
 		 * and BCM6358 need special handling for their shared TLB, so
