From 69c15bfd4b9b78ab8f0dd9a2c0902bcc5d4f02e4 Mon Sep 17 00:00:00 2001
From: Jonas Gorski <jogo@openwrt.org>
Date: Sun, 1 Dec 2013 13:07:35 +0100
Subject: [PATCH] spi/bcm63xx-hsspi: make it compile with 3.10

---
 drivers/spi/spi-bcm63xx-hsspi.c | 3 +--
 1 file changed, 1 insertion(+), 2 deletions(-)

--- a/drivers/spi/spi-bcm63xx-hsspi.c
+++ b/drivers/spi/spi-bcm63xx-hsspi.c
@@ -375,8 +375,7 @@ static int bcm63xx_hsspi_probe(struct pl
 	master->setup = bcm63xx_hsspi_setup;
 	master->transfer_one_message = bcm63xx_hsspi_transfer_one;
 	master->mode_bits = SPI_CPOL | SPI_CPHA | SPI_CS_HIGH;
-	master->bits_per_word_mask = SPI_BPW_MASK(8);
-	master->auto_runtime_pm = true;
+	master->bits_per_word_mask = BIT(8 - 1);
 
 	platform_set_drvdata(pdev, master);
 
