From a2da7b7a2cb8319b6383e93d99905cb027252584 Mon Sep 17 00:00:00 2001
From: Hauke Mehrtens <hauke@hauke-m.de>
Date: Fri, 3 Jan 2014 20:41:59 +0100
Subject: [PATCH] MIPS: BCM47XX: add board detection for Linksys WRT54GS V1

This adds board detection for Linksys WRT54GS V1.

Signed-off-by: Hauke Mehrtens <hauke@hauke-m.de>
Acked-by: Rafa? Mi?ecki <zajec5@gmail.com>
---
 arch/mips/bcm47xx/board.c                          |    1 +
 arch/mips/include/asm/mach-bcm47xx/bcm47xx_board.h |    1 +
 2 files changed, 2 insertions(+)

--- a/arch/mips/bcm47xx/board.c
+++ b/arch/mips/bcm47xx/board.c
@@ -175,6 +175,7 @@ struct bcm47xx_board_type_list3 bcm47xx_
 	{{BCM47XX_BOARD_PHICOMM_M1, "Phicomm M1"}, "0x0590", "80", "0x1104"},
 	{{BCM47XX_BOARD_ZTE_H218N, "ZTE H218N"}, "0x053d", "1234", "0x1305"},
 	{{BCM47XX_BOARD_NETGEAR_WNR3500L, "Netgear WNR3500L"}, "0x04CF", "3500", "02"},
+	{{BCM47XX_BOARD_LINKSYS_WRT54GSV1, "Linksys WRT54GS V1"}, "0x0101", "42", "0x10"},
 	{ {0}, 0},
 };
 
--- a/arch/mips/include/asm/mach-bcm47xx/bcm47xx_board.h
+++ b/arch/mips/include/asm/mach-bcm47xx/bcm47xx_board.h
@@ -66,6 +66,7 @@ enum bcm47xx_board {
 	BCM47XX_BOARD_LINKSYS_WRT310NV1,
 	BCM47XX_BOARD_LINKSYS_WRT310NV2,
 	BCM47XX_BOARD_LINKSYS_WRT54G3GV2,
+	BCM47XX_BOARD_LINKSYS_WRT54GSV1,
 	BCM47XX_BOARD_LINKSYS_WRT610NV1,
 	BCM47XX_BOARD_LINKSYS_WRT610NV2,
 	BCM47XX_BOARD_LINKSYS_WRTSL54GS,
